CSEM March 2025 Deployment Transect Plans
[image: ]Transect 1 (9.5 nautical miles):
N/E Latitude: 36.962084°
N/E Longitude-121.937092°
S/W Latitude: 36.804267°
S/W Longitude: -121.962061°

Transect 2 (12.7 nautical miles):
N/E Latitude: 36.961052°
N/E Longitude: -121.929009°
S/W Latitude: 36.827343°
S/W Longitude: -122.133825°
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Gains of dataloggers = 000110, 36
Ch 0 = 0
Ch 1 = 1
Ch 2 = 2
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Profile Average Frequency Source | Acquisition Speed
Bathymetry (m) (Hz) (kn)
Profile 1 18m 5Hz 3.5kn
Profile 2 40m 0.5 Hz 2kn
Profile 3 110m 0.5 Hz 1.5kn
Profile 4 15m 5Hz 3.5kn
Profile 5 45m 1Hz for first part 2.5kn
and 0.5 Hz for the
second one
Priority Line 1 100 m 0.5 Hz 1.5kn
Priority Line 2 80m 0.5Hz 2kn





