Target Position: 36 47.724	121 49.153
Bring:
1) Apex float
2) Spool of spectra
3) 20 meter spectra tail line
4) 2 floats
5) Extra swivels and snaps
6) 2x 10 lb weights
7) Bag of tools
8) Iridium phone box w/GPS and antennas
9) Laptop
10)  Extra line
11) Cable ties and duct tape
12) Cell phone(s)
13) Food and drink
Before leaving the dock
1) Setup computer and sat phone
2) Check sat phone connection to MBARI network
3) Check ArcGIS program
4) Check Google Earth program
5) Check float status
6) Rig line loops on floats
Deployment plan
1) Deploy weight, down line and top float
2) Recover 5 meters checking for expected pull up force, redeploy
3) Watch for awhile
4) Start the mission, confirm.
5) Remove the top float, string the float, add the float and tail line/tail float

