LRAUV Argos relocation transmitter information:
1. [bookmark: _GoBack]Administer transmitters here: https://argos-system.clsamerica.com
a. Login with username: stedshob1 password: quinto
i. This account also has Benthic Rover transmitters
ii. LRAUV program is 9228
b. Go to Data Access
i. Go to Most Recent Messages to see latest message from each tag.  Scroll to right (with slider bar on the bottom) to see the date and time of last message, which may be more recent than latest location date.
ii. Go to Messages to see messages from the last 20 days (max number held in the system)
iii. Go to Mapping, to see recent fixes on a map
c. Transmitter (Platform) IDs
i. Tethys 136621
ii. Daphne 136622
iii. Makai 136623
d. Satellite Pass Prediction page will allow you to know exactly when an argos receiver equipped satellite will be overhead.  Typically satellites are in view for ~10 min every couple of hours
