{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["CPF003.004","Copy of all data","Ascend Science Samples","Single Ascend Science Sample"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CPF003.004","index":0,"n_rows":32198,"n_cols":52,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["$","Date","Time","State","Comment","Pressure","BelPos","PumpVolts","PumpMilliamps","PumpoCoulombs","PumpJoules","PumpMotor","HotelVolts","HotelMilliamps","HotelCoulombs","HotelJoules","CTDTemp","CTDSal","RawPress","LPFPress","LPFVel","DiffVel","Diff2 Vel","SlopeLPFPress.","CTDSamplePeriod","LPS331Press","LPS331Temp","SHT21Humid","SHT21Temp","pidSP","pidPV","pidY1","pidY2","pidI","pid_v","pid_u","pid_uCPS","pid_h","FLBB","Topt","Tphase","Rphase","NO3","pHVrs","OCRtext","OCRCh1","OCRCh2","OCRCh3","OCRCH4","GPS","IridModem","MSC"]
["$","2022-02-24","00:45:43","Surface Ops","Opened new engr log file: \\SD\\data\\2022-2-23T16-59-6\\CPF003.004.eng"]
["$","2022-02-24","00:45:43.100","Surface Ops","Opening new .dura file: \\SD\\data\\2022-2-23T16-59-6\\CPF003.004.dura"]
["$","2022-02-24","00:45:43.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:43.600","Surface Ops","Opening new .isus file: \\SD\\data\\2022-2-23T16-59-6\\CPF003.004.isus"]
["$","2022-02-24","00:45:43.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:43.700","Surface Ops","Skipping over SendFilesViaRudics"]
["$","2022-02-24","00:45:43.700","Surface Ops","2022-02-24T00:45:43Z,,Lat,3652.79313","N,,Lon,12156.36559","W,GPS TOF,004542.00,Num Sats,5,Surface Ops,Console set SV.ForceRecoveryState false,ProfileNum,3,NAK SBD,SQ,5,MO Stat,-,,Mission TO,02:00:00,Park Time,02:00:00,Park P,85,Prof Num,3 of 20,Max P,-100.000,BBVolts,32.375,Can P,1218.1,Can Hum,38.8,BBHealth,0FFF"]
["$","2022-02-24","00:45:43.700","Surface Ops","IModem Sending SBDWT cmd"]
["$","2022-02-24","00:45:43.700","Surface Ops","Sent SBDWT Command"]
["$","2022-02-24","00:45:43.800","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","00:45:43.800","Surface Ops","IModem invalid response: IModem Looking for IModem-->READY<--  IModem Got-->  <--  "]
["$","2022-02-24","00:45:43.800","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"READY  "]
["$","2022-02-24","00:45:43.800","Surface Ops","IModem correct response: IModem Looking for IModem-->READY<--  IModem Got-->READY  <--  "]
["$","2022-02-24","00:45:43.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:45:43.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","00:45:43.900","Surface Ops","IModem Sending loadSBDWT cmd"]
["$","2022-02-24","00:45:44.100","Surface Ops","IModem Loaded SBDWT Buffer with->2022-02-24T00:45:43Z,,Lat,3652.79313","N,,Lon,12156.36559","W,GPS TOF,004542.00,Num Sats,5,Surface Ops,Console set SV.ForceRecoveryState false,ProfileNum,3,NAK SBD,SQ,5,MO Stat,-,,Mission TO,02:00:00,Park Time,02:00:00,Park P,85,Prof Num,3 of 20,Max P,-100.000,BBVolts,32.375,Can P,1218.1,Can Hum,38.8,BBHealth,0FFF<-"]
["$","2022-02-24","00:45:44.300","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","00:45:44.300","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->  <--  "]
["$","2022-02-24","00:45:44.300","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","00:45:44.400","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->0  <--  "]
["$","2022-02-24","00:45:44.300","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","00:45:44.400","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->  <--  "]
["$","2022-02-24","00:45:44.300","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OK  "]
["$","2022-02-24","00:45:44.400","Surface Ops","IModem correct response: IModem Looking for IModem-->OK<--  IModem Got-->OK  <--  "]
["$","2022-02-24","00:45:44.400","Surface Ops","IModem Sending SBDIX cmd"]
["$","2022-02-24","00:45:44.500","Surface Ops","IModem Sent SBDIX Command"]
["$","2022-02-24","00:45:44.700","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:45.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:45:45.200","Surface Ops","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:45:45.700","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:46.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:46.700","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:46.700","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:45:47","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.06]
["$","2022-02-24","00:45:47","Surface Ops","SBE41 Message",0.06,44.822620999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.06,0.06,-0.128243,-3.7529999999999998E-3,-8.6666999999999994E-2,-1.3332999999999999E-2,-1.95E-4,3000]
["$","2022-02-24","00:45:47.700","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:47.700","Surface Ops","System Data (dBar %full Volts mAmps): ",0.06,44.833466999999999,0.2,0,614.53313200000002,70487.231639999998,null,32.375,146,1443.958674,7048.5754209999996,null,null,null,null,null,null,null,null,null,1218.099976,12.48,37.881999999999998,12.48]
["$","2022-02-24","00:45:47.800","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","00:45:49.200","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","00:45:49.200","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","00:45:49.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:49.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:49.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:45:49.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:45:50.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.24]
["$","2022-02-24","00:45:50.200","Surface Ops","SBE41 Message",-0.24,44.83381,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.24,-0.24,-0.13390099999999999,-4.4710000000000001E-3,0.1,6.6670000000000002E-3,-1.6200000000000001E-4,3000]
["$","2022-02-24","00:45:50.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:51.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:52","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:45:52","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:45:52.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:52.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:52.700","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:45:53.100","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.16]
["$","2022-02-24","00:45:53.100","Surface Ops","SBE41 Message",-0.16,44.822532000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.16,-0.16,-0.124348,-2.8059999999999999E-3,-2.6667E-2,3.6666999999999998E-2,-1.4300000000000001E-4,3000]
["$","2022-02-24","00:45:53.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:54.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:55.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:55.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:55.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:45:55.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:45:56.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:45:56.200","Surface Ops","SBE41 Message",-0.09,44.830872999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.10817400000000001,-4.1599999999999997E-4,-2.3333E-2,-2.5000000000000001E-2,-1.6000000000000001E-4,3000]
["$","2022-02-24","00:45:56.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:57.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:57.500","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","00:45:57.600","Surface Ops","IModem got invalid SBDIX response:   "]
["$","2022-02-24","00:45:57.600","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+SBDIX: 0, 0, 0, 0, 0, 0  "]
["$","2022-02-24","00:45:57.600","Surface Ops","IModem SBDIX Response: +SBDIX: 0, 0, 0, 0, 0, 0     sbdixMOStatus = 0   sbdixMTStatus = 0   sbdixMTQueued = 0"]
["$","2022-02-24","00:45:57.600","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","00:45:57.600","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OK  "]
["$","2022-02-24","00:45:57.700","Surface Ops","IModem SBDIX try num: 1"]
["$","2022-02-24","00:45:58.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:58.700","Surface Ops","Sending Elmo Echo Off command"]
["$","2022-02-24","00:46:00.700","Surface Ops","Setting Elmo current and acc limits"]
["$","2022-02-24","00:46:00.700","Surface Ops","Setting Elmo Acceleration limit = AC[1]=1e9;"]
["$","2022-02-24","00:46:00.700","Surface Ops","Setting Elmo Deacceleration limit = DC=1e9;"]
["$","2022-02-24","00:46:00.700","Surface Ops","Sending Elmo CL[1]=4.76 command"]
["$","2022-02-24","00:46:01.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:46:01.700","Surface Ops","Sending Elmo PL1[1]=13.5 command"]
["$","2022-02-24","00:46:02.700","Surface Ops","Sending Elmo PL2[1]=2 command"]
["$","2022-02-24","00:46:04.100","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:04.100","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:04.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:46:06.600","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:06.600","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:06.600","Surface Ops","Normal State Exit"]
["$","2022-02-24","00:46:06.600","Init Profile","Setting Execution Constraint = 600000"]
["$","2022-02-24","00:46:06.600","Init Profile","State Entry"]
["$","2022-02-24","00:45:58","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:45:58","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:45:58.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:45:59","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:45:59","Init Profile","SBE41 Message",-0.12,44.83719,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-9.9048999999999998E-2,5.6599999999999999E-4,0.01,-6.6670000000000002E-3,-2.12E-4,3000]
["$","2022-02-24","00:46:01","Init Profile","Twitter msg"]
["$","2022-02-24","00:46:01","Init Profile","Twitter msg",null,null,null,null,null,null,"\u0002?;"]
["$","2022-02-24","00:46:01","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1]=4.76;"]
["$","2022-02-24","00:46:01","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:01.700","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1]=13.5;"]
["$","2022-02-24","00:46:01.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:01.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:01.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:02.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:46:02.200","Init Profile","SBE41 Message",-0.12,44.83719,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.107136,-5.6499999999999996E-4,0,5.0000000000000001E-3,-2.7700000000000001E-4,3000]
["$","2022-02-24","00:46:02.700","Init Profile","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:02.700","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:02.900","Init Profile","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:02.900","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:03.100","Init Profile","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:03.100","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:03.300","Init Profile","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:03.300","Init Profile","Twitter msg",null,null,null,null,null,null,"33603584;"]
["$","2022-02-24","00:46:03.500","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:03.500","Init Profile","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:03.700","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:03.700","Init Profile","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:03.900","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:03.900","Init Profile","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:04.200","Init Profile","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:04.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:04.200","Init Profile","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:04.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:04.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:04.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:05.200","Init Profile","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:05.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.18]
["$","2022-02-24","00:46:05.200","Init Profile","SBE41 Message",-0.18,44.83719,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.18,-0.18,-0.12615899999999999,-2.16E-3,0.02,0.01,-3.2499999999999999E-4,3000]
["$","2022-02-24","00:46:05.200","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:05.400","Init Profile","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:05.400","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:05.600","Init Profile","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:05.600","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:05.800","Init Profile","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:05.800","Init Profile","Twitter msg",null,null,null,null,null,null,"33603584;"]
["$","2022-02-24","00:46:06","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:06","Init Profile","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:06.200","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:06.200","Init Profile","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:06.400","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:06.400","Init Profile","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:07.700","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:07.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:07.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:08.100","Init Profile","Initializing SBE 41 LPF"]
["$","2022-02-24","00:46:08.100","Init Profile","[MSC] Powering up MSC"]
["$","2022-02-24","00:46:08.100","Init Profile","[MSC] Resetting Sequencers"]
["$","2022-02-24","00:46:08.100","Init Profile","Sending SBE41 stopProfile"]
["$","2022-02-24","00:46:09.100","Init Profile","Power cycling SBE41"]
["$","2022-02-24","00:46:09.100","Init Profile","Power Cycling SBE41"]
["$","2022-02-24","00:46:09.100","Init Profile","Powering Down CTD"]
["$","2022-02-24","00:46:10.200","Init Profile","Powering Up CTD"]
["$","2022-02-24","00:46:10.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:11.200","Init Profile","Profile number = 4"]
["$","2022-02-24","00:46:11.200","Init Profile","Writing Header to msg File"]
["$","2022-02-24","00:46:11.600","Init Profile","[MSC] Starting config data collection."]
["$","2022-02-24","00:46:08.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>stopprofile  "]
["$","2022-02-24","00:46:09.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:10.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:11","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.19]
["$","2022-02-24","00:46:11","Init Profile","SBE41 Message",-0.19,44.83719,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.19,-0.19,-0.18,0,3.333E-3,1.6670000000000001E-3,0,3000]
["$","2022-02-24","00:46:11.700","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:11.700","Init Profile","System Data (dBar %full Volts mAmps): ",-0.19,44.826158999999997,32.375,10,2.4920999999999999E-2,29.951415999999998,null,32.375,175.5,0.62866599999999995,2.9817100000000001,null,null,null,null,null,null,null,null,null,1218.0500489999999,12.49,38.180999999999997,12.49]
["$","2022-02-24","00:46:11.800","Init Profile","Pump motor not faulted"]
["$","2022-02-24","00:46:13.200","Init Profile","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:13.200","Init Profile","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:13.300","Init Profile","[MSC] TX: W"]
["$","2022-02-24","00:46:11.800","Init Profile","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:11.800","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:12","Init Profile","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:12","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:12.200","Init Profile","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:12.200","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:12.400","Init Profile","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:12.400","Init Profile","Twitter msg",null,null,null,null,null,null,"33604352;"]
["$","2022-02-24","00:46:12.600","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:12.600","Init Profile","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:12.800","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:12.800","Init Profile","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:12.900","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:12.900","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:13","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:13","Init Profile","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:13.200","Init Profile","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:13.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:13.200","Init Profile","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:13.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:13.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:13.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:13.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:14.100","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.18]
["$","2022-02-24","00:46:14.100","Init Profile","SBE41 Message",-0.18,44.829211000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.18,-0.18,-0.18002099999999999,0,-3.333E-3,0,0,3000]
["$","2022-02-24","00:46:14.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:15.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:16.200","Init Profile","[MSC] Timeout for CommandWake"]
["$","2022-02-24","00:46:16.300","Init Profile","[MSC] TX: W"]
["$","2022-02-24","00:46:16.400","Init Profile","[MSC] RX: "]
["$","2022-02-24","00:46:16.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:16.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:16.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:16.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:17.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:46:17.200","Init Profile","SBE41 Message",-0.14000000000000001,44.835759000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.18024000000000001,-1.9999999999999999E-6,-1.3332999999999999E-2,-8.3330000000000001E-3,0,3000]
["$","2022-02-24","00:46:17.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:18.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:19","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:19","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:19.300","Init Profile","[MSC] Timeout for CommandWake"]
["$","2022-02-24","00:46:19.300","Init Profile","[MSC] TX: W"]
["$","2022-02-24","00:46:19.400","Init Profile","[MSC] RX: ACK  "]
["$","2022-02-24","00:46:19.500","Init Profile","[MSC] TX: RTC,1645663579"]
["$","2022-02-24","00:46:19.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:19.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:19.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:19.800","Init Profile","[MSC] RX: ACK,RTC,1645663579,1645663579  "]
["$","2022-02-24","00:46:19.800","Init Profile","[MSC] TX: ACK "]
["$","2022-02-24","00:46:19.800","Init Profile","[MSC] TX: MODE,1"]
["$","2022-02-24","00:46:20.100","Init Profile","[MSC] RX: ACK,MODE,1  "]
["$","2022-02-24","00:46:20.100","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:46:20.100","Init Profile","SBE41 Message",-0.12,44.832031999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.18093600000000001,-9.9999999999999995E-7,-6.6670000000000002E-3,-0.01,9.9999999999999995E-7,3000]
["$","2022-02-24","00:46:20.100","Init Profile","[MSC] TX: ACK "]
["$","2022-02-24","00:46:20.200","Init Profile","[MSC] TX: C"]
["$","2022-02-24","00:46:20.400","Init Profile","[MSC] RX: H, Datalogger Serial Num , SN:0003  "]
["$","2022-02-24","00:46:20.500","Init Profile","[MSC] RX: H, Application      Name , CPF_MAIN.C  "]
["$","2022-02-24","00:46:20.500","Init Profile","[MSC] RX: H, App Build        Date , Nov 20 2020, 13:19:41  "]
["$","2022-02-24","00:46:20.600","Init Profile","[MSC] RX: H, Power Up Time   (GMT) , 02/23/2022 22:32:51  "]
["$","2022-02-24","00:46:20.600","Init Profile","[MSC] RX: H, Current  Time   (GMT) , 02/24/2022 00:46:19  "]
["$","2022-02-24","00:46:20.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:20.700","Init Profile","[MSC] RX: H, Alarm    Time   (GMT) , 02/24/2022 08:32:56  "]
["$","2022-02-24","00:46:20.700","Init Profile","[MSC] RX: H, Power Active  Timeout , 10  "]
["$","2022-02-24","00:46:20.800","Init Profile","[MSC] RX: H, Persistor CF2-1M Info , S/N:15079 - BIOS:4.03 - PicoDOS:4.03  "]
["$","2022-02-24","00:46:20.800","Init Profile","[MSC] RX: H, Compact FLASH    Size , 256614400  "]
["$","2022-02-24","00:46:20.800","Init Profile","[MSC] RX: H, Compact FLASH    Left , 90.94%  "]
["$","2022-02-24","00:46:20.900","Init Profile","[MSC] RX: H, Power Cycle   Counter , 5  "]
["$","2022-02-24","00:46:20.900","Init Profile","[MSC] RX: H, System Reset  Counter , 5  "]
["$","2022-02-24","00:46:20.900","Init Profile","[MSC] RX: H, System Error  Counter , 0  "]
["$","2022-02-24","00:46:21","Init Profile","[MSC] RX: H, Last System     Error , 0  "]
["$","2022-02-24","00:46:21","Init Profile","[MSC] RX: H, Last System ErrorTime , 01/01/1970 00:00:00  "]
["$","2022-02-24","00:46:21.100","Init Profile","[MSC] RX: H, ISUS  Error   Counter , 0  "]
["$","2022-02-24","00:46:21.100","Init Profile","[MSC] RX: H, Last ISUS       Error , 0  "]
["$","2022-02-24","00:46:21.100","Init Profile","[MSC] RX: H, Last ISUS Error  Time , 01/01/1970 00:00:00  "]
["$","2022-02-24","00:46:21.200","Init Profile","[MSC] RX: H, ISUS Sample   Counter , 46  "]
["$","2022-02-24","00:46:21.200","Init Profile","[MSC] RX: H, Last Sample Rec. Time , 02/24/2022 00:40:20  "]
["$","2022-02-24","00:46:21.300","Init Profile","[MSC] RX: H, Fiberlite    Odometer , 05:23:43  "]
["$","2022-02-24","00:46:21.300","Init Profile","[MSC] RX: H, Fiberlite      Cycles , 7410  "]
["$","2022-02-24","00:46:21.300","Init Profile","[MSC] RX: H, Spec Intensity LampON , 5000  "]
["$","2022-02-24","00:46:21.400","Init Profile","[MSC] RX: H, Spec Integration Time , 375  "]
["$","2022-02-24","00:46:21.400","Init Profile","[MSC] RX: H, Spec Pre  scans taken , 2  "]
["$","2022-02-24","00:46:21.400","Init Profile","[MSC] RX: H, Spec Lite scans taken , 3  "]
["$","2022-02-24","00:46:21.500","Init Profile","[MSC] RX: H, Spec Dark scans taken , 1  "]
["$","2022-02-24","00:46:21.500","Init Profile","[MSC] RX: H, Calibration      Date , 11/24/2020  "]
["$","2022-02-24","00:46:21.500","Init Profile","[MSC] RX: H, Sw Calibration   Temp , 19.94  "]
["$","2022-02-24","00:46:21.600","Init Profile","[MSC] RX: H, Wavelength Fit  Range , 217.295 <-> 239.828  "]
["$","2022-02-24","00:46:21.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:21.600","Init Profile","[MSC] RX: H, Pixel Fit       Range , 36 <-> 64  "]
["$","2022-02-24","00:46:21.700","Init Profile","[MSC] RX: H, Fitted Concentrations , 2  "]
["$","2022-02-24","00:46:21.700","Init Profile","[MSC] RX: H, Baseline        Model , (ax + b)  "]
["$","2022-02-24","00:46:21.700","Init Profile","[MSC] RX: H, Br Temp  Compensation , ENABLED  "]
["$","2022-02-24","00:46:21.800","Init Profile","[MSC] RX: H, Bromide Term in Model , will be FIXED (to external CTD value)  "]
["$","2022-02-24","00:46:21.900","Init Profile","[MSC] RX: H, Zeiss Coefficient Vals, 1.885090e+02,7.959960e-01,1.113850e-04,-3.090260e-07,0.000000e+00  "]
["$","2022-02-24","00:46:22.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:22.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:22.600","Init Profile","System Data (dBar %full Volts mAmps): ",-0.12,44.820202999999999,32.375,10,0.13247500000000001,119.53704,null,32.375,184.5,2.6298249999999999,11.940272999999999,null,null,null,null,null,null,null,null,null,1218.130005,12.5,38.203999000000003,12.5]
["$","2022-02-24","00:46:22.700","Init Profile","Pump motor not faulted"]
["$","2022-02-24","00:46:24.100","Init Profile","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:24.100","Init Profile","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:22.700","Init Profile","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:22.700","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:22.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:22.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:22.900","Init Profile","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:22.900","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:23.100","Init Profile","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:23.100","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:23.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","00:46:23.200","Init Profile","SBE41 Message",-0.1,44.820202999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.181171,3.3000000000000003E-5,-6.6670000000000002E-3,-6.6670000000000002E-3,3.0000000000000001E-6,3000]
["$","2022-02-24","00:46:23.300","Init Profile","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:23.300","Init Profile","Twitter msg",null,null,null,null,null,null,"33604352;"]
["$","2022-02-24","00:46:23.500","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:23.500","Init Profile","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:23.700","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:23.700","Init Profile","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:23.900","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:23.900","Init Profile","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:24.200","Init Profile","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:24.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:24.200","Init Profile","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:24.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:24.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:25.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:25.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:25.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:25.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:26.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.19]
["$","2022-02-24","00:46:26.200","Init Profile","SBE41 Message",-0.19,44.831905999999996,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.19,-0.19,-0.17721999999999999,1.21E-4,0.03,1.1667E-2,-9.9999999999999995E-7,3000]
["$","2022-02-24","00:46:26.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:27.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:28","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:28","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:28.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:28.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:28.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:29","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:46:29","Init Profile","SBE41 Message",-0.09,44.827361000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.16519300000000001,1.2899999999999999E-4,-3.3333000000000002E-2,-1.6670000000000001E-3,-1.9000000000000001E-5,3000]
["$","2022-02-24","00:46:29.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:30.400","Init Profile","[MSC] TX: SE,?"]
["$","2022-02-24","00:46:30.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:30.600","Init Profile","[MSC] RX: ACK,SE?,0  "]
["$","2022-02-24","00:46:30.700","Init Profile","[MSC] ERRORS AVAILABLE: 0"]
["$","2022-02-24","00:46:30.700","Init Profile","[MSC] TX: W"]
["$","2022-02-24","00:46:30.800","Init Profile","[MSC] RX: ACK  "]
["$","2022-02-24","00:46:30.900","Init Profile","[MSC] TX: MODE,2"]
["$","2022-02-24","00:46:31.100","Init Profile","[MSC] RX: ACK,MODE,2  "]
["$","2022-02-24","00:46:31.200","Init Profile","[MSC] TX: ACK "]
["$","2022-02-24","00:46:31.200","Init Profile","[MSC] TX: C"]
["$","2022-02-24","00:46:31.400","Init Profile","[MSC] RX: H, Datalogger Serial Num , SN:0003  "]
["$","2022-02-24","00:46:31.500","Init Profile","[MSC] RX: H, Application      Name , CPF_MAIN.C  "]
["$","2022-02-24","00:46:31.500","Init Profile","[MSC] RX: H, App Build        Date , Nov 20 2020, 13:19:41  "]
["$","2022-02-24","00:46:31.600","Init Profile","[MSC] RX: H, Power Up Time   (GMT) , 02/23/2022 22:32:51  "]
["$","2022-02-24","00:46:31.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:31.600","Init Profile","[MSC] RX: H, Current  Time   (GMT) , 02/24/2022 00:46:30  "]
["$","2022-02-24","00:46:31.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:31.700","Init Profile","[MSC] RX: H, Alarm    Time   (GMT) , 02/24/2022 08:32:56  "]
["$","2022-02-24","00:46:31.700","Init Profile","[MSC] RX: H, Power Active  Timeout , 10  "]
["$","2022-02-24","00:46:31.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:31.800","Init Profile","[MSC] RX: H, Persistor CF2-1M Info , S/N:15079 - BIOS:4.03 - PicoDOS:4.03  "]
["$","2022-02-24","00:46:31.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:31.800","Init Profile","[MSC] RX: H, Compact FLASH    Size , 256614400  "]
["$","2022-02-24","00:46:31.900","Init Profile","[MSC] RX: H, Compact FLASH    Left , 90.94%  "]
["$","2022-02-24","00:46:31.900","Init Profile","[MSC] RX: H, Power Cycle   Counter , 5  "]
["$","2022-02-24","00:46:31.900","Init Profile","[MSC] RX: H, System Reset  Counter , 5  "]
["$","2022-02-24","00:46:32","Init Profile","[MSC] RX: H, System Error  Counter , 0  "]
["$","2022-02-24","00:46:32","Init Profile","[MSC] RX: H, Last System     Error , 0  "]
["$","2022-02-24","00:46:32","Init Profile","[MSC] RX: H, Last System ErrorTime , 01/01/1970 00:00:00  "]
["$","2022-02-24","00:46:32.100","Init Profile","[MSC] RX: H, DURA  Error   Counter , 0  "]
["$","2022-02-24","00:46:32.100","Init Profile","[MSC] RX: H, Last DURA       Error , 0  "]
["$","2022-02-24","00:46:32.200","Init Profile","[MSC] RX: H, Last DURA Error  Time , 01/01/1970 00:00:00  "]
["$","2022-02-24","00:46:32.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.23]
["$","2022-02-24","00:46:32.200","Init Profile","SBE41 Message",-0.23,44.826250999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.23,-0.23,-0.14768200000000001,-2.9399999999999999E-4,4.6667E-2,6.6670000000000002E-3,-5.7000000000000003E-5,3000]
["$","2022-02-24","00:46:32.300","Init Profile","[MSC] RX: H, DURA Sample   Counter , 46  "]
["$","2022-02-24","00:46:32.300","Init Profile","[MSC] RX: H, Last Sample Rec. Time , 02/24/2022 00:40:28  "]
["$","2022-02-24","00:46:32.300","Init Profile","[MSC] RX: H, AtoD Reads per Sample , 10  "]
["$","2022-02-24","00:46:32.300","Init Profile","[MSC] RX: H, AtoD Reading    Delay , 100  "]
["$","2022-02-24","00:46:32.300","Init Profile","[MSC] RX: H, Samps per AtoD  Recal , 250  "]
["$","2022-02-24","00:46:32.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:33.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:33.600","Init Profile","System Data (dBar %full Volts mAmps): ",-0.23,44.817672999999999,32.375,5,0.21248500000000001,209.525598,null,32.375,186.5,4.6481669999999999,20.939129000000001,null,null,null,null,null,null,null,null,null,1218.150024,12.49,38.502997999999998,12.49]
["$","2022-02-24","00:46:33.700","Init Profile","Pump motor not faulted"]
["$","2022-02-24","00:46:34.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:35.100","Init Profile","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:35.100","Init Profile","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:33.700","Init Profile","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:33.700","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:33.900","Init Profile","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:33.900","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:34","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:34","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:34.100","Init Profile","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:34.100","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:34.300","Init Profile","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:34.300","Init Profile","Twitter msg",null,null,null,null,null,null,"33604352;"]
["$","2022-02-24","00:46:34.500","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:34.500","Init Profile","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:34.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:34.700","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:34.700","Init Profile","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:34.900","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:34.900","Init Profile","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:35","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","00:46:35","Init Profile","SBE41 Message",-0.17,44.817672999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-0.13459699999999999,-1.413E-3,-0.02,1.3332999999999999E-2,-1.0900000000000001E-4,3000]
["$","2022-02-24","00:46:35.100","Init Profile","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:35.100","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:35.100","Init Profile","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:35.100","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:35.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:36.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:37.100","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:37.100","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:37.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:37.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:37.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:38.100","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.21]
["$","2022-02-24","00:46:38.100","Init Profile","SBE41 Message",-0.21,44.819037000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.21,-0.21,-0.13330400000000001,-2.9099999999999998E-3,1.3332999999999999E-2,-3.333E-3,-1.6000000000000001E-4,3000]
["$","2022-02-24","00:46:38.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:39.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:40.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:40.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:40.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:40.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:41.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:46:41.200","Init Profile","SBE41 Message",-0.08,44.824097000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.142341,-3.9240000000000004E-3,-4.3333000000000003E-2,-1.4999999999999999E-2,-1.9699999999999999E-4,3000]
["$","2022-02-24","00:46:41.400","Init Profile","[MSC] TX: SE,?"]
["$","2022-02-24","00:46:41.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:41.700","Init Profile","[MSC] RX: ACK,SE?,0  "]
["$","2022-02-24","00:46:41.700","Init Profile","[MSC] ERRORS AVAILABLE: 0"]
["$","2022-02-24","00:46:41.700","Init Profile","Normal State Exit"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Setting Execution Constraint = 900000"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","State Entry"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:42.100","Decrease Buoyancy Fast","Decreasing Buoyancy to pressure = 0.30 at 200000 cps"]
["$","2022-02-24","00:46:42.100","Decrease Buoyancy Fast","Initializing SBE 41 LPF"]
["$","2022-02-24","00:46:42.100","Decrease Buoyancy Fast","Checking global issues before power down"]
["$","2022-02-24","00:46:42.100","Decrease Buoyancy Fast","Disabling unneeded power"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","[MSC] Powering down MSC"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","Powering down GPS"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","[MSC] Powering down MSC"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","Powering down FLBB"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","Powering down 4330 Optode"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","Powering down OCR504"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","Powering down Bluetooth"]
["$","2022-02-24","00:46:43.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:45.200","Decrease Buoyancy Fast","Checking global issues after power down"]
["$","2022-02-24","00:46:45.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:45.300","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.08,44.818860000000001,32.375,10,0.29774099999999998,305.02091799999999,null,32.375,142,6.6663779999999999,30.488661,null,null,null,null,null,null,null,null,null,1218.099976,12.51,38.823002000000002,12.51]
["$","2022-02-24","00:46:45.400","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:46:46.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:43.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:44","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:46:44","Decrease Buoyancy Fast","SBE41 Message",-0.15,44.818860000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-8.0001000000000003E-2,0,2.3333E-2,1.1667E-2,0,3000]
["$","2022-02-24","00:46:45.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:45.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:45.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:45.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:45.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:45.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:46","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:46","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"33604352;"]
["$","2022-02-24","00:46:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:46.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:46.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:46.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:46.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:47.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","00:46:47.200","Decrease Buoyancy Fast","SBE41 Message",-0.05,44.818860000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-8.0147999999999997E-2,-1.9999999999999999E-6,-3.3333000000000002E-2,-5.0000000000000001E-3,0,3000]
["$","2022-02-24","00:46:47.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:47.400","Decrease Buoyancy Fast","Decrease buoyancy is opening valve"]
["$","2022-02-24","00:46:47.400","Decrease Buoyancy Fast","BE::openMV: Starting valve open"]
["$","2022-02-24","00:46:49.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","BE::sendJV: 200000"]
["$","2022-02-24","00:46:49.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:49.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"JV=200000;"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:50.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:46:50.200","Decrease Buoyancy Fast","SBE41 Message",-0.14000000000000001,44.836132999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-8.1617999999999996E-2,-1.2999999999999999E-5,0.03,-1.6670000000000001E-3,1.9999999999999999E-6,3000]
["$","2022-02-24","00:46:50.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:51.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:52","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:52","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:52.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:52.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:52.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:53","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.11]
["$","2022-02-24","00:46:53","Decrease Buoyancy Fast","SBE41 Message",-0.11,44.910612999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.11,-0.11,-8.6555000000000007E-2,-6.9999999999999999E-6,-0.01,0.01,1.0000000000000001E-5,3000]
["$","2022-02-24","00:46:53.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:54.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:55.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:55.300","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.11,45.161051,32.25,1135,6.4047070000000001,387.488045,null,32.274999999999999,158.5,8.2337799999999994,38.735373000000003,null,null,null,null,null,null,null,null,null,1219.01001,12.51,38.084000000000003,12.51]
["$","2022-02-24","00:46:55.400","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:46:55.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:55.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:55.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197657;"]
["$","2022-02-24","00:46:55.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:55.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.68450;"]
["$","2022-02-24","00:46:55.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:55.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:55.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:55.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"2.07450;"]
["$","2022-02-24","00:46:56","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:56","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:46:56.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.01]
["$","2022-02-24","00:46:56.200","Decrease Buoyancy Fast","SBE41 Message",0.01,45.161051,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.01,0.01,-9.4257999999999995E-2,1.5899999999999999E-4,-0.04,-2.5000000000000001E-2,2.6999999999999999E-5,3000]
["$","2022-02-24","00:46:56.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:56.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:56.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:56.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:56.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:56.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:57.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:58.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:58.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:58.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:58.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:59.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.23]
["$","2022-02-24","00:46:59.100","Decrease Buoyancy Fast","SBE41 Message",-0.23,45.516581000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.23,-0.23,-0.100286,6.1600000000000001E-4,0.08,0.02,5.0000000000000002E-5,3000]
["$","2022-02-24","00:46:59.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:00.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:01.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:01.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:01.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:01.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:02.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.01]
["$","2022-02-24","00:47:02.200","Decrease Buoyancy Fast","SBE41 Message",-0.01,45.800851999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.01,-0.01,-0.10185,1.2440000000000001E-3,-7.3332999999999995E-2,3.333E-3,7.3999999999999996E-5,3000]
["$","2022-02-24","00:47:02.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:03.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:04","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:04","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:04.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:04.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:04.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:05","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:47:05","Decrease Buoyancy Fast","SBE41 Message",-0.14000000000000001,46.106814,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-9.8904000000000006E-2,1.714E-3,4.3333000000000003E-2,-1.4999999999999999E-2,9.2999999999999997E-5,3000]
["$","2022-02-24","00:47:05.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:06.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:06.300","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.14000000000000001,46.310864000000002,32.225000000000001,1085,18.669792999999999,477.34229099999999,null,32.225000000000001,157,9.9348379999999992,47.720798000000002,null,null,null,null,null,null,null,null,null,1220.48999,12.51,38.050998999999997,12.51]
["$","2022-02-24","00:47:06.400","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:47:07.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:47:06.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:47:06.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196423;"]
["$","2022-02-24","00:47:06.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:47:06.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.72395;"]
["$","2022-02-24","00:47:06.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:47:06.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1.98416;"]
["$","2022-02-24","00:47:07","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:47:07","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","00:47:07.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:47:07.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:47:07.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:47:07.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:47:07.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:47:07.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:08.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:08.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:47:08.200","Decrease Buoyancy Fast","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:47:08.200","Decrease Buoyancy Fast","SBE41 Message",-0.14000000000000001,46.391285000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-9.4349000000000002E-2,1.6739999999999999E-3,0,2.1666999999999999E-2,1.06E-4,3000]
["$","2022-02-24","00:47:09.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:10.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:10.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:10.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:11","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:47:11","Decrease Buoyancy Fast","SBE41 Message",-0.08,46.713799000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-9.4411999999999996E-2,9.8900000000000008E-4,-0.02,-0.01,1.17E-4,3000]
["$","2022-02-24","00:47:11.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:12.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:13.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:13.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:14.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:14.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:47:14.200","Decrease Buoyancy Fast","SBE41 Message",-0.15,47.132662000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-9.9584000000000006E-2,7.2999999999999999E-5,2.3333E-2,1.6670000000000001E-3,1.34E-4,3000]
["$","2022-02-24","00:47:15.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:16.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:16.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:16.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:17.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","00:47:17.100","Decrease Buoyancy Fast","SBE41 Message",-0.1,47.325462000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.104979,-4.0700000000000003E-4,-1.6667000000000001E-2,3.333E-3,1.5699999999999999E-4,3000]
["$","2022-02-24","00:47:17.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:17.200","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.1,47.476422999999997,32.200000000000003,1130,30.736822,566.65929300000005,null,32.25,156,11.628418999999999,56.652498000000001,null,null,null,null,null,null,null,null,null,1222.079956,12.51,38.459999000000003,12.51]
["$","2022-02-24","00:47:17.300","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:47:17.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:47:17.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197505;"]
["$","2022-02-24","00:47:17.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:47:17.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.20629;"]
["$","2022-02-24","00:47:17.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:47:17.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.02729;"]
["$","2022-02-24","00:47:17.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:47:17.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"79741712;"]
["$","2022-02-24","00:47:18.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:47:18.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:47:18.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:47:18.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:47:18.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:47:18.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:19","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:19.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:20","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:20.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:47:20.200","Decrease Buoyancy Fast","SBE41 Message",-0.12,47.736158000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.110177,-1.95E-4,6.6670000000000002E-3,-5.0000000000000001E-3,1.84E-4,3000]
["$","2022-02-24","00:47:21","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:22","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:22.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:22.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:23","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:23","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","00:47:23","Decrease Buoyancy Fast","SBE41 Message",-0.05,47.981763999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-0.115027,5.1599999999999997E-4,-2.3333E-2,-8.3330000000000001E-3,2.1599999999999999E-4,3000]
["$","2022-02-24","00:47:24","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:25","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:25.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:26","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:26.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:47:26.200","Decrease Buoyancy Fast","SBE41 Message",-0.09,48.412565999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.117079,1.3159999999999999E-3,1.3332999999999999E-2,-5.0000000000000001E-3,2.4800000000000001E-4,3000]
["$","2022-02-24","00:47:27","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:28","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:28","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.09,48.589958000000003,32.25,1130,42.680557,655.707672,null,32.25,156,13.31413,65.557336000000006,null,null,null,null,null,null,null,null,null,1223.5500489999999,12.54,38.382998999999998,12.54]
["$","2022-02-24","00:47:28.100","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:47:28.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:47:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:28.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:47:28.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196705;"]
["$","2022-02-24","00:47:28.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:47:28.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.11642;"]
["$","2022-02-24","00:47:28.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:47:28.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.71379;"]
["$","2022-02-24","00:47:28.600","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:28.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:47:28.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:47:28.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:47:28.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:47:29","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.23]
["$","2022-02-24","00:47:29","Decrease Buoyancy Fast","SBE41 Message",-0.23,48.589958000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.23,-0.23,-0.115735,1.74E-3,4.6667E-2,0.03,2.7599999999999999E-4,3000]
["$","2022-02-24","00:47:29.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:47:29.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:47:29.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:47:29.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:30","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:31","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:31.500","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:31.500","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:31.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:31.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:32","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:32","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.21]
["$","2022-02-24","00:47:32","Decrease Buoyancy Fast","SBE41 Message",-0.21,49.024785000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.21,-0.21,-0.10975,1.572E-3,-6.6670000000000002E-3,0.02,2.9399999999999999E-4,3000]
["$","2022-02-24","00:47:33","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:34","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:34.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:34.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:34.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:35","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:35.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.22]
["$","2022-02-24","00:47:35.200","Decrease Buoyancy Fast","SBE41 Message",-0.22,49.319819000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.22,-0.22,-0.101577,8.9300000000000002E-4,3.333E-3,-1.6670000000000001E-3,2.9999999999999997E-4,3000]
["$","2022-02-24","00:47:36","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:37","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:37","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:37","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:37.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:37.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:38","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:38.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.11]
["$","2022-02-24","00:47:38.100","Decrease Buoyancy Fast","SBE41 Message",-0.11,49.655622999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.11,-0.11,-0.105013,-1.9900000000000001E-4,-3.6666999999999998E-2,-1.6667000000000001E-2,3.0899999999999998E-4,3000]
["$","2022-02-24","00:47:39","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:39","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.11,49.675153999999999,32.174999999999997,1030,54.624293000000002,745.83054100000004,null,32.200000000000003,155.5,15.021089999999999,74.569623000000007,null,null,null,null,null,null,null,null,null,1225.089966,12.53,37.930999999999997,12.53]
["$","2022-02-24","00:47:39.100","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:47:39.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:47:39.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"195820;"]
["$","2022-02-24","00:47:39.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:47:39.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.49682;"]
["$","2022-02-24","00:47:40.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:39.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:47:39.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.10167;"]
["$","2022-02-24","00:47:39.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:47:39.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:47:39.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:47:39.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:47:40.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:47:40.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:47:40.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:47:40.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:40.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:41.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","00:47:41.200","Decrease Buoyancy Fast","SBE41 Message",-0.17,49.804412999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-0.13144700000000001,-1.1999999999999999E-3,0.02,-8.3330000000000001E-3,3.4900000000000003E-4,3000]
["$","2022-02-24","00:47:41.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:42.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:43.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:43.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:43.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:44.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.16]
["$","2022-02-24","00:47:44.100","Decrease Buoyancy Fast","SBE41 Message",-0.16,50.149845999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.16,-0.16,-0.168514,-8.2700000000000004E-4,-3.333E-3,8.3330000000000001E-3,4.3199999999999998E-4,3000]
["$","2022-02-24","00:47:44.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:45.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:46.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:46.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:47.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:47:47.200","Decrease Buoyancy Fast","SBE41 Message",-0.09,50.463326000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.18921199999999999,1.6540000000000001E-3,-2.3333E-2,-1.3332999999999999E-2,5.3499999999999999E-4,3000]
["$","2022-02-24","00:47:47.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:48.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:49.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:49.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:49.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:49.900","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.09,50.752968000000003,32.225000000000001,1160,66.564093999999997,835.28185399999995,null,32.25,156.5,16.715720999999998,83.514753999999996,null,null,null,null,null,null,null,null,null,1226.650024,12.53,38.528998999999999,12.53]
["$","2022-02-24","00:47:50","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:47:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:47:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197243;"]
["$","2022-02-24","00:47:50","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:47:50","Decrease Buoyancy Fast","SBE41 Message",-0.15,50.752968000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-0.18359900000000001,5.084E-3,0.02,-1.6670000000000001E-3,6.2399999999999999E-4,3000]
["$","2022-02-24","00:47:50.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:47:50.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.61254;"]
["$","2022-02-24","00:47:50.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:47:50.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"2.46768;"]
["$","2022-02-24","00:47:50.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:47:50.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","00:47:50.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:47:50.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:47:51","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:47:51","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:47:51.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:47:51.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:51.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:52.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","00:47:52.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:53.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:54.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:54.200","Decrease Buoyancy Fast","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:47:54.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:55.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:55.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:55.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:56","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:47:56","Decrease Buoyancy Fast","SBE41 Message",-0.08,51.341512999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.16617699999999999,7.1929999999999997E-3,-2.3333E-2,-1.6670000000000001E-3,6.8400000000000004E-4,3000]
["$","2022-02-24","00:47:56.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:57.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:58.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:58.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:59.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:47:59.200","Decrease Buoyancy Fast","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:47:59.200","Decrease Buoyancy Fast","SBE41 Message",-0.08,51.659756000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.151534,6.4460000000000003E-3,0,-1.1667E-2,7.18E-4,3000]
["$","2022-02-24","00:47:59.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:00.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:00.900","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.08,51.839185000000001,32.15,1050,79.192502000000005,925.00179000000003,null,32.200000000000003,157,18.414549000000001,92.486748000000006,null,null,null,null,null,null,null,null,null,1228.160034,12.54,38.383999000000003,12.54]
["$","2022-02-24","00:48:00.900","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:01.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:01","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:01","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"195013;"]
["$","2022-02-24","00:48:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:01.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:01.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.06292;"]
["$","2022-02-24","00:48:01.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:01.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1.33122;"]
["$","2022-02-24","00:48:01.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:01.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"79741712;"]
["$","2022-02-24","00:48:01.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:01.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:01.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:02","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:02","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:02","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:48:02","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,51.839185000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.13977000000000001,3.078E-3,-3.333E-3,-1.6670000000000001E-3,7.3300000000000004E-4,3000]
["$","2022-02-24","00:48:02.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:02.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:02.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:03.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:04.300","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:04.300","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:04.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:04.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:04.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:05","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:48:05","Decrease Buoyancy Fast","SBE41 Message",-0.12,52.257353000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.126999,-1.126E-3,1.6667000000000001E-2,6.6670000000000002E-3,7.27E-4,3000]
["$","2022-02-24","00:48:05.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:06.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:07.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:07.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:08.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.11]
["$","2022-02-24","00:48:08.200","Decrease Buoyancy Fast","SBE41 Message",-0.11,52.539012,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.11,-0.11,-0.11290699999999999,-4.0749999999999996E-3,-3.333E-3,6.6670000000000002E-3,7.0100000000000002E-4,3000]
["$","2022-02-24","00:48:08.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:09.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:10.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:10.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:10.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:11","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.18]
["$","2022-02-24","00:48:11","Decrease Buoyancy Fast","SBE41 Message",-0.18,52.830970000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.18,-0.18,-9.8955000000000001E-2,-4.9950000000000003E-3,2.3333E-2,0.01,6.5700000000000003E-4,3000]
["$","2022-02-24","00:48:11.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:11.800","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.18,52.909388999999997,32.200000000000003,1155,91.965190000000007,1015.124659,null,32.174999999999997,153.5,20.123739,101.49903500000001,null,null,null,null,null,null,null,null,null,1229.719971,12.56,38.574001000000003,12.56]
["$","2022-02-24","00:48:11.900","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:13.300","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:13.400","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:11.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:11.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"195727;"]
["$","2022-02-24","00:48:12.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:12.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.26283;"]
["$","2022-02-24","00:48:12.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:12.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1.86312;"]
["$","2022-02-24","00:48:12.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:12.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"46187280;"]
["$","2022-02-24","00:48:12.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:12.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:12.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:13","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:13.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:13.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:13.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:13.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:13.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:13.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:13.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:13.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:14.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.11]
["$","2022-02-24","00:48:14.200","Decrease Buoyancy Fast","SBE41 Message",-0.11,52.979253,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.11,-0.11,-9.0315999999999994E-2,-4.8149999999999998E-3,-2.3333E-2,0,6.0099999999999997E-4,3000]
["$","2022-02-24","00:48:14.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:15.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:16.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:16.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:16.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:17.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","00:48:17.100","Decrease Buoyancy Fast","SBE41 Message",0,53.399253999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0,0,-9.3354000000000006E-2,-4.5960000000000003E-3,-3.6666999999999998E-2,-0.03,5.4900000000000001E-4,3000]
["$","2022-02-24","00:48:17.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:18.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:19.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:19.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:20.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:48:20.200","Decrease Buoyancy Fast","SBE41 Message",-0.08,53.658524999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.10709200000000001,-4.1669999999999997E-3,2.6667E-2,-5.0000000000000001E-3,5.1400000000000003E-4,3000]
["$","2022-02-24","00:48:20.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:21.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:22.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:22.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:22.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:22.700","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.08,53.988062999999997,32.15,1050,104.61327300000001,1104.3073489999999,null,32.225000000000001,156,21.811024,110.417304,null,null,null,null,null,null,null,null,null,1231.3100589999999,12.56,38.884998000000003,12.56]
["$","2022-02-24","00:48:22.800","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:22.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:22.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"194762;"]
["$","2022-02-24","00:48:23","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:23","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.74971;"]
["$","2022-02-24","00:48:23","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:48:23","Decrease Buoyancy Fast","SBE41 Message",-0.14000000000000001,53.988062999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.120505,-2.7529999999999998E-3,0.02,2.3333E-2,4.9299999999999995E-4,3000]
["$","2022-02-24","00:48:23.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:23.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-1.80043;"]
["$","2022-02-24","00:48:23.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:23.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:48:23.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:23.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:23.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:23.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:24","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:24","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:24.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:25.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:25.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:26.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:48:26.200","Decrease Buoyancy Fast","SBE41 Message",-0.08,54.279539999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.11851399999999999,-3.6400000000000001E-4,-0.02,0,4.6799999999999999E-4,3000]
["$","2022-02-24","00:48:26.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:27.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:28.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:28.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:28.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:29","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:48:29","Decrease Buoyancy Fast","SBE41 Message",-0.12,54.521110999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-9.8710000000000006E-2,1.774E-3,1.3332999999999999E-2,-3.333E-3,4.1800000000000002E-4,3000]
["$","2022-02-24","00:48:29.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:30.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:31.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:31.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:31.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:31.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:32.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:48:32.200","Decrease Buoyancy Fast","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:48:32.200","Decrease Buoyancy Fast","SBE41 Message",-0.12,54.799463000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-8.0685999999999994E-2,2.088E-3,0,6.6670000000000002E-3,3.4499999999999998E-4,3000]
["$","2022-02-24","00:48:32.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:33.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:33.700","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.12,55.011890000000001,32.200000000000003,1180,117.17741100000001,1194.0272849999999,null,32.174999999999997,160,23.513787000000001,119.389297,null,null,null,null,null,null,null,null,null,1232.790039,12.56,38.011001999999998,12.56]
["$","2022-02-24","00:48:33.700","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:34.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:33.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:33.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"198063;"]
["$","2022-02-24","00:48:34","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:34","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.38084;"]
["$","2022-02-24","00:48:34","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:34","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:34.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:34.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.93212;"]
["$","2022-02-24","00:48:34.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:34.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"96518928;"]
["$","2022-02-24","00:48:34.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:34.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:34.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:34.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:34.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:35","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:35","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:35","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:48:35","Decrease Buoyancy Fast","SBE41 Message",-0.15,55.011890000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-8.2055000000000003E-2,2.9500000000000001E-4,0.01,5.0000000000000001E-3,2.7500000000000002E-4,3000]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:35.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:36.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:37.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:37.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:37.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:37.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:37.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:38.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:48:38.100","Decrease Buoyancy Fast","SBE41 Message",-0.08,55.400098,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-9.5448000000000005E-2,-2.0330000000000001E-3,-2.3333E-2,-6.6670000000000002E-3,2.2100000000000001E-4,3000]
["$","2022-02-24","00:48:38.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:39.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:40.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:40.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:41.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.16]
["$","2022-02-24","00:48:41.200","Decrease Buoyancy Fast","SBE41 Message",-0.16,55.721471000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.16,-0.16,-0.106507,-2.9870000000000001E-3,2.6667E-2,1.6670000000000001E-3,1.8000000000000001E-4,3000]
["$","2022-02-24","00:48:41.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:42.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:43.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:43.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:43.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:44.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:48:44.100","Decrease Buoyancy Fast","SBE41 Message",-0.14000000000000001,55.956040000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.11397699999999999,-1.9109999999999999E-3,-6.6670000000000002E-3,0.01,1.46E-4,3000]
["$","2022-02-24","00:48:44.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:44.600","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.14000000000000001,56.050801,32.174999999999997,1170,129.7022,1284.1501539999999,null,32.225000000000001,157.5,25.222714,128.40158400000001,null,null,null,null,null,null,null,null,null,1234.380005,12.58,38.553001000000002,12.58]
["$","2022-02-24","00:48:44.700","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:46.100","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:46.100","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:44.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:44.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"199230;"]
["$","2022-02-24","00:48:44.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:44.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.71885;"]
["$","2022-02-24","00:48:45.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:45.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.748429e-04;"]
["$","2022-02-24","00:48:45.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:45.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"96518928;"]
["$","2022-02-24","00:48:45.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:45.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:45.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:45.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:45.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:45.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:46.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:46.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:47.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:48:47.200","Decrease Buoyancy Fast","SBE41 Message",-0.08,56.161847000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.120007,4.7899999999999999E-4,-0.02,-1.3332999999999999E-2,1.17E-4,3000]
["$","2022-02-24","00:48:47.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:48.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:49.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:49.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:49.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:50","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:48:50","Decrease Buoyancy Fast","SBE41 Message",-0.15,56.555619,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-0.123269,2.6389999999999999E-3,2.3333E-2,1.6670000000000001E-3,9.0000000000000006E-5,3000]
["$","2022-02-24","00:48:50.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:51.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:52.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:52.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:53.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","00:48:53.200","Decrease Buoyancy Fast","SBE41 Message",-0.1,56.853907999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.125218,3.2629999999999998E-3,-1.6667000000000001E-2,3.333E-3,6.3999999999999997E-5,3000]
["$","2022-02-24","00:48:53.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:54.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:55","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:55","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:55.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:55.500","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.1,57.184972999999999,32.174999999999997,1255,142.11812399999999,1373.198533,null,32.15,155.5,26.911442000000001,137.306422,null,null,null,null,null,null,null,null,null,1235.959961,12.58,39.173999999999999,12.58]
["$","2022-02-24","00:48:55.600","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:55.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:55.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:55.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196866;"]
["$","2022-02-24","00:48:55.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:55.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:55.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.06470;"]
["$","2022-02-24","00:48:56","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:56","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-1.10416;"]
["$","2022-02-24","00:48:56","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:48:56","Decrease Buoyancy Fast","SBE41 Message",-0.15,57.184972999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-0.126799,2.555E-3,1.6667000000000001E-2,0,4.3000000000000002E-5,3000]
["$","2022-02-24","00:48:56.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:56.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","00:48:56.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:56.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:56.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:56.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:57.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:58.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:58.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:59.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:48:59.200","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,57.440992999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.125113,1.6750000000000001E-3,-2.6667E-2,-5.0000000000000001E-3,2.6999999999999999E-5,3000]
["$","2022-02-24","00:48:59.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:00.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:01.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:01.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:01.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:02","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:49:02","Decrease Buoyancy Fast","SBE41 Message",-0.12,57.697634000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.121397,1.0449999999999999E-3,1.6667000000000001E-2,-5.0000000000000001E-3,1.2999999999999999E-5,3000]
["$","2022-02-24","00:49:02.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:03.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:04.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:04.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:04.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:04.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:05.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","00:49:05.200","Decrease Buoyancy Fast","SBE41 Message",-0.05,58.000996000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-0.11996800000000001,4.1599999999999997E-4,-2.3333E-2,-3.333E-3,-3.0000000000000001E-6,3000]
["$","2022-02-24","00:49:05.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:06.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:06.500","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.05,58.193772000000003,32.174999999999997,1155,154.51830799999999,1463.05278,null,32.200000000000003,155,28.613417999999999,146.27841599999999,null,null,null,null,null,null,null,null,null,1237.5,12.58,38.918998999999999,12.58]
["$","2022-02-24","00:49:06.500","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:49:07.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:49:06.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:49:06.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196054;"]
["$","2022-02-24","00:49:06.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:49:06.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.99357;"]
["$","2022-02-24","00:49:07","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:49:07","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.74678;"]
["$","2022-02-24","00:49:07","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:07","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:07.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:49:07.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"96518928;"]
["$","2022-02-24","00:49:07.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:49:07.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:49:07.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:49:07.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:49:07.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:49:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.11]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","SBE41 Message",-0.11,58.193772000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.11,-0.11,-0.118953,-1.3200000000000001E-4,0.02,-1.6670000000000001E-3,-2.4000000000000001E-5,3000]
["$","2022-02-24","00:49:08.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:09.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:10.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:10.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:10.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:11","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","00:49:11","Decrease Buoyancy Fast","SBE41 Message",-0.1,58.541772000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.113371,-4.2400000000000001E-4,-3.333E-3,8.3330000000000001E-3,-5.8999999999999998E-5,3000]
["$","2022-02-24","00:49:11.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:12.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:13.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:13.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:14.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:49:14.200","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,58.906404999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.103365,-6.5899999999999997E-4,-0.01,-6.6670000000000002E-3,-1.07E-4,3000]
["$","2022-02-24","00:49:14.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:15.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:16.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:16.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:16.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:17","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.04]
["$","2022-02-24","00:49:17","Decrease Buoyancy Fast","SBE41 Message",-0.04,59.166539999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.04,-0.04,-9.3922000000000005E-2,-1.067E-3,-0.01,-0.01,-1.6000000000000001E-4,3000]
["$","2022-02-24","00:49:17.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:17.400","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.04,59.330317000000001,32.15,1060,166.97751500000001,1553.041338,null,32.15,157.5,30.320903000000001,155.27727200000001,null,null,null,null,null,null,null,null,null,1239.030029,12.59,39.318001000000002,12.59]
["$","2022-02-24","00:49:17.500","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:49:18.900","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:49:18.900","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:49:17.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:49:17.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"194223;"]
["$","2022-02-24","00:49:17.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:49:17.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.73562;"]
["$","2022-02-24","00:49:17.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:49:17.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.62581;"]
["$","2022-02-24","00:49:18.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:49:18.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","00:49:18.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:49:18.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:49:18.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:49:18.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:49:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:49:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:49:19","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:49:19","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:19","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:49:19","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:19.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:19.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:20.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:49:20.200","Decrease Buoyancy Fast","SBE41 Message",-0.08,59.353662999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-8.9493000000000003E-2,-1.6440000000000001E-3,1.3332999999999999E-2,1.6670000000000001E-3,-2.12E-4,3000]
["$","2022-02-24","00:49:20.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:21.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:22.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:22.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:22.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:23","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:49:23","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,59.796044999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-8.8497000000000006E-2,-2.2009999999999998E-3,-3.333E-3,5.0000000000000001E-3,-2.5700000000000001E-4,3000]
["$","2022-02-24","00:49:23.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:24.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:25.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:25.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:26.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","00:49:26.200","Decrease Buoyancy Fast","SBE41 Message",0,59.977243999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0,0,-8.412E-2,-2.398E-3,-2.3333E-2,-1.3332999999999999E-2,-3.01E-4,3000]
["$","2022-02-24","00:49:26.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:27.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:28.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:28.300","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",0,60.288666999999997,32.15,1190,179.26489900000001,1642.0897170000001,null,32.200000000000003,156,32.012253999999999,164.19554099999999,null,null,null,null,null,null,null,null,null,1240.599976,12.6,38.334000000000003,12.6]
["$","2022-02-24","00:49:28.400","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:49:28.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:49:28.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:49:28.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197115;"]
["$","2022-02-24","00:49:28.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:49:28.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1.11942;"]
["$","2022-02-24","00:49:28.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:28.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:49:28.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1.03083;"]
["$","2022-02-24","00:49:29","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:49:29","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:49:29","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.02]
["$","2022-02-24","00:49:29","Decrease Buoyancy Fast","SBE41 Message",0.02,60.288666999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.02,0.02,-7.4582999999999997E-2,-2.1289999999999998E-3,-6.6670000000000002E-3,-1.4999999999999999E-2,-3.5199999999999999E-4,3000]
["$","2022-02-24","00:49:29.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:49:29.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:49:29.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:49:29.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:49:29.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:49:29.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:30.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:31.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:31.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:31.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:31.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:32.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:49:32.100","Decrease Buoyancy Fast","SBE41 Message",-0.09,60.598512999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-6.5625000000000003E-2,-1.776E-3,3.6666999999999998E-2,1.4999999999999999E-2,-4.1300000000000001E-4,3000]
["$","2022-02-24","00:49:32.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:33.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:34.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:34.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:34.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:34.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:35.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:49:35.200","Decrease Buoyancy Fast","SBE41 Message",-0.12,60.86647,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-5.7674000000000003E-2,-1.7080000000000001E-3,0.01,2.3333E-2,-4.8899999999999996E-4,3000]
["$","2022-02-24","00:49:35.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:36.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:37","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:37","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:37.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:37.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:37.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:38","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","00:49:38","Decrease Buoyancy Fast","SBE41 Message",0,61.165126000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0,0,-4.4837000000000002E-2,-1.9949999999999998E-3,-0.04,-1.4999999999999999E-2,-5.8799999999999998E-4,3000]
["$","2022-02-24","00:49:38.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:39.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:39.300","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",0,61.333185,32.125,1080,191.61655300000001,1732.0782750000001,null,32.15,156,33.718034000000003,173.19439600000001,null,null,null,null,null,null,null,null,null,1242.209961,12.6,37.902999999999999,12.6]
["$","2022-02-24","00:49:39.400","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:49:40.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:49:39.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:49:39.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196392;"]
["$","2022-02-24","00:49:39.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:49:39.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.96612;"]
["$","2022-02-24","00:49:39.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:49:39.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.46999;"]
["$","2022-02-24","00:49:40","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:49:40","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","00:49:40.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:49:40.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:49:40.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:49:40.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:49:40.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:49:40.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:41.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:41.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:49:41.200","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,61.507972000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-3.2650999999999999E-2,-2.6719999999999999E-3,2.3333E-2,-8.3330000000000001E-3,-6.9499999999999998E-4,3000]
["$","2022-02-24","00:49:42.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:43.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:43.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:43.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:44","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:49:44","Decrease Buoyancy Fast","SBE41 Message",-0.09,61.691792999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-3.6065E-2,-3.4870000000000001E-3,6.6670000000000002E-3,1.4999999999999999E-2,-7.6000000000000004E-4,3000]
["$","2022-02-24","00:49:44.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:45.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:46.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:46.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:47.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:47.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","00:49:47.200","Decrease Buoyancy Fast","SBE41 Message",-0.17,62.109158999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-5.2559000000000002E-2,-3.5739999999999999E-3,2.6667E-2,1.6667000000000001E-2,-7.5100000000000004E-4,3000]
["$","2022-02-24","00:49:48.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:49.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:49.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:49.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:50","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:49:50","Decrease Buoyancy Fast","SBE41 Message",-0.08,62.285446,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-6.3098000000000001E-2,-2.3530000000000001E-3,-0.03,-1.6670000000000001E-3,-6.9499999999999998E-4,3000]
["$","2022-02-24","00:49:50.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:50.200","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.08,62.436242999999997,32.174999999999997,1130,203.83966599999999,1821.3952770000001,null,32.174999999999997,155,35.412533000000003,182.12609699999999,null,null,null,null,null,null,null,null,null,1243.75,12.6,39.165000999999997,12.6]
["$","2022-02-24","00:49:50.200","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:49:51.600","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:49:51.700","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:49:50.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:49:50.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196434;"]
["$","2022-02-24","00:49:50.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:49:50.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-1.03954;"]
["$","2022-02-24","00:49:50.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:49:50.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.03864;"]
["$","2022-02-24","00:49:50.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:49:50.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","00:49:51.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:49:51.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:49:51.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:49:51.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:49:51.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:49:51.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:49:51.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:49:51.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:51.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:49:51.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:52","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:52.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:53","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:53.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.04]
["$","2022-02-24","00:49:53.200","Decrease Buoyancy Fast","SBE41 Message",0.04,62.674703999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.04,0.04,-6.5087999999999993E-2,-3.97E-4,-0.04,-3.5000000000000003E-2,-6.3500000000000004E-4,3000]
["$","2022-02-24","00:49:54","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:55","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:55","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:55","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:55.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:55.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:56","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:56","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:49:56","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,62.971617000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-7.4315999999999993E-2,1.366E-3,3.6666999999999998E-2,-1.6670000000000001E-3,-5.7799999999999995E-4,3000]
["$","2022-02-24","00:49:57","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:58","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:58.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:59","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:59.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","00:49:59.200","Decrease Buoyancy Fast","SBE41 Message",-0.05,63.207141,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-9.0900999999999996E-2,2.6649999999999998E-3,-6.6670000000000002E-3,1.4999999999999999E-2,-5.1400000000000003E-4,3000]
["$","2022-02-24","00:50:00","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:01","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:01","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.05,63.430210000000002,32.174999999999997,1170,216.04704000000001,1910.4436559999999,null,32.174999999999997,156.5,37.103228999999999,191.030934,null,null,null,null,null,null,null,null,null,1245.3599850000001,12.61,38.168998999999999,12.61]
["$","2022-02-24","00:50:01.100","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:50:01.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:01.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:01.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196897;"]
["$","2022-02-24","00:50:01.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:01.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.32136;"]
["$","2022-02-24","00:50:01.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:01.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.31309;"]
["$","2022-02-24","00:50:01.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:01.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:01.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","00:50:01.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:01.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:02","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.03]
["$","2022-02-24","00:50:02","Decrease Buoyancy Fast","SBE41 Message",-0.03,63.430210000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.03,-0.03,-9.3081999999999998E-2,3.4979999999999998E-3,-6.6670000000000002E-3,-6.6670000000000002E-3,-4.5899999999999999E-4,3000]
["$","2022-02-24","00:50:02.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:02.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:02.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:02.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:03","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:04","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:04.500","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:04.500","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:04.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:04.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:05","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:05","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.09]
["$","2022-02-24","00:50:05","Decrease Buoyancy Fast","SBE41 Message",0.09,63.800210999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.09,0.09,-7.1984000000000006E-2,3.5239999999999998E-3,-0.04,-2.3333E-2,-4.4299999999999998E-4,3000]
["$","2022-02-24","00:50:06","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:07","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:07.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:08","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:08.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:50:08.200","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,64.114885999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-4.7541E-2,2.3960000000000001E-3,5.3332999999999998E-2,6.6670000000000002E-3,-4.7100000000000001E-4,3000]
["$","2022-02-24","00:50:09","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:10","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:10.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:10.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:11","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:11.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:50:11.100","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,64.442313999999996,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-3.6160999999999999E-2,2.9100000000000003E-4,0,2.6667E-2,-5.2700000000000002E-4,3000]
["$","2022-02-24","00:50:12","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:12","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-7.0000000000000007E-2,64.509366999999997,32.15,1175,228.35672099999999,2000.566525,null,32.174999999999997,153,38.811762999999999,200.04322099999999,null,null,null,null,null,null,null,null,null,1247.01001,12.62,38.004002,12.62]
["$","2022-02-24","00:50:12.100","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:12.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:12.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197708;"]
["$","2022-02-24","00:50:12.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:12.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.76077;"]
["$","2022-02-24","00:50:12.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:12.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.46275;"]
["$","2022-02-24","00:50:13.700","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:12.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:12.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:50:12.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:12.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:13.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:13.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:13.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:13.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:13.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:14.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","00:50:14.200","Decrease Buoyancy Fast","SBE41 Message",-0.05,64.587228999999994,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-2.801E-2,-2.209E-3,-6.6670000000000002E-3,-3.333E-3,-5.9999999999999995E-4,3000]
["$","2022-02-24","00:50:14.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:15.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:16.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:16.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:16.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:17","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.02]
["$","2022-02-24","00:50:17","Decrease Buoyancy Fast","SBE41 Message",-0.02,64.910131000000007,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.02,-0.02,-1.5001E-2,-4.4270000000000004E-3,-0.01,-8.3330000000000001E-3,-6.8199999999999999E-4,3000]
["$","2022-02-24","00:50:17.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:18.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:19.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:19.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:20.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.01]
["$","2022-02-24","00:50:20.200","Decrease Buoyancy Fast","SBE41 Message",0.01,65.185338999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.01,0.01,-1.1454000000000001E-2,-5.6059999999999999E-3,-0.01,-0.01,-7.4399999999999998E-4,3000]
["$","2022-02-24","00:50:20.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:21.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:22.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:22.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:22.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:22.900","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",0.01,65.570761000000005,32.174999999999997,1155,240.51949999999999,2089.883527,null,32.15,156.5,40.508361000000001,208.97492199999999,null,null,null,null,null,null,null,null,null,1248.48999,12.62,38.801997999999998,12.62]
["$","2022-02-24","00:50:23","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:23","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:23","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197349;"]
["$","2022-02-24","00:50:23","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.03]
["$","2022-02-24","00:50:23","Decrease Buoyancy Fast","SBE41 Message",0.03,65.570761000000005,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.03,0.03,-2.5864999999999999E-2,-5.1050000000000002E-3,-6.6670000000000002E-3,-8.3330000000000001E-3,-7.67E-4,3000]
["$","2022-02-24","00:50:23.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:23.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-1.20743;"]
["$","2022-02-24","00:50:23.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:23.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-1.21772;"]
["$","2022-02-24","00:50:23.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:23.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","00:50:23.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:23.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:24","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:24","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:24.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:25.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","00:50:25.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:26.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:27.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:27.200","Decrease Buoyancy Fast","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:50:27.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:28.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:28.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:28.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:29","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.16]
["$","2022-02-24","00:50:29","Decrease Buoyancy Fast","SBE41 Message",0.16,66.085576000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.16,0.16,-4.0897999999999997E-2,-3.0990000000000002E-3,-4.3333000000000003E-2,-2.5000000000000001E-2,-7.6400000000000003E-4,3000]
["$","2022-02-24","00:50:29.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:30.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:31.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:31.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:31.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:31.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:32.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.25]
["$","2022-02-24","00:50:32.200","Decrease Buoyancy Fast","SBE41 Message",0.25,66.310615999999996,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.25,0.25,-3.7883E-2,-6.5700000000000003E-4,-0.03,-3.6666999999999998E-2,-7.85E-4,3000]
["$","2022-02-24","00:50:32.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:33.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:33.800","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",0.25,66.570903999999999,32.15,1040,252.71638100000001,2179.603462,null,32.15,157,42.206926000000003,217.94691499999999,null,null,null,null,null,null,null,null,null,1250.130005,12.62,38.501998999999998,12.62]
["$","2022-02-24","00:50:33.900","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:50:34.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:35.300","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:35.300","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:33.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:33.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"194354;"]
["$","2022-02-24","00:50:34","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:34","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:34.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:34.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.05560;"]
["$","2022-02-24","00:50:34.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:34.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.21171;"]
["$","2022-02-24","00:50:34.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:34.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","00:50:34.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:34.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:34.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:34.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:34.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:35","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.36]
["$","2022-02-24","00:50:35","Decrease Buoyancy Fast","SBE41 Message",0.36,66.570903999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.36,0.36,-1.6070000000000001E-2,1.188E-3,-3.6666999999999998E-2,-3.3333000000000002E-2,-8.5300000000000003E-4,3000]
["$","2022-02-24","00:50:35.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:35.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:35.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:35.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:35.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:35.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:35.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:36.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:37.300","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:37.300","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:37.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:37.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:37.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:38","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.42]
["$","2022-02-24","00:50:38","Decrease Buoyancy Fast","SBE41 Message",0.42,66.931781999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.42,0.42,2.1349E-2,1.779E-3,-0.02,-2.8333000000000001E-2,-9.6000000000000002E-4,3000]
["$","2022-02-24","00:50:38.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:39.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:40.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:40.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:41.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.56000000000000005]
["$","2022-02-24","00:50:41.200","Decrease Buoyancy Fast","SBE41 Message",0.56000000000000005,67.205616000000006,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.56000000000000005,0.56000000000000005,7.8839000000000006E-2,2.7E-4,-4.6667E-2,-3.3333000000000002E-2,-1.1150000000000001E-3,3000]
["$","2022-02-24","00:50:41.300","Decrease Buoyancy Fast","2022-Feb-24T00:50:41Z,Exiting Dec Buocy depth > threshold 0.3 dBar,0.56,67.21,32.15,155.50"]
["$","2022-02-24","00:50:41.300","Decrease Buoyancy Fast","Normal State Exit"]
["$","2022-02-24","00:50:41.300","Descend","Setting Execution Constraint = 1800000"]
["$","2022-02-24","00:50:41.400","Descend","State Entry"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"~?;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,":?;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"~?;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,":?;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.900","Descend","BE::openMV: Starting valve open"]
["$","2022-02-24","00:50:41.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:42.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:43","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:43","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:43.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:43.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:43.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:43.900","Descend","System Data (dBar %full Volts mAmps): ",0.56000000000000005,67.366259999999997,32.274999999999999,5,261.00328200000001,2262.0705889999999,null,32.274999999999999,148.5,43.743112000000004,226.18019699999999,null,null,null,null,null,null,null,null,null,1251.26001,12.63,38.935001,12.63]
["$","2022-02-24","00:50:44","Descend","Pump motor not faulted"]
["$","2022-02-24","00:50:45.400","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:45.400","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:44","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:44","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:44","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.76]
["$","2022-02-24","00:50:44","Descend","SBE41 Message",0.76,67.366259999999997,32.15,155.5,null,null,null,null,null,null,null,null,0.76,0.76,0.15839400000000001,-3.9449999999999997E-3,-6.6667000000000004E-2,-5.6667000000000002E-2,-1.34E-3,3000]
["$","2022-02-24","00:50:44.200","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:44.200","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:44.400","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:44.400","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:44.600","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:44.600","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:50:44.800","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:44.800","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:45","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:45","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:45.200","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:45.200","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:45.400","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:45.400","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:45.400","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:45.400","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:46.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:46.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:46.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:46.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","00:50:47.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:48.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:48.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:48.200","Descend","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:50:49.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:49.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:49.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:50","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,1.27]
["$","2022-02-24","00:50:50","Descend","SBE41 Message",1.27,67.384682999999995,32.15,155.5,null,null,null,null,null,null,null,null,1.27,1.27,0.25160900000000003,-1.0200000000000001E-2,-0.17,-0.11833299999999999,-1.658E-3,3000]
["$","2022-02-24","00:50:50.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:51.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:52.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:52.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:52.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:52.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:53.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:53.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,1.52]
["$","2022-02-24","00:50:53.200","Descend","SBE41 Message",1.52,67.373531999999997,32.15,155.5,null,null,null,null,null,null,null,null,1.52,1.52,0.35157500000000003,-1.6917999999999999E-2,-8.3333000000000004E-2,-0.126667,-2.062E-3,3000]
["$","2022-02-24","00:50:54.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:54.200","Descend","System Data (dBar %full Volts mAmps): ",1.52,67.371357000000003,32.299999999999997,5,261.06623999999999,2346.283762,null,32.299999999999997,147,45.247686999999999,234.61494500000001,null,null,null,null,null,null,null,null,null,1251.290039,12.64,39.055999999999997,12.64]
["$","2022-02-24","00:50:54.300","Descend","Pump motor not faulted"]
["$","2022-02-24","00:50:55.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:55.700","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:55.700","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:54.300","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:54.300","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:54.500","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:54.500","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:54.700","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:54.700","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:54.900","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:54.900","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:50:55","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:55","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:55.100","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:55.100","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:55.300","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:55.300","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:55.500","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:55.500","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:55.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:55.700","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:55.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:55.700","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:55.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:56","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,1.78]
["$","2022-02-24","00:50:56","Descend","SBE41 Message",1.78,67.371357000000003,32.15,155.5,null,null,null,null,null,null,null,null,1.78,1.78,0.47111900000000001,-2.2915000000000001E-2,-8.6666999999999994E-2,-8.5000000000000006E-2,-2.5730000000000002E-3,3000]
["$","2022-02-24","00:50:56.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:57.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:58.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:58.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:58.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:58.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:59.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:59.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,2.0699999999999998]
["$","2022-02-24","00:50:59.200","Descend","SBE41 Message",2.0699999999999998,67.369152,32.15,155.5,null,null,null,null,null,null,null,null,2.0699999999999998,2.0699999999999998,0.64299399999999995,-2.8049999999999999E-2,-9.6667000000000003E-2,-9.1666999999999998E-2,-3.2450000000000001E-3,3000]
["$","2022-02-24","00:51:00.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:01","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:01","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:01.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:01.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:01.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:02.100","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,2.3199999999999998]
["$","2022-02-24","00:51:02.100","Descend","SBE41 Message",2.3199999999999998,67.377156999999997,32.15,155.5,null,null,null,null,null,null,null,null,2.3199999999999998,2.3199999999999998,0.88953300000000002,-3.3603000000000001E-2,-8.3333000000000004E-2,-0.09,-4.1520000000000003E-3,3000]
["$","2022-02-24","00:51:02.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:03.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:04.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:04.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:04.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:04.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:05.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:05.100","Descend","System Data (dBar %full Volts mAmps): ",2.3199999999999998,67.380388999999994,32.299999999999997,10,261.14625000000001,2436.27232,null,32.299999999999997,146.5,46.860734000000001,243.613801,null,null,null,null,null,null,null,null,null,1251.369995,12.63,39.112999000000002,12.63]
["$","2022-02-24","00:51:05.200","Descend","Pump motor not faulted"]
["$","2022-02-24","00:51:06.600","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:51:06.600","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:51:05.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,2.56]
["$","2022-02-24","00:51:05.200","Descend","SBE41 Message",2.56,67.380388999999994,32.15,155.5,null,null,null,null,null,null,null,null,2.56,2.56,1.189921,-4.2166000000000002E-2,-0.08,-8.1667000000000003E-2,-5.3439999999999998E-3,3000]
["$","2022-02-24","00:51:05.200","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:51:05.200","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:05.400","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:51:05.400","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:05.600","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:51:05.600","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:05.800","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:51:05.800","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:51:06","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:51:06","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:51:06.200","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:51:06.200","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:51:06.400","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:51:06.400","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:51:06.700","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:51:06.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:06.700","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:51:06.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:07.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:07.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:07.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:07.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","00:51:08.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:09.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:09.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:09.200","Descend","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:51:10.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:10.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:10.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:11","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,3.09]
["$","2022-02-24","00:51:11","Descend","SBE41 Message",3.09,67.385194999999996,32.15,155.5,null,null,null,null,null,null,null,null,3.09,3.09,1.4968490000000001,-5.5555E-2,-0.17666699999999999,-0.128333,-6.8360000000000001E-3,3000]
["$","2022-02-24","00:51:11.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:12.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:13.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:13.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:13.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:13.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:14.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:14.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,3.43]
["$","2022-02-24","00:51:14.200","Descend","SBE41 Message",3.43,67.373047,32.15,155.5,null,null,null,null,null,null,null,null,3.43,3.43,1.7842720000000001,-7.2261000000000006E-2,-0.113333,-0.14499999999999999,-8.5389999999999997E-3,3000]
["$","2022-02-24","00:51:15.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:16","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:16","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:16.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:16.100","Descend","System Data (dBar %full Volts mAmps): ",3.43,67.376509999999996,32.299999999999997,10,261.25117999999998,2526.3951889999998,null,32.325000000000003,143.5,48.500669000000002,252.61265700000001,null,null,null,null,null,null,null,null,null,1251.530029,12.64,38.758999000000003,12.64]
["$","2022-02-24","00:51:16.200","Descend","Pump motor not faulted"]
["$","2022-02-24","00:51:16.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:17.600","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:51:17.600","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:51:16.200","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:51:16.200","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:16.400","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:51:16.400","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:16.600","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:51:16.600","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:16.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:16.800","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:51:16.800","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:51:17","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:51:17","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:51:17","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,3.77]
["$","2022-02-24","00:51:17","Descend","SBE41 Message",3.77,67.376509999999996,32.15,155.5,null,null,null,null,null,null,null,null,3.77,3.77,2.060225,-8.7763999999999995E-2,-0.113333,-0.113333,-1.0416999999999999E-2,3000]
["$","2022-02-24","00:51:17.200","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:51:17.200","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:51:17.400","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:51:17.400","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:51:17.600","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:51:17.600","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:17.600","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:51:17.600","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:18","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:19","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:19.500","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:19.500","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:19.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:19.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:20","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,4.09]
["$","2022-02-24","00:51:20","Descend","SBE41 Message",4.09,67.377459999999999,32.15,155.5,null,null,null,null,null,null,null,null,4.09,4.09,2.3495210000000002,-9.7588999999999995E-2,-0.106667,-0.11,-1.2474000000000001E-2,3000]
["$","2022-02-24","00:51:20.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:21.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:22.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:22.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:22.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:22.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:23.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:23.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,4.4800000000000004]
["$","2022-02-24","00:51:23.200","Descend","SBE41 Message",4.4800000000000004,67.375208999999998,32.15,155.5,null,null,null,null,null,null,null,null,4.4800000000000004,4.4800000000000004,2.6757070000000001,-0.100634,-0.13,-0.11833299999999999,-1.4737E-2,3000]
["$","2022-02-24","00:51:24.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:25","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:25","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:25.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:25.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:25.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:26.100","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,4.71]
["$","2022-02-24","00:51:26.100","Descend","SBE41 Message",4.71,67.378809000000004,32.15,155.5,null,null,null,null,null,null,null,null,4.71,4.71,3.0375640000000002,-0.100412,-7.6666999999999999E-2,-0.10333299999999999,-1.7229999999999999E-2,3000]
["$","2022-02-24","00:51:26.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:26.100","Descend","System Data (dBar %full Volts mAmps): ",4.71,67.388374999999996,32.325000000000003,5,261.32725499999998,2608.4593810000001,null,32.325000000000003,146.5,49.966419999999999,260.83250700000002,null,null,null,null,null,null,null,null,null,1251.5600589999999,12.64,38.737000000000002,12.64]
["$","2022-02-24","00:51:26.200","Descend","Pump motor not faulted"]
["$","2022-02-24","00:51:27.600","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:51:27.600","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:51:26.200","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:51:26.200","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:26.400","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:51:26.400","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:26.600","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:51:26.600","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:26.800","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:51:26.800","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:51:27","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:51:27","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:51:27.200","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:51:27.200","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:51:27.400","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:51:27.400","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:51:27.700","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:51:27.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:27.700","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:51:27.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:28","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:28.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:28.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:28.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:29","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:29.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,5.05]
["$","2022-02-24","00:51:29.200","Descend","SBE41 Message",5.05,67.387358000000006,32.15,155.5,null,null,null,null,null,null,null,null,5.05,5.05,3.4069440000000002,-0.102191,-0.113333,-9.5000000000000001E-2,-1.993E-2,3000]
["$","2022-02-24","00:51:30","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:31","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:31","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:31","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:31.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:31.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:32","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:32","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,5.35]
["$","2022-02-24","00:51:32","Descend","SBE41 Message",5.35,67.383105,32.15,155.5,null,null,null,null,null,null,null,null,5.35,5.35,3.7616990000000001,-0.10806,-0.1,-0.106667,-2.2801999999999999E-2,3000]
["$","2022-02-24","00:51:33","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:34","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:34.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:34.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:34.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:35","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:35.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,5.71]
["$","2022-02-24","00:51:35.200","Descend","SBE41 Message",5.71,67.373375999999993,32.15,155.5,null,null,null,null,null,null,null,null,5.71,5.71,4.1002000000000001,-0.11565300000000001,-0.12,-0.11,-2.5808000000000001E-2,3000]
["$","2022-02-24","00:51:36","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:37","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:37","Descend","System Data (dBar %full Volts mAmps): ",5.71,67.383714999999995,32.325000000000003,5,261.41644600000001,2697.50776,null,32.325000000000003,146,51.55612,269.737345,null,null,null,null,null,null,null,null,null,1251.6099850000001,12.65,38.294998,12.65]
["$","2022-02-24","00:51:37.100","Descend","Pump motor not faulted"]
["$","2022-02-24","00:51:37.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:38.500","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:51:38.500","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:51:37","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:37","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:37.100","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:51:37.100","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:37.300","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:51:37.300","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:37.500","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:51:37.500","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:37.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:37.700","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:51:37.700","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:51:37.900","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:51:37.900","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:51:38","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,6.01]
["$","2022-02-24","00:51:38","Descend","SBE41 Message",6.01,67.383714999999995,32.15,155.5,null,null,null,null,null,null,null,null,6.01,6.01,4.4248830000000003,-0.121223,-0.1,-0.11,-2.8934999999999999E-2,3000]
["$","2022-02-24","00:51:38.100","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:51:38.100","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:51:38.300","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:51:38.300","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:51:38.500","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:51:38.500","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:38.500","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:51:38.500","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:39","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:40","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:40.400","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:40.400","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:40.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:40.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:41","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:41","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,6.37]
["$","2022-02-24","00:51:41","Descend","SBE41 Message",6.37,67.375658999999999,32.15,155.5,null,null,null,null,null,null,null,null,6.37,6.37,4.7383829999999998,-0.12248000000000001,-0.12,-0.11,-3.2152E-2,3000]
["$","2022-02-24","00:51:42","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:43","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:43.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:43.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:43.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:44","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:44.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,6.71]
["$","2022-02-24","00:51:44.200","Descend","SBE41 Message",6.71,67.373706999999996,32.15,155.5,null,null,null,null,null,null,null,null,6.71,6.71,5.0502370000000001,-0.119561,-0.113333,-0.11666700000000001,-3.5437000000000003E-2,3000]
["$","2022-02-24","00:51:45","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:46","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:46","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:46","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:46.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:46.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:47","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:47.100","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,7.07]
["$","2022-02-24","00:51:47.100","Descend","SBE41 Message",7.07,67.372551999999999,32.15,155.5,null,null,null,null,null,null,null,null,7.07,7.07,5.3694160000000002,-0.11482000000000001,-0.12,-0.11666700000000001,-3.8810999999999998E-2,3000]
["$","2022-02-24","00:51:48","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:48","Descend","System Data (dBar %full Volts mAmps): ",7.07,67.372733999999994,32.325000000000003,5,261.48465099999999,2787.6306300000001,null,32.325000000000003,143.5,53.162871000000003,278.74963200000002,null,null,null,null,null,null,null,null,null,1251.6099850000001,12.64,38.007998999999998,12.64]
["$","2022-02-24","00:51:48.100","Descend","Pump motor not faulted"]
["$","2022-02-24","00:51:49.500","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:51:49.500","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:51:48.100","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:51:48.100","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:48.300","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:51:48.300","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:48.500","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:51:48.500","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:48.700","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:51:49.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:48.700","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:51:48.900","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:51:48.900","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:51:49.100","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:51:49.100","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:51:49.300","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:51:49.300","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:51:49.500","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:51:49.500","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:49.500","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:51:49.500","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:49.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:49.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:49.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:50.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,7.41]
["$","2022-02-24","00:51:50.200","Descend","SBE41 Message",7.41,67.387585999999999,32.15,155.5,null,null,null,null,null,null,null,null,7.41,7.41,5.6967179999999997,-0.111002,-0.113333,-0.11666700000000001,-4.2254E-2,3000]
["$","2022-02-24","00:51:50.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:51.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:52","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:52","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:52.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:52.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:52.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:53.100","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,7.71]
["$","2022-02-24","00:51:53.100","Descend","SBE41 Message",7.71,67.365510999999998,32.15,155.5,null,null,null,null,null,null,null,null,7.71,7.71,6.0302579999999999,-0.109287,-0.1,-0.106667,-4.5766000000000001E-2,3000]
["$","2022-02-24","00:51:53.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:54.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:55.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:55.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:55.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:55.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:56.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,8.09]
["$","2022-02-24","00:51:56.200","Descend","SBE41 Message",8.09,67.377598000000006,32.15,155.5,null,null,null,null,null,null,null,null,8.09,8.09,6.3700890000000001,-0.109502,-0.126667,-0.113333,-4.9304000000000001E-2,3000]
["$","2022-02-24","00:51:56.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:57.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:58","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:58","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:58.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:58.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:58.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:59.400","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:59.800","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:52:03.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:52:08.800","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:10.500","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:52:11.800","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:16.800","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:22.300","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:52:22.400","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:52:25.700","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:31.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:52:32.400","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:52:34.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:52:38.600","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:42.900","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:52:44","Descend","SBE41 Message",13.63,67.387022000000002,32.15,155.5,null,null,null,null,null,null,null,null,13.63,13.63,11.873355,-0.11995500000000001,-0.106667,-0.11833299999999999,-0.100353,3000]
["$","2022-02-24","00:52:49.600","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:53.600","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:54.700","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:52:56.400","Descend","Checking Global Issues."]
["$","2022-02-24","00:53:02.200","Descend","SBE41 Message",15.82,67.378823999999994,32.15,155.5,null,null,null,null,null,null,null,null,15.82,15.82,14.010498999999999,-0.12194099999999999,-0.13,-0.123333,-0.110816,3000]
["$","2022-02-24","00:53:05","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:53:06","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:53:11","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,16.82]
["$","2022-02-24","00:53:16.900","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:53:16.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:53:19","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:53:25.400","Descend","Checking Global Issues."]
["$","2022-02-24","00:53:26.900","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:53:28.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:53:34.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:53:37.400","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:53:38.600","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:53:43.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:53:47.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:53:49.100","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:53:52","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:53:52","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:53:57.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:54:00.700","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:54:00.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:54:05","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,23.07]
["$","2022-02-24","00:54:11.500","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:54:11","Descend","SBE41 Message",23.879999000000002,67.360870000000006,32.15,155.5,null,null,null,null,null,null,null,null,23.88,23.879999000000002,22.038558999999999,-0.116342,-0.13666700000000001,-0.13500000000000001,-0.11776499999999999,3000]
["$","2022-02-24","00:54:14","Descend","Checking Global Issues."]
["$","2022-02-24","00:54:19.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:54:21.700","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:54:22.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:54:28.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:54:33.400","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:54:33.200","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:54:37.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:54:42.600","Descend","Descend glide on"]
["$","2022-02-24","00:54:42.800","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:54:44","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,27.89]
["$","2022-02-24","00:54:46.700","Descend","Checking Global Issues."]
["$","2022-02-24","00:54:52.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:54:54.200","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:54:55.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:55:01.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:55:06.100","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:55:05.900","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:55:10","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:55:15.500","Descend","Checking Global Issues."]
["$","2022-02-24","00:55:16.200","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:55:18.500","Descend","Checking Global Issues."]
["$","2022-02-24","00:55:25","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:55:26.600","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:55:28","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:55:32","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,34.020000000000003]
["$","2022-02-24","00:55:37.400","Descend","System Data (dBar %full Volts mAmps): ",34.290000999999997,67.378039999999999,32.35,5,263.18190499999997,4668.9287379999996,null,32.35,146,86.872904000000005,466.86601200000001,null,null,null,null,null,null,null,null,null,1251.290039,12.67,38.896000000000001,12.67]
["$","2022-02-24","00:55:38.300","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:55:41.100","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,35.14]
["$","2022-02-24","00:55:46.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:55:48.800","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:55:49.800","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:55:49.800","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:55:55.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:55:59.300","Descend","System Data (dBar %full Volts mAmps): ",37.25,67.378048000000007,32.35,10,263.33798999999999,4849.0401650000003,null,32.35,147.5,90.085224999999994,484.87715400000002,null,null,null,null,null,null,null,null,null,1251.339966,12.67,38.740001999999997,12.67]
["$","2022-02-24","00:56:00.900","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:56:04","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:56:08.300","Descend","Checking Global Issues."]
["$","2022-02-24","00:56:10.800","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:56:12.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:56:18.300","Descend","Checking Global Issues."]
["$","2022-02-24","00:56:21.400","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:56:22.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:56:26","Descend","SBE41 Message",40.720001000000003,67.372715999999997,32.15,155.5,null,null,null,null,null,null,null,null,40.72,40.720001000000003,38.803722,-0.13111999999999999,-0.12,-0.12,-0.12635399999999999,3000]
["$","2022-02-24","00:56:31.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:56:32.800","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:56:35.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,41.93]
["$","2022-02-24","00:56:40.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:56:43.600","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:56:44.500","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:56:49.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:56:54","Descend","System Data (dBar %full Volts mAmps): ",44.110000999999997,67.370616999999996,32.35,10,263.72229800000002,5297.1025970000001,null,32.35,144,98.075959999999995,529.69682899999998,null,null,null,null,null,null,null,null,null,1251.3100589999999,12.65,38.728999999999999,12.65]
["$","2022-02-24","00:56:55.100","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:56:58","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:57:02.300","Descend","Normal State Exit"]
["$","2022-02-24","00:57:02.300","Anchor","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:57:02.400","Anchor","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:57:12.400","Anchor","[MSC] RX: "]
["$","2022-02-24","00:57:12.700","Anchor","[MSC] RX:   "]
["$","2022-02-24","00:57:13","Anchor","[MSC] RX:   Last Error     Time = Thu Jan  1 00:00:00 1970  "]
["$","2022-02-24","00:57:13.200","Anchor","[MSC] RX:   "]
["$","2022-02-24","00:57:13.300","Anchor","Optode: Disable text"]
["$","2022-02-24","00:57:15.200","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Last Calibration,4330,2707,2016-08-22  "]
["$","2022-02-24","00:57:16","Anchor","Sending Optode Get DataXML"]
["$","2022-02-24","00:57:18.100","Anchor","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S/N: 0545 "]
["$","2022-02-24","00:57:16.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:57:17.200","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output,4330,2707,O2Concentration  "]
["$","2022-02-24","00:57:17.700","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Geographic Position,4330,2707,60.323605,5.37225  "]
["$","2022-02-24","00:57:17.700","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","00:57:19.300","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"0\" Descr=\"System Control\" Type=\"VT_ARRAY|VT_I2\" Access=\"R3W4\">0;0;0</Property>  "]
["$","2022-02-24","00:57:20.200","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,</PropertyCategory>  "]
["$","2022-02-24","00:57:21.800","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"3\" Descr=\"PhaseCoef\" Type=\"VT_ARRAY|VT_R4\" Access=\"R1W3\">6.919999E-01;1.000000E+00;0.000000E+00;0.000000E+00</Property>  "]
["$","2022-02-24","00:57:21.800","Anchor","Checking Global Issues."]
["$","2022-02-24","00:57:23.800","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,<PropertyCategory ID=\"5\" Descr=\"Sample Settings\">  "]
["$","2022-02-24","00:57:24.900","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,</PropertyCategory>  "]
["$","2022-02-24","00:57:26.900","Anchor","Pump motor not faulted"]
["$","2022-02-24","00:57:27","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,</PropertyCategory>  "]
["$","2022-02-24","00:57:27.700","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:57:28.200","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,<Point ID=\"3\" Descr=\"Temperature\" Type=\"VT_R4\" Unit=\"Deg.C\" Format=\"%0.3f\" RangeMin=\"-5\" RangeMax=\"40\" />  "]
["$","2022-02-24","00:57:29.700","Anchor","Checking Global Issues."]
["$","2022-02-24","00:57:38","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:57:42.600","Anchor","Checking Global Issues."]
["$","2022-02-24","00:57:48.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:57:50.100","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:58:00.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","00:58:01","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:58:02.400","Anchor","Sending FLBB run command"]
["$","2022-02-24","00:58:07.900","Anchor","FLBB post: /99/99,99:99:99,695,105,700,1828,551  "]
["$","2022-02-24","00:58:10.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:58:11.200","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:58:15.200","Anchor","[MSC] TX: W"]
["$","2022-02-24","00:58:21.500","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:58:22.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:58:29.600","Anchor","[MSC] RX: 0x7A29,pH,02/24/2022 00:58:28,1645664287,44.81,10.6715,33.6818,46,6,0,13.15,38.69,11.672,4.580e-02,7.1234,3.550,-0.964262,0.000016,-0.920896,0.000017,+9.440e-10,+4.883e-11  "]
["$","2022-02-24","00:58:32.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:58:33.200","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:58:43.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:58:44.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:58:55.400","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","00:58:55.400","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:59:06.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","00:59:05.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:59:15.500","Anchor","Checking Global Issues."]
["$","2022-02-24","00:59:16.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:59:25.400","Anchor","Checking Global Issues."]
["$","2022-02-24","00:59:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:59:35.200","Anchor","Checking Global Issues."]
["$","2022-02-24","00:59:38.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:59:38.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:59:48.800","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:59:52.900","Anchor","Checking Global Issues."]
["$","2022-02-24","00:59:53.900","Anchor","Checking Global Issues."]
["$","2022-02-24","00:59:59.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:00:02.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:00:10.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:00:11.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:00:20.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:00:22.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:00:31.600","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:00:33","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:00:43.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:00:49.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:00:53.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:00:54.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:01:04","Anchor","System Data (dBar %full Volts mAmps): ",44.810001,67.371196999999995,32.35,5,265.55202700000001,7348.0358530000003,null,32.35,167,140.71572499999999,734.77672299999995,null,null,null,null,null,null,null,null,null,1251.150024,12.58,38.521999000000001,12.58]
["$","2022-02-24","01:01:05.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:01:13.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:01:16","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:01:25.800","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:01:26.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:01:32.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:01:37.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:01:42.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:01:47.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:01:56.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:01:58.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:02:00.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:02:09.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:02:10.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:02:20.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:02:21.600","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:02:27.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:02:32.400","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:02:41.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:02:43","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:02:52.600","Anchor","System Data (dBar %full Volts mAmps): ",44.810001,67.373515999999995,32.35,10,266.35605800000002,8238.6539539999994,null,32.35,166.5,158.82190900000001,823.83853299999998,null,null,null,null,null,null,null,null,null,1250.9399410000001,12.55,38.495998,12.55]
["$","2022-02-24","01:02:53.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:03:02.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:04","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:03:11.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:12.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:15.200","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:03:21.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:25.900","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:03:37.500","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:03:36.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:03:39.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:47.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:03:49.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:58","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:03:59.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:04:08.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:04:10.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:04:21","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:04:21.100","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:04:30.500","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:04:31.700","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:04:36.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:04:42.300","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:04:51.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:04:53","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:05:00.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:05:03.800","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:05:09.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:05:14.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:05:18.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:05:25.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:05:28.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:05:35.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:05:38.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:05:46.700","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:05:47.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:05:57.300","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:05:58.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:06:09.600","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:06:09.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:06:19","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:06:19.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:06:29.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:06:30.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:06:30.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:06:39.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:06:41.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:06:49.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:06:53.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:06:58.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:07:03","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:07:08.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:07:13.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:07:17","Anchor","Checking Global Issues."]
["$","2022-02-24","01:07:24.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:07:25.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:07:35","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:07:36.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:07:45.800","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:07:47.300","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:07:58.100","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:07:57.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:08:02.400","Anchor","Sci Logger sending sample FLBB"]
["$","2022-02-24","01:08:06.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:08:08.400","Anchor","[MSC] Starting ISUS Sample"]
["$","2022-02-24","01:08:07.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:08:14.400","Anchor","[MSC] TX: W"]
["$","2022-02-24","01:08:17.400","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:08:19.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:08:27.400","Anchor","[MSC] RX: 0xCACD,pH,02/24/2022 01:08:26,1645664888,44.58,10.6336,33.6886,47,6,0,12.83,39.07,11.672,4.580e-02,7.1234,3.550,-0.965220,0.000018,-0.920814,0.000008,+4.875e-09,-4.395e-09  "]
["$","2022-02-24","01:08:28.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:08:31.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:08:38.900","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:08:41.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:08:50.800","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:08:50.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:09:00.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:09:01.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:09:12.500","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:09:12.500","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:09:23.300","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:09:22.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:09:32.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:09:32.700","Anchor","System Data (dBar %full Volts mAmps): ",44.580002,67.365713999999997,32.325000000000003,5,269.00293499999998,11519.3413,null,32.35,166,226.46377200000001,1151.893836,null,null,null,null,null,null,null,null,null,1250.599976,12.43,38.375999,12.43]
["$","2022-02-24","01:09:33.800","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:09:43.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:09:44.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:09:52.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:09:55.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:10:01.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:10:06","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:10:11.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:10:16.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:10:21","Anchor","Checking Global Issues."]
["$","2022-02-24","01:10:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:10:28.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:10:38.100","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:10:39.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:10:48.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:10:50.200","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:11:01","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:11:01","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:11:10.500","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:11:11.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:11:21.200","Anchor","System Data (dBar %full Volts mAmps): ",44.580002,67.366134000000002,32.325000000000003,5,269.81877100000003,12409.42215,null,32.325000000000003,166,244.56903700000001,1240.9153530000001,null,null,null,null,null,null,null,null,null,1250.48999,12.43,38.175998999999997,12.43]
["$","2022-02-24","01:11:22.300","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:11:32.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:11:33.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:11:40.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:11:43.800","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:11:49.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:11:54.500","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:11:59.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:12:05.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:12:10.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:12:15.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:12:17.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:12:26.600","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:12:27.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:12:37.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:12:38.700","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:12:38.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:12:49.500","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:12:49.500","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:12:59","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:13:00.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:13:09.800","Anchor","System Data (dBar %full Volts mAmps): ",44.580002,67.356382999999994,32.325000000000003,5,270.68969600000003,13299.50301,null,32.325000000000003,166.5,262.63587200000001,1329.9234389999999,null,null,null,null,null,null,null,null,null,1250.410034,12.41,37.985999999999997,12.41]
["$","2022-02-24","01:13:11.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:13:19.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:13:21.500","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:13:29.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:13:32.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:13:38.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:13:43","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:13:49.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:13:53.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:13:57","Anchor","Checking Global Issues."]
["$","2022-02-24","01:14:04.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:14:06.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:14:15.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:14:16.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:14:26.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:14:27.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:14:38.100","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:14:38.100","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:14:47.500","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:14:48.700","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:14:58.400","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:14:59.400","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:15:08.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:10","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:15:18","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:20.900","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:15:27.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:30.800","Anchor","System Data (dBar %full Volts mAmps): ",44.580002,67.356983,32.325000000000003,10,271.731133,14456.326069999999,null,32.325000000000003,168,286.11726099999998,1445.592314,null,null,null,null,null,null,null,null,null,1250.380005,12.38,38.150002000000001,12.38]
["$","2022-02-24","01:15:35.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:42.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:15:45.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:52.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:15:55.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:57.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:16:03.700","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:16:04.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:16:14.300","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:16:15.800","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:16:26.600","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:16:26.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:16:36.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:16:37.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:16:46.800","Anchor","System Data (dBar %full Volts mAmps): ",44.580002,67.351833999999997,32.325000000000003,10,272.469583,15079.530409999999,null,32.325000000000003,166.5,298.84732100000002,1507.912748,null,null,null,null,null,null,null,null,null,1250.3000489999999,12.36,38.548000000000002,12.36]
["$","2022-02-24","01:16:47.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:16:56.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:16:58.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:17:06.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:17:10","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:17:15.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:17:20","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:17:25.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:17:30.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:17:34","Anchor","Checking Global Issues."]
["$","2022-02-24","01:17:41.900","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:17:42.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:17:52.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:17:53.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:18:02.400","Anchor","Sending Optode Do Sample"]
["$","2022-02-24","01:18:03","Anchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>pts  "]
["$","2022-02-24","01:18:03.800","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:18:05.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:18:12.900","Anchor","[MSC] TX: W"]
["$","2022-02-24","01:18:13.800","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:18:19.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:18:25.300","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:18:25.100","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:18:30.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:18:34.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:18:39.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:18:46.100","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:18:48.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:18:56.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:18:58.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:19:02.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:19:07.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:19:08.800","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:19:18.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:19:19.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:19:30.500","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:19:30.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:19:40.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:19:41.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:19:50.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:19:51.800","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:20:00.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:20:02.500","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:20:12.400","Anchor","System Data (dBar %full Volts mAmps): ",44.689999,67.350544999999997,32.325000000000003,10,274.446214,16766.077160000001,null,32.325000000000003,166,334.01956300000001,1676.567423,null,null,null,null,null,null,null,null,null,1250.170044,12.33,38.035998999999997,12.33]
["$","2022-02-24","01:20:13.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:20:18.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:20:24","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:20:28.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:20:34.600","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:20:38","Anchor","Checking Global Issues."]
["$","2022-02-24","01:20:45.900","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:20:46.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:20:56","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:20:57.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:21:06.800","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:21:08.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:21:19.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:21:18.500","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:21:28.400","Anchor","System Data (dBar %full Volts mAmps): ",44.689999,67.366877000000002,32.325000000000003,5,275.17679399999997,17389.012879999998,null,32.325000000000003,164,346.70568300000002,1738.860995,null,null,null,null,null,null,null,null,null,1250.089966,12.32,38.841000000000001,12.32]
["$","2022-02-24","01:21:29.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:21:39.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:21:40.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:21:49.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:21:50.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:21:57","Anchor","Checking Global Issues."]
["$","2022-02-24","01:22:01.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:22:06.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:22:12.500","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:22:16.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:22:23.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:22:24.200","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:22:25.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:22:33.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:22:35.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:22:44.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:22:45.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:22:55.300","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:23:02.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:23:07.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:23:07.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:23:17","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:23:18.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:23:27.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:23:28.500","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:23:36.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:23:39.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:23:46.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:23:50.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:23:56.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:24:01.100","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:24:01.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:24:11.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:24:14.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:24:22.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:24:23.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:24:33","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:24:34.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:24:45.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:24:45.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:24:56.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:24:56","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:25:05.600","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:25:06.800","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:25:10.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:25:17.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:25:25.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:25:28.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:25:35","Anchor","Checking Global Issues."]
["$","2022-02-24","01:25:38.800","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:25:39","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:25:49.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:25:49.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:25:53.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:26:00.300","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:26:03.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:26:10.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:26:21.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:26:21.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:26:23","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:26:33.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:26:33.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:26:44.700","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:26:44.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:26:53","Anchor","Checking Global Issues."]
["$","2022-02-24","01:26:55.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:27:04.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:06","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:27:14.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:16.600","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:27:23.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:27:32.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:37.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:27:42.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:48.800","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:27:52.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:59.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:28:00.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:28:04.500","Anchor","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",2.8400000000000002E-2,2.4299999999999999E-2,1.26E-2,0.22950000000000001]
["$","2022-02-24","01:28:08.100","Anchor","SciLogger: Setting get PH true"]
["$","2022-02-24","01:28:11.500","Anchor","[MSC] Timeout for CommandWake"]
["$","2022-02-24","01:28:11.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:28:17.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:28:22.500","Anchor","[MSC] Data: 0x505F,A,02/24/2022 01:28:20,1645666088,44.73,10.5894,33.6976,49,6,0,0,12.76,38.93,11.500,5.662e-01,18412.00,1126.00,1016.52,5.39,33.70,29.29,7.639e-04,36,77,288B2D58312233DA3588366636A9368B3636360535DD361636B1379839003AE83D5640344389475E4B8D501754B359585DCF61C5651E678068CC68EF67CC658D62715EA35A66562251D04DBA4A1646C143C54143,1030.6  "]
["$","2022-02-24","01:28:22.800","Anchor","[MSC] Done Sampling."]
["$","2022-02-24","01:28:29.300","Anchor","[MSC] Post pH: -0.965494"]
["$","2022-02-24","01:28:32.500","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:28:37.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:28:38.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:28:44.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:28:46.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:28:54","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:28:56.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:29:04.700","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:29:06.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:29:15.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:29:16.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:29:27.600","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:29:27.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:29:38.400","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:29:38.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:29:47.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:29:49.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:29:57.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:29:59.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:30:07.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:30:10.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:30:17.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:30:21","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:30:27.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:30:31.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:30:35","Anchor","Checking Global Issues."]
["$","2022-02-24","01:30:42.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:30:44.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:30:53.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:30:54.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:31:03.800","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:31:05.200","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:31:16.100","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:31:16.100","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:31:26.900","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:31:26.700","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:31:36.400","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:31:37.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:31:46.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:31:48.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:31:56","Anchor","Checking Global Issues."]
["$","2022-02-24","01:31:58.900","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:31:58.900","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:32:05.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:32:09.500","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:32:14.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:32:20.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:32:24.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:32:31","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:32:33.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:32:41.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:32:42.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:32:52.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:32:53.800","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:33:04.600","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:33:04.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:33:15.400","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:33:15.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:33:24.800","Anchor","System Data (dBar %full Volts mAmps): ",44.73,67.361643000000001,32.299999999999997,10,281.18276500000002,23264.19123,null,32.299999999999997,166.5,466.77642700000001,2326.3653989999998,null,null,null,null,null,null,null,null,null,1249.8000489999999,12.24,38.305,12.24]
["$","2022-02-24","01:33:25.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:33:35.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:33:36.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:33:44.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:33:47.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:33:53.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:33:58","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:34:03.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:34:08.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:34:13","Anchor","Checking Global Issues."]
["$","2022-02-24","01:34:19.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:34:20.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:34:30.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:34:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:34:40.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:34:42.300","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:34:53.100","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:34:51.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:35:02.500","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:35:03.800","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:35:13.300","Anchor","System Data (dBar %full Volts mAmps): ",44.73,67.356258999999994,32.299999999999997,5,282.00253600000002,24154.00347,null,32.299999999999997,167,484.782533,2415.346622,null,null,null,null,null,null,null,null,null,1249.670044,12.24,38.158999999999999,12.24]
["$","2022-02-24","01:35:14.400","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:35:14.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:35:24.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:35:25.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:35:33","Anchor","Checking Global Issues."]
["$","2022-02-24","01:35:35.900","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:35:42.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:35:46.600","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:35:51.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:35:57.400","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:36:05.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:36:08.100","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:36:10.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:36:18.700","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:36:20.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:36:29.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:36:31.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:36:41.600","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:36:41.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:36:52.500","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:36:52.300","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:37:01.800","Anchor","System Data (dBar %full Volts mAmps): ",44.73,67.362954000000002,32.299999999999997,5,282.81181400000003,25044.084320000002,null,32.299999999999997,165,502.87599399999999,2504.3547079999998,null,null,null,null,null,null,null,null,null,1249.6099850000001,12.22,38.789000999999999,12.22]
["$","2022-02-24","01:37:03.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:37:14.200","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:37:13.600","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:37:21.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:37:24.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:37:31.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:37:35.100","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:37:42.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:37:45.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:37:49.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:37:56.600","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:37:58.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:38:02.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:38:08.500","Anchor","FLBB Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"/99/99,99:99:99,695,92,700,1352,546  "]
["$","2022-02-24","01:38:08.600","Anchor","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","01:38:08.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:38:16","Anchor","Checking Global Issues."]
["$","2022-02-24","01:38:17.900","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:38:18.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:38:21.300","Anchor","[MSC] Starting pH sample"]
["$","2022-02-24","01:38:27.900","Anchor","[MSC] Done Sampling."]
["$","2022-02-24","01:38:29.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:38:35.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:38:39.700","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:38:45.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:38:50.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:38:55.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:39:01.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:39:03.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:39:11.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:39:13.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:39:22.500","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:39:23.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:39:33.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:39:39.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:39:45.400","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:39:45.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:39:54.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:39:56","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:40:05.600","Anchor","System Data (dBar %full Volts mAmps): ",44.75,67.353831,32.299999999999997,10,284.031633,26550.788270000001,null,32.299999999999997,166.5,534.37723600000004,2655.0251020000001,null,null,null,null,null,null,null,null,null,1249.5600589999999,12.21,38.112999000000002,12.21]
["$","2022-02-24","01:40:06.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:40:07.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:40:17.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:40:24.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:40:28.200","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:40:34.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:40:38.800","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:40:39.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:40:49.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:40:51.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:41:00.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:41:01.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:41:11","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:41:12.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:41:18.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:41:23.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:41:33.900","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:41:33.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:41:33.900","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:41:43.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:41:48.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:41:54.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:41:55.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:42:03.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:42:05.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:42:13.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:42:16.700","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:42:28.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:42:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:42:31.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:42:38","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:42:41.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:42:48.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:42:51.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:42:59.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:43:00.700","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:43:10.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:43:11.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:43:22.400","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:43:22.400","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:43:26.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:43:33","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:43:42.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:43:43.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:43:52.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:43:54.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:44:02.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:44:04.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:44:10.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:44:15.800","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:44:20","Anchor","Checking Global Issues."]
["$","2022-02-24","01:44:26.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:44:29.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:44:36.800","Anchor","System Data (dBar %full Volts mAmps): ",44.75,67.356791999999999,32.299999999999997,10,286.10794900000002,28775.52032,null,32.299999999999997,166.5,579.47578999999996,2877.4983080000002,null,null,null,null,null,null,null,null,null,1249.4799800000001,12.2,38.144001000000003,12.2]
["$","2022-02-24","01:44:38.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:44:47.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:44:49.200","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:44:49.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:44:58.600","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:45:00.100","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:45:10.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:45:10.700","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:45:20.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:45:21.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:45:31.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:45:32.200","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:45:40.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:45:42.800","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:45:49.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:45:53.500","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:45:59.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:46:04.400","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:46:09.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:46:14.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:46:17.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:46:25.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:46:27.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:46:36.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:46:37.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:46:47.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:46:48.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:46:59.400","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:46:59.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:47:08.900","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:47:10.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:47:19.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:47:20.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:47:26.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:47:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:47:38.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:47:42","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:47:48.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:47:52.900","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:47:56","Anchor","Checking Global Issues."]
["$","2022-02-24","01:48:02.500","Anchor","Sci Logger sending sample Radiometer"]
["$","2022-02-24","01:48:03.300","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","01:48:03.300","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:48:04.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:48:06.800","Anchor","SBE41 Message",44.619999,67.348641000000001,32.15,155.5,null,null,null,null,null,null,null,null,"   44.62, 10.5763, 33.6997  ",44.619999,44.703921000000001,-0.105334,4.3333999999999998E-2,1.8332999999999999E-2,-3.326E-3,3000]
["$","2022-02-24","01:48:14.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:48:20.900","Anchor","[MSC] RX: 0x7C3B,A,02/24/2022 01:48:21,1645667286,44.62,10.5763,33.6997,51,6,0,0,12.72,38.96,11.500,5.678e-01,18220.00,1123.00,1014.69,4.93,33.70,29.40,7.825e-04,36,77,27A22C61301B32D7347E35573598357B352434F534EC351435A2369337FB39DD3C353EFF425B461D4A484EB6534A57E45C4C602E638265E467296748663663EE60F35D2558F254B150724C6E48D645824296401F,915.2  "]
["$","2022-02-24","01:48:21","Anchor","[MSC] Done Sampling."]
["$","2022-02-24","01:48:24.300","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:48:25.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:48:34.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:48:36","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:48:43.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:48:46.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:48:52.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:48:57.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:49:02.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:49:07.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:49:12.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:49:18.600","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:49:21.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:49:29.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:49:30.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:49:40.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:49:41.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:49:52.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:49:52.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:50:01.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:50:03","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:50:12.500","Anchor","System Data (dBar %full Volts mAmps): ",44.619999,67.364789999999999,32.274999999999999,5,288.55808000000002,31528.498640000002,null,32.274999999999999,167,636.30126600000006,3152.7827080000002,null,null,null,null,null,null,null,null,null,1249.369995,12.18,37.811999999999998,12.18]
["$","2022-02-24","01:50:13.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:50:23.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:50:24.300","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:50:32.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:50:35.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:50:41.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:50:45.800","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:50:50.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:50:56.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:50:56.600","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:51:07.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:51:07.300","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:51:09.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:51:17.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:51:19.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:51:28.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:51:30","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:51:40.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:51:40.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:51:51.700","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:51:51.500","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:52:01","Anchor","System Data (dBar %full Volts mAmps): ",44.619999,67.363602,32.274999999999999,5,289.37522799999999,32418.310870000001,null,32.274999999999999,166.5,654.40023599999995,3241.7639319999998,null,null,null,null,null,null,null,null,null,1249.290039,12.19,38.652999999999999,12.19]
["$","2022-02-24","01:52:02.300","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:52:10.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:52:13","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:52:20.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:52:23.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:52:30.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:52:34.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:52:39.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:52:44.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:52:48.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:52:55.800","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:52:58.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:53:06.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:53:09","Anchor","Checking Global Issues."]
["$","2022-02-24","01:53:17.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:53:18.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:53:29.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:53:29.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:53:40.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:53:40","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:53:49.600","Anchor","System Data (dBar %full Volts mAmps): ",44.619999,67.350908000000004,32.274999999999999,5,290.19237600000002,33308.794670000003,null,32.274999999999999,166.5,672.42641000000003,3330.7988799999998,null,null,null,null,null,null,null,null,null,1249.290039,12.19,38.453999000000003,12.19]
["$","2022-02-24","01:53:50.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:53:59.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:01.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:54:09.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:12.200","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:54:19.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:22.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:27","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:28","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:33.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:54:37.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:44.300","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:54:47.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:55","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:54:56.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:55:05.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:55:07.100","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:55:17.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:55:17.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:55:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:55:28.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:55:38.100","Anchor","System Data (dBar %full Volts mAmps): ",44.619999,67.356902000000005,32.274999999999999,5,290.974109,34198.606899999999,null,32.274999999999999,167.5,690.43723799999998,3419.7801030000001,null,null,null,null,null,null,null,null,null,1249.209961,12.17,37.945,12.17]
["$","2022-02-24","01:55:39.200","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:55:49","Anchor","Checking Global Issues."]
["$","2022-02-24","01:55:50.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:55:57.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:56:01.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:56:06.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:56:11.400","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:56:16.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:56:22","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:56:26.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:56:33.100","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:56:34.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:56:43.500","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:56:44.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:56:54.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:56:55.600","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:57:06.400","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:57:05.600","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:57:15.900","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:57:17.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:57:26.600","Anchor","System Data (dBar %full Volts mAmps): ",44.619999,67.352304000000004,32.274999999999999,10,291.77420599999999,35088.687760000001,null,32.274999999999999,166,708.54289700000004,3508.8016200000002,null,null,null,null,null,null,null,null,null,1249.290039,12.17,38.165999999999997,12.17]
["$","2022-02-24","01:57:27.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:57:37.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:57:39","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:57:45.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:57:46.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:57:49.200","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:57:56.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:57:59.900","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:58:02.400","Anchor","Sci Logger sending PTS to CTD"]
["$","2022-02-24","01:58:08","Anchor","FLBB post: /99/99,99:99:99,695,77,700,1351,546  "]
["$","2022-02-24","01:58:08.200","Anchor","[MSC] Starting ISUS Sample"]
["$","2022-02-24","01:58:09.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:58:11.300","Anchor","[MSC] RX: "]
["$","2022-02-24","01:58:20.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:58:21.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:58:24","Anchor","Checking Global Issues."]
["$","2022-02-24","01:58:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:58:32.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:58:41.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:58:43","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:58:51.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:58:53.700","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:59:05.100","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:59:04.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:59:09.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:59:15.200","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:59:19.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:59:25.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:59:29.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:59:35.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:59:38","Anchor","Checking Global Issues."]
["$","2022-02-24","01:59:47.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:59:48.600","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:59:58","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:59:59.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:00:10.200","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:00:09.400","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:00:19.600","Anchor","System Data (dBar %full Volts mAmps): ",44.759998000000003,67.349097,32.274999999999999,10,293.08846299999999,36507.149189999996,null,32.274999999999999,167,738.26634999999999,3650.6343320000001,null,null,null,null,null,null,null,null,null,1249.1800539999999,12.16,39.987999000000002,12.16]
["$","2022-02-24","02:00:20.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:00:30.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:00:31.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:00:40.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:00:41.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:00:42.200","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:00:49.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:00:52.900","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:00:59","Anchor","Checking Global Issues."]
["$","2022-02-24","02:01:03.700","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:01:08.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:01:15.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:01:16.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:01:25","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:01:26.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:01:35.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:01:37.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:01:47.100","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:01:47.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:01:58.800","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:01:58.600","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:02:08.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:02:09.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:02:19","Anchor","System Data (dBar %full Volts mAmps): ",44.759998000000003,67.363221999999993,32.274999999999999,5,293.98168500000003,37486.278429999998,null,32.274999999999999,167,758.17432499999995,3748.5472559999998,null,null,null,null,null,null,null,null,null,1249.130005,12.17,38.441001999999997,12.17]
["$","2022-02-24","02:02:19.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:02:27.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:02:30.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:02:37.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:02:41.400","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:02:47.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:02:52.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:02:53.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:03:02.900","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:03:05.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:03:13.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:03:15.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:03:24.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:03:25.200","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:03:36.500","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:03:36.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:03:47.300","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:03:47.100","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:03:56.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:03:58","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:04:04.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:04:07.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:04:08.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:04:17.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:04:19.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:04:26.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:04:30.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:04:40.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:04:40.700","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:04:44.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:04:51.400","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:04:54.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:05:02","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:05:03.300","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:05:12.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:05:14.100","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:05:23.600","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:05:25","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:05:35.800","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:05:35.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:05:43.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:05:46.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:05:56","Anchor","Checking Global Issues."]
["$","2022-02-24","02:05:57.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:06:05.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:06:07.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:06:08.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:06:18.400","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:06:23.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:06:29.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:06:33.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:06:39.900","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:06:43.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:06:51.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:06:52.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:07:01.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:07:02.700","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:07:12.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:07:13.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:07:24.300","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:07:24.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:07:24.100","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:07:33.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:07:35","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:07:44.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:07:45.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:07:55.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:07:56.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:08:01.400","Anchor","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","02:08:04.600","Anchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","02:08:06.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:08:07","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:08:11.100","Anchor","[MSC] TX: W"]
["$","2022-02-24","02:08:17.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:08:17.900","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:08:22.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:08:28.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:08:28.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:08:39.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:08:39.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:08:47.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:08:50.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:08:58.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:00.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:09:08.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:11.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:09:17.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:22.200","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:09:27.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:32.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:09:36.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:43.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:09:46.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:54.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:09:55.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:10:05","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:10:06.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:10:17.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:10:17.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:10:17.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:10:26.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:10:27.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:10:37.500","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.350326999999993,32.25,10,297.40504900000002,41574.310879999997,null,32.274999999999999,167,842.03296399999999,4157.3505009999999,null,null,null,null,null,null,null,null,null,1248.959961,12.15,38.694000000000003,12.15]
["$","2022-02-24","02:10:38.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:10:48.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:10:49.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:10:56.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:11:00.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:11:06","Anchor","Checking Global Issues."]
["$","2022-02-24","02:11:10.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:11:15.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:11:21.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:11:25.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:11:32.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:11:33.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:11:42.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:11:44.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:11:53.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:11:54.900","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:12:05.800","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:12:05.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:12:15.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:12:16.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:12:26","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.360930999999994,32.25,10,298.16842000000003,42464.12311,null,32.274999999999999,165,860.13586799999996,4246.3182930000003,null,null,null,null,null,null,null,null,null,1248.98999,12.15,38.782001000000001,12.15]
["$","2022-02-24","02:12:27.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:12:36.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:12:37.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:12:44.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:12:48.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:12:54.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:12:59.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:13:04.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:13:09.900","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:13:13.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:13:20.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:13:22.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:13:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:13:32.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:13:32.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:13:42.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:13:43.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:13:54.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:13:54.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:14:05.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:14:04.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:14:14.500","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.347303999999994,32.25,10,298.899,43353.935340000004,null,32.25,167,878.15391,4335.299516,null,null,null,null,null,null,null,null,null,1248.98999,12.15,38.847999999999999,12.15]
["$","2022-02-24","02:14:16","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:14:24.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:14:26.200","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:14:34.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:14:37.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:14:44","Anchor","Checking Global Issues."]
["$","2022-02-24","02:14:47.900","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:14:51.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:14:58.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:15:01.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:15:09","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:15:11.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:15:19.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:15:25.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:15:30.500","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:15:31.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:15:42.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:15:42.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:15:53.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:15:53.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:16:04.500","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:16:04.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:16:12.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:16:14.700","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:16:22.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:16:25.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:16:26.200","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:16:36.200","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:16:40.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:16:46.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:16:50.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:16:51.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:16:57.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:17:04.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:17:08.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:17:09.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:17:19","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:17:20.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:17:31.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:17:33.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:17:40.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:17:42","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:17:51.500","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.361530000000002,32.25,10,300.32343400000002,45133.828439999997,null,32.25,166.5,914.28403800000001,4513.288826,null,null,null,null,null,null,null,null,null,1248.910034,12.14,38.758999000000003,12.14]
["$","2022-02-24","02:17:52.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:18:01.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:18:04","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:18:03.400","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:18:06.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:18:09.900","Anchor","[MSC] Timeout for CommandWake"]
["$","2022-02-24","02:18:13","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:18:14.600","Anchor","[MSC] RX: ACK  "]
["$","2022-02-24","02:18:21.300","Anchor","[MSC] TX: T2,1645669086,10.5828,33.6989,44.7000"]
["$","2022-02-24","02:18:24.300","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:18:24.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:18:35.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:18:35.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:18:46.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:18:46.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:18:56","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:18:56.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:19:06.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:19:07.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:19:15.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:19:18.500","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:19:25.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:19:29.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:19:30","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:19:39.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:19:44.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:19:50.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:19:53","Anchor","Checking Global Issues."]
["$","2022-02-24","02:19:54","Anchor","Checking Global Issues."]
["$","2022-02-24","02:20:01.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:20:11.900","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.355819999999994,32.25,10,301.38323400000002,46285.279040000001,null,32.25,166.5,938.64120500000001,4628.4338859999998,null,null,null,null,null,null,null,null,null,1248.910034,12.15,37.941001999999997,12.15]
["$","2022-02-24","02:20:12","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:20:13.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:20:22.800","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:20:24.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:20:35.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:20:38.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:20:44.400","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.353274999999996,32.25,5,301.61539299999998,46552.155559999999,null,32.25,166.5,944.04789000000005,4655.1349689999997,null,null,null,null,null,null,null,null,null,1248.910034,12.13,37.752997999999998,12.13]
["$","2022-02-24","02:20:45.800","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:20:55.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:20:56.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:21:05.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:21:07.100","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:21:10","Anchor","Checking Global Issues."]
["$","2022-02-24","02:21:17.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:21:22.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:21:28.500","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:21:32.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:21:39.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:21:40","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:21:49.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:21:51.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:22:00.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:22:01.900","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:22:11.300","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:22:12.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:22:17.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:22:23.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:22:33","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.353628999999998,32.25,5,302.33154500000001,47442.102099999996,null,32.25,168,962.16023800000005,4744.1161929999998,null,null,null,null,null,null,null,null,null,1248.8599850000001,12.14,38.394001000000003,12.14]
["$","2022-02-24","02:22:34.300","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:22:43.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:22:44.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:22:53.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:22:55","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:23:02.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:23:06.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:23:11.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:23:12.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:23:17.100","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:23:27.200","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.344561999999996,32.25,10,302.70273700000001,47886.941070000001,null,32.25,165.5,971.17116099999998,4788.6000889999996,null,null,null,null,null,null,null,null,null,1248.910034,12.14,38.097000000000001,12.14]
["$","2022-02-24","02:23:27.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:23:30","Anchor","Checking Global Issues."]
["$","2022-02-24","02:23:38.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:23:39.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:23:49","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:23:50.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:24:00.700","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:24:01.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:24:12.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:24:11.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:24:21.600","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:24:22.800","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:24:32.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:24:33.200","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:24:41.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:24:44.100","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:24:51","Anchor","Checking Global Issues."]
["$","2022-02-24","02:24:54.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:25:00.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:25:05","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:25:08.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:25:16.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:25:18.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:25:26.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:25:28.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:25:37.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:25:39","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:25:49.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:25:49.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:26:00.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:26:00.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:26:10.100","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:26:10.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:26:19.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:21.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:26:29.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:30.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:32.600","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:26:39.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:46.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:48.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:53.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:26:58.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:27:04.800","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:27:08.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:27:15.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:27:16.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:27:26.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:27:27.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:27:36.900","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:27:38.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:27:49.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:27:49","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:27:58.500","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.355626999999998,32.225000000000001,10,304.58362,50112.076050000003,null,32.25,166.5,1016.3320179999999,5011.1135869999998,null,null,null,null,null,null,null,null,null,1248.7700199999999,12.13,38.658000999999999,12.13]
["$","2022-02-24","02:27:59.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:28:02.400","Anchor","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","02:28:06.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:28:09.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:28:10.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:28:12.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:28:20.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:28:21.600","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:28:28.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:28:31.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:28:32.800","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:28:42.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:28:43.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:28:53","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:28:54.300","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:29:03.800","Anchor","System Data (dBar %full Volts mAmps): ",44.5,67.360138000000006,32.225000000000001,5,305.10433799999998,50647.440820000003,null,32.25,164.5,1028.2211890000001,5064.6366330000001,null,null,null,null,null,null,null,null,null,1248.75,12.13,38.382998999999998,12.13]
["$","2022-02-24","02:29:05.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:29:14.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:15.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:29:23.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:26.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:29:32.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:33.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:37.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:29:43.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:48","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:29:51.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:58.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:30:01","Anchor","Checking Global Issues."]
["$","2022-02-24","02:30:09.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:30:10.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:30:21.400","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:30:21.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:30:32.200","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:30:32.200","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:30:43","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:30:42.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:30:52.500","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:30:53.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:31:02.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:04.300","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:31:12.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:15","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:31:21.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:25.600","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:31:33.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:36.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:31:39.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:47.100","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:31:49.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:57.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:31:59.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:32:08.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:32:09.900","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:32:20.700","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:32:20.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:32:31.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:32:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:32:31.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:32:42","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:32:50.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:32:51.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:32:52.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:33:01.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:33:03.500","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:33:12.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:33:14.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:33:19.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:33:24.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:33:29.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:33:35.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:33:42","Anchor","Checking Global Issues."]
["$","2022-02-24","02:33:46.300","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:33:47.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:33:57","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:33:58.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:34:09.200","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:34:09.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:34:18.700","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:34:19.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:34:29.400","Anchor","System Data (dBar %full Volts mAmps): ",44.5,67.366268000000005,32.225000000000001,5,307.59119600000002,53317.952010000001,null,32.225000000000001,166,1082.4155290000001,5331.6877519999998,null,null,null,null,null,null,null,null,null,1248.75,12.14,38.591999000000001,12.14]
["$","2022-02-24","02:34:30.500","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:34:40.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:34:41.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:34:51.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:34:52","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:34:58","Anchor","Checking Global Issues."]
["$","2022-02-24","02:35:02.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:35:07.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:35:13.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:35:17.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:35:24.500","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:35:26.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:35:34.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:35:36.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:35:45.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:35:47","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:35:56.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:35:56.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:36:07.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:36:08.700","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:36:08.500","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:36:18","Anchor","System Data (dBar %full Volts mAmps): ",44.5,67.355423999999999,32.225000000000001,5,308.37161800000001,54208.435799999999,null,32.225000000000001,187,1100.4852490000001,5420.7361309999997,null,null,null,null,null,null,null,null,null,1248.6899410000001,12.13,38.790999999999997,12.13]
["$","2022-02-24","02:36:19.300","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:36:30.400","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:36:30","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:36:37.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:36:40.700","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:36:47.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:36:51.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:36:56.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:37:02.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:37:05.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:37:12.800","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:37:15.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:37:23.500","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:37:25","Anchor","Checking Global Issues."]
["$","2022-02-24","02:37:34.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:37:35.600","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:37:46.400","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:37:46.400","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:37:57.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:37:57","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:38:02.400","Anchor","Sending Optode Do Sample"]
["$","2022-02-24","02:38:03.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:38:08.400","Anchor","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","02:38:07.800","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:38:13.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:38:17.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:38:19.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:38:26.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:38:27.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:38:29.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:38:38.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:38:40","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:38:49.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:38:50.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:38:55.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:39:01.500","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:39:01.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:39:11.100","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:39:12.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:39:21.900","Anchor","System Data (dBar %full Volts mAmps): ",44.630001,67.353106999999994,32.225000000000001,5,309.71866499999999,55716.482859999996,null,32.225000000000001,168,1132.1298529999999,5571.5408369999996,null,null,null,null,null,null,null,null,null,1248.6400149999999,12.13,38.459000000000003,12.13]
["$","2022-02-24","02:39:23","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:39:34.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:39:33.700","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:39:40.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:39:44.500","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:39:50.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:39:55.200","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:40:00.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:40:06.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:40:09.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:40:16.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:40:18","Anchor","Checking Global Issues."]
["$","2022-02-24","02:40:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:40:28.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:40:38.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:40:39.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:40:50.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:40:50.200","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:40:59.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:41:00.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:41:10.400","Anchor","System Data (dBar %full Volts mAmps): ",44.630001,67.355540000000005,32.225000000000001,5,310.50958000000003,56606.429409999997,null,32.225000000000001,165,1150.1642899999999,5660.5220600000002,null,null,null,null,null,null,null,null,null,1248.6899410000001,12.13,38.216999000000001,12.13]
["$","2022-02-24","02:41:10.900","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:41:19.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:41:22.200","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:41:29.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:41:33","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:41:39","Anchor","Checking Global Issues."]
["$","2022-02-24","02:41:43.100","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:41:47.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:41:54.300","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:41:57.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:42:05","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:42:06.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:42:15.800","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:42:16.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:42:27.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:42:26.500","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:42:27.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:42:38.700","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:42:38.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:42:48.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:42:54.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:42:58.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:00","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:43:08.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:10.700","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:43:18.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:22.200","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:43:26.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:32.200","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:43:36.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:42.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:43:46.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:53.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:43:54.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:44:04.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:44:05.600","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:44:15","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:44:16.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:44:27.200","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:44:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:44:33.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:44:37.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:44:47.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:44:48.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:44:57.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:44:59.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:45:03.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:45:09.900","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:45:15.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:45:20.800","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:45:24.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:45:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:45:34.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:45:43.300","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:45:42.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:45:43.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:45:52.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:45:54.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:46:03.600","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:46:14.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:46:15.800","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:46:15.600","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:46:25.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:46:26.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:46:36","Anchor","System Data (dBar %full Volts mAmps): ",44.630001,67.356645,32.200000000000003,5,312.67508700000002,59276.940600000002,null,32.225000000000001,167,1204.463166,5927.5731800000003,null,null,null,null,null,null,null,null,null,1248.6099850000001,12.12,38.581001000000001,12.12]
["$","2022-02-24","02:46:37.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:46:41.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:46:47.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:46:54.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:46:58.400","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:47:04.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:47:09.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:47:14.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:47:19.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:47:22.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:47:30.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:47:32.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:47:41.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:47:42.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:47:52","Anchor","System Data (dBar %full Volts mAmps): ",44.630001,67.345500999999999,32.200000000000003,5,313.15645699999999,59899.742010000002,null,32.200000000000003,166.5,1217.0882959999999,5989.8533200000002,null,null,null,null,null,null,null,null,null,1248.6099850000001,12.12,38.847000000000001,12.12]
["$","2022-02-24","02:47:53.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:48:02.400","Anchor","Sending CTD PTS"]
["$","2022-02-24","02:48:03","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:48:03.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:48:06.800","Anchor","Setting MSC time and CTD Values: 1645670886,33.70,10.578,44.71"]
["$","2022-02-24","02:48:12.900","Anchor","[MSC] Timeout for CommandWake"]
["$","2022-02-24","02:48:13.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:48:16.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:48:23.800","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.357984000000002,32.200000000000003,10,313.38599299999998,60160.70882,null,32.200000000000003,181.5,1223.211264,6015.9500019999996,null,null,null,null,null,null,null,null,null,1248.6400149999999,12.12,38.459000000000003,12.12]
["$","2022-02-24","02:48:24.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:48:27.700","Anchor","[MSC] Done Sampling."]
["$","2022-02-24","02:48:35.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:48:37.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:48:39.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:48:45.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:48:47.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:48:56.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:48:57.900","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:49:07.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:49:08.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:49:18.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:49:19.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:49:29","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.344905999999995,32.200000000000003,5,313.77554800000001,60694.999100000001,null,32.200000000000003,165.5,1234.2365930000001,6069.3924610000004,null,null,null,null,null,null,null,null,null,1248.6400149999999,12.13,38.205002,12.13]
["$","2022-02-24","02:49:30.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:49:39.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:49:40.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:49:50.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:49:51.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:49:57.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:50:02.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:50:07.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:50:13.100","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:50:16.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:50:23.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:50:26.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:50:34.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:50:35.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:50:45","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:50:46.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:50:55.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:50:57.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:51:06.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:51:07.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:51:17.500","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.337872000000004,32.200000000000003,10,314.50481600000001,61584.811329999997,null,32.200000000000003,165.5,1252.365337,6158.3602529999998,null,null,null,null,null,null,null,null,null,1248.5600589999999,12.13,38.039000999999999,12.13]
["$","2022-02-24","02:51:18.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:51:28.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:51:29.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:51:37.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:51:40.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:51:46","Anchor","Checking Global Issues."]
["$","2022-02-24","02:51:50.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:51:55.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:51:58.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:52:01.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:52:04.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:52:12.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:52:14.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:52:22.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:52:24.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:52:33.700","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:52:34.900","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:52:45.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:52:45.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:52:56.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:52:56.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:53:06","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.341504999999998,32.200000000000003,10,315.28786200000002,62474.623570000003,null,32.200000000000003,167,1270.4042340000001,6247.3414769999999,null,null,null,null,null,null,null,null,null,1248.530029,12.12,38.625999,12.12]
["$","2022-02-24","02:53:07.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:53:15.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:53:17.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:53:25.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:53:28.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:53:35.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:53:39.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:53:44.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:53:49.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:53:53.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:54:00.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:54:03.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:54:11.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:54:15.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:54:22","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:54:23.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:54:34.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:54:34.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:54:45.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:54:45.100","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:54:54.500","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.356866999999994,32.200000000000003,5,316.01713000000001,63364.570110000001,null,32.200000000000003,165,1288.452706,6336.336131,null,null,null,null,null,null,null,null,null,1248.589966,12.13,37.884998000000003,12.13]
["$","2022-02-24","02:54:55.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:55:04.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:06.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:55:14.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:17.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:55:17.500","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:55:23","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:27.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:55:32.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:38.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:55:42.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:49.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:55:54.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:59.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:56:01.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:56:10.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:56:12","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:56:22.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:56:24.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:56:32.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:56:33.500","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:56:43","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.350992000000005,32.200000000000003,5,316.89198900000002,64254.650970000002,null,32.200000000000003,166.5,1306.5857779999999,6425.3307860000004,null,null,null,null,null,null,null,null,null,1248.4799800000001,12.12,37.905997999999997,12.12]
["$","2022-02-24","02:56:44.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:56:53.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:56:55","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:57:04.800","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.350209000000007,32.200000000000003,10,317.06643700000001,64433.016349999998,null,32.200000000000003,166,1310.2030010000001,6443.167324,null,null,null,null,null,null,null,null,null,1248.530029,12.12,37.883999000000003,12.12]
["$","2022-02-24","02:57:05.700","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:57:11.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:57:16.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:57:19.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:57:26.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:57:29.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:57:35.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:57:38.800","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:57:48.300","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:57:49.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:58:00.500","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:58:00.500","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:58:00.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:58:11.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:58:17.200","Anchor","Normal State Exit"]
["$","2022-02-24","02:58:17.300","Start CP Mode","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","02:58:20.700","Start CP Mode","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.337405000000004,32.200000000000003,10,317.693398,65055.952069999999,null,32.200000000000003,166.5,1322.8434769999999,6505.4743269999999,null,null,null,null,null,null,null,null,null,1248.5600589999999,12.13,38.470001000000003,12.13]
["$","2022-02-24","02:58:22.200","Start CP Mode","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:58:22.400","Start CP Mode","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:58:24","DeAnchor","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","02:58:24","DeAnchor","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","02:58:24.400","DeAnchor","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","02:58:32.500","DeAnchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:58:32.300","DeAnchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:58:35.400","DeAnchor","SBE41 Message",44.700001,66.815740000000005,32.15,155.5,null,null,null,null,null,null,null,null,"   44.70, 10.5779, 33.6992  ",44.700001,44.660772000000001,2.029E-3,-1.6666E-2,-1.6667000000000001E-2,2.3E-5,3000]
["$","2022-02-24","02:58:42.500","DeAnchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:58:41.700","DeAnchor","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","02:58:43.400","DeAnchor","SBE41 Message",44.66,66.373259000000004,32.15,155.5,null,null,null,null,null,null,null,null,"   44.66, 10.5779, 33.6998  ",44.66,44.637791999999997,9.4399999999999996E-4,-0.02,-1.6666E-2,7.1000000000000005E-5,3000]
["$","2022-02-24","02:58:49","DeAnchor","Checking Global Issues."]
["$","2022-02-24","02:58:51.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.60, 10.5785, 33.6996  "]
["$","2022-02-24","02:58:52.500","DeAnchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:58:57.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.56, 10.5797, 33.6991  "]
["$","2022-02-24","02:59:01.300","DeAnchor","SBE41 Message",44.75,65.107254999999995,32.15,155.5,null,null,null,null,null,null,null,null,"   44.75, 10.5791, 33.6990  ",44.75,44.575597999999999,1.9870000000000001E-3,-0.02,-0.02,1.16E-4,3000]
["$","2022-02-24","02:59:02.100","DeAnchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:59:05.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.58, 10.5790, 33.6995  "]
["$","2022-02-24","02:59:10.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.64, 10.5789, 33.6993  "]
["$","2022-02-24","02:59:11.700","DeAnchor","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","02:59:13.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.72, 10.5795, 33.6988  "]
["$","2022-02-24","02:59:18.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.54, 10.5786, 33.6995  "]
["$","2022-02-24","02:59:21.100","DeAnchor","Pump motor not faulted"]
["$","2022-02-24","02:59:22.300","DeAnchor","SBE41 Message",44.650002000000001,63.740324999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   44.65, 10.5789, 33.6994  ",44.650002000000001,44.584418999999997,-3.28E-4,-1.3334E-2,-1.4999999999999999E-2,-3.1700000000000001E-4,3000]
["$","2022-02-24","02:59:26.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.63, 10.5785, 33.6993  "]
["$","2022-02-24","02:59:31.100","DeAnchor","Pump motor not faulted"]
["$","2022-02-24","02:59:32.100","DeAnchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:59:35","DeAnchor","Checking Global Issues."]
["$","2022-02-24","02:59:37.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.62, 10.5785, 33.6996  "]
["$","2022-02-24","02:59:41.500","DeAnchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:59:43","DeAnchor","Checking Global Issues."]
["$","2022-02-24","02:59:48","DeAnchor","Checking Global Issues."]
["$","2022-02-24","02:59:51.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.63, 10.5786, 33.6995  "]
["$","2022-02-24","02:59:52.300","DeAnchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:59:56.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.44, 10.5783, 33.6997  "]
["$","2022-02-24","02:59:59.300","DeAnchor","SBE41 Message",44.419998,61.088261000000003,32.15,155.5,null,null,null,null,null,null,null,null,"   44.42, 10.5784, 33.7002  ",44.419998,44.597019000000003,5.6899999999999995E-4,-1.6666E-2,-3.333E-3,6.38E-4,3000]
["$","2022-02-24","03:00:01.900","DeAnchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:00:04.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.40, 10.5780, 33.6998  "]
["$","2022-02-24","03:00:09.300","DeAnchor","SBE41 Message",44.119999,60.359456999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   44.12, 10.5819, 33.6985  ",44.119999,44.382106999999998,3.7069999999999998E-3,3.3340000000000002E-3,8.3330000000000001E-3,5.0309999999999999E-3,3000]
["$","2022-02-24","03:00:11.600","DeAnchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","03:00:11.600","DeAnchor","Twitter msg",null,null,null,null,null,null,"-3.99919;"]
["$","2022-02-24","03:00:13.100","DeAnchor","Checking Global Issues."]
["$","2022-02-24","03:00:20.300","DeAnchor","SBE41 Message",43.52,59.602936,32.15,155.5,null,null,null,null,null,null,null,null,"   43.52, 10.5884, 33.6979  ",43.52,43.799086000000003,1.6205000000000001E-2,0.02,1.8332999999999999E-2,1.7387E-2,3000]
["$","2022-02-24","03:00:21.200","DeAnchor","Twitter msg",null,null,null,null,null,null,"-146884;"]
["$","2022-02-24","03:00:22.400","DeAnchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:00:26.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   42.91, 10.6052, 33.6942  "]
["$","2022-02-24","03:00:31.100","DeAnchor","System Data (dBar %full Volts mAmps): ",42.619999,58.806688000000001,32.049999999999997,725,419.75029599999999,66124.935549999995,null,32.049999999999997,184.5,1346.7877410000001,6612.3726749999996,null,null,null,null,null,null,null,null,null,1235.589966,12.12,38.282001000000001,12.12]
["$","2022-02-24","03:00:32","DeAnchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:00:35.400","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:35.400","Ascend","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","03:00:35.800","Ascend","[MSC] Resetting Sequencers"]
["$","2022-02-24","03:00:37.300","Ascend","SBE41 Message",41.720001000000003,58.38823,32.15,155.5,null,null,null,null,null,null,null,null,"   41.72, 10.6506, 33.6831  ",41.720001000000003,42.376551999999997,3.0995999999999999E-2,3.6666999999999998E-2,4.1667000000000003E-2,5.5944000000000001E-2,3000]
["$","2022-02-24","03:00:38.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:40.300","Ascend","BE::sendJV: -83284"]
["$","2022-02-24","03:00:41.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:42.800","Ascend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:00:43.200","Ascend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:00:44","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:45.300","Ascend","BE::sendJV: -69682"]
["$","2022-02-24","03:00:46.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-65948;"]
["$","2022-02-24","03:00:47.800","Ascend","Checking Global Issues."]
["$","2022-02-24","03:00:48.800","Ascend","Checking Global Issues."]
["$","2022-02-24","03:00:50.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:51.600","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:00:54.400","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:00:54.800","Ascend","FLBB Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"/99/99,99:99:99,695,91,700,771,546  "]
["$","2022-02-24","03:00:53.900","Ascend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","03:00:54.500","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:55.200","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   39.44, 10.6708, 33.6850  "]
["$","2022-02-24","03:00:56.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:00:57.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:00:58.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:00.200","Ascend","SBE41 Message",38.75,57.617007999999998,32.15,155.5,null,null,null,null,null,null,null,null,"   38.75, 10.6958, 33.6779  ",38.75,39.432664000000003,4.2882999999999998E-2,3.3333000000000002E-2,3.8332999999999999E-2,0.11249199999999999,3000]
["$","2022-02-24","03:01:01.200","Ascend","SBE41 Message",38.630001,57.598629000000003,32.15,155.5,null,null,null,null,null,null,null,null,"   38.63, 10.7009, 33.6739  ",38.630001,39.271684,4.3625999999999998E-2,0.04,3.6665999999999997E-2,0.114582,3000]
["$","2022-02-24","03:01:02.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:01:03.300","Ascend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:01:04.800","Ascend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","03:01:05.200","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   37.97, 10.7079, 33.6716  "]
["$","2022-02-24","03:01:06.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:01:07.400","Ascend","Vel PID Values",37.689999,57.352257999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,4.3333999999999998E-2,4.7995999999999997E-2,4.7399999999999997E-4,5.6429999999999996E-3,7.7865869999999999,7.7865869999999999,63787,1]
["$","2022-02-24","03:01:07.200","Ascend","SBE41 Message",37.689999,57.352257999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   37.69, 10.7089, 33.6716  ",37.689999,38.475914000000003,4.6066000000000003E-2,4.3333999999999998E-2,4.6667E-2,0.124191,3000]
["$","2022-02-24","03:01:09.200","Ascend","SBE41 Message",37.409999999999997,57.305956000000002,32.15,155.5,null,null,null,null,null,null,null,null,"   37.41, 10.7097, 33.6718  ",37.409999999999997,38.152149000000001,4.6156000000000003E-2,5.0000999999999997E-2,4.6665999999999999E-2,0.12694800000000001,3000]
["$","2022-02-24","03:01:09.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:11.400","Ascend","Vel PID Values",37.090000000000003,57.241768,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.3333E-2,4.9097000000000002E-2,3.59E-4,6.2919999999999998E-3,7.7910750000000002,7.7910750000000002,63824,1]
["$","2022-02-24","03:01:12.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-63556;"]
["$","2022-02-24","03:01:13.800","Ascend","[MSC] Data: 0x41E6,pH,02/24/2022 03:01:20,1645671654,39.88,10.6689,33.6802,58,6,0,12.76,38.14,11.672,4.620e-02,7.1234,3.549,-0.964876,0.000015,-0.919728,0.000011,+1.790e-09,+8.138e-11  "]
["$","2022-02-24","03:01:14.200","Ascend","SBE41 Message",36.529998999999997,57.112580000000001,32.15,155.5,null,null,null,null,null,null,null,null,"   36.53, 10.7258, 33.6689  ",36.529998999999997,37.407798999999997,4.9806999999999997E-2,6.3334000000000001E-2,6.6667000000000004E-2,0.133631,3000]
["$","2022-02-24","03:01:15.400","Ascend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","03:01:16.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:17.300","Ascend","BE::sendJV: -62890"]
["$","2022-02-24","03:01:18.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-64860;"]
["$","2022-02-24","03:01:19.900","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:21.300","Ascend","SBE41 Message",35.529998999999997,56.894159999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   35.53, 10.7337, 33.6662  ",35.529998999999997,36.230051000000003,5.4488000000000002E-2,6.6667000000000004E-2,5.6667000000000002E-2,0.142183,3000]
["$","2022-02-24","03:01:22.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:01:23.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:24.600","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:01:26.600","Ascend","Setting MSC time and CTD Values: 1645671686,33.67,10.745,34.72"]
["$","2022-02-24","03:01:25.500","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,160.294,10.661,40.234,39.542,48.467,8.925,930.6,669.2,439.4  "]
["$","2022-02-24","03:01:26.400","Ascend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","03:01:27.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:28.200","Ascend","SBE41 Message",34.259998000000003,56.641359999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   34.26, 10.7949, 33.6588  ",34.259998000000003,35.105649999999997,5.2393000000000002E-2,5.3332999999999998E-2,4.8333000000000001E-2,0.148262,3000]
["$","2022-02-24","03:01:29.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:01:31","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:32.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:01:33.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:01:34.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:35.200","Ascend","SBE41 Message",33.040000999999997,56.441867000000002,32.15,155.5,null,null,null,null,null,null,null,null,"   33.04, 10.9028, 33.6287  ",33.040000999999997,33.951425999999998,5.6085999999999997E-2,6.6667000000000004E-2,6.6666000000000003E-2,0.15606300000000001,3000]
["$","2022-02-24","03:01:36.300","Ascend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:01:37.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:38.200","Ascend","BE::sendJV: -57373"]
["$","2022-02-24","03:01:39.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:40.900","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:41.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:43.200","Ascend","BE::sendJV: -60802"]
["$","2022-02-24","03:01:44.200","Ascend","SBE41 Message",31.5,56.162190000000002,32.15,155.5,null,null,null,null,null,null,null,null,"   31.50, 11.0821, 33.5896  ",31.5,32.317307,6.0595000000000003E-2,5.6667000000000002E-2,5.5E-2,0.164961,3000]
["$","2022-02-24","03:01:45.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:46.600","Ascend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","03:01:47.400","Ascend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","03:01:48.500","Ascend","Vel PID Values",30.700001,56.033450999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.3333E-2,5.8867000000000003E-2,4.0400000000000001E-4,1.1924000000000001E-2,6.9791679999999996,6.9791679999999996,57173,1]
["$","2022-02-24","03:01:48.200","Ascend","SBE41 Message",30.700001,56.033450999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   30.70, 11.1350, 33.5754  ",30.700001,31.662185000000001,5.7044999999999998E-2,6.3333E-2,7.0000000000000007E-2,0.16770299999999999,3000]
["$","2022-02-24","03:01:49.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:51.200","Ascend","BE::sendJV: -55807"]
["$","2022-02-24","03:01:52.200","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:01:53.700","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:54.700","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   29.69, 11.1676, 33.5729  "]
["$","2022-02-24","03:01:55.500","Ascend","[MSC] RX: ACK  "]
["$","2022-02-24","03:01:55.700","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:01:56.400","Ascend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","03:01:57.500","Ascend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","03:01:58.200","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   28.90, 11.1933, 33.5604  "]
["$","2022-02-24","03:01:59.200","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:02:00.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:02.300","Ascend","Vel PID Values",28.129999000000002,55.700105000000001,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,5.3333999999999999E-2,6.1305999999999999E-2,2.0699999999999999E-4,1.3936E-2,6.9439339999999996,6.9439339999999996,56884,1]
["$","2022-02-24","03:02:03.200","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-58355;"]
["$","2022-02-24","03:02:04.200","Ascend","SBE41 Message",27.82,55.639701000000002,32.15,155.5,null,null,null,null,null,null,null,null,"   27.82, 11.2655, 33.5554  ",27.82,28.691898999999999,5.9587000000000001E-2,5.3332999999999998E-2,5.1666999999999998E-2,0.177012,3000]
["$","2022-02-24","03:02:05.200","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-58542;"]
["$","2022-02-24","03:02:06.800","Ascend","Checking Global Issues."]
["$","2022-02-24","03:02:07.500","Ascend","Twitter msg",null,null,null,null,null,null,"46187280;"]
["$","2022-02-24","03:02:08.500","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:02:09.200","Ascend","SBE41 Message",26.790001,55.490949000000001,32.15,155.5,null,null,null,null,null,null,null,null,"   26.79, 11.3601, 33.5313  ",26.790001,27.799472000000002,6.2579999999999997E-2,7.0000000000000007E-2,7.1665999999999994E-2,0.17939099999999999,3000]
["$","2022-02-24","03:02:10.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:11.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:12.700","Ascend","Checking Global Issues."]
["$","2022-02-24","03:02:14.200","Ascend","SBE41 Message",25.959999,55.339058999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   25.96, 11.4226, 33.5118  ",25.959999,26.811354000000001,6.1683000000000002E-2,6.3334000000000001E-2,5.6667000000000002E-2,0.18230199999999999,3000]
["$","2022-02-24","03:02:15.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:17.200","Ascend","BE::sendJV: -57091"]
["$","2022-02-24","03:02:17.800","Ascend","Twitter msg",null,null,null,null,null,null,"-55573;"]
["$","2022-02-24","03:02:18.600","Ascend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:02:19.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:20.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:22.500","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:02:22.400","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,171.175,11.109,39.180,38.488,47.415,8.927,900.7,667.6,425.0  "]
["$","2022-02-24","03:02:22.900","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:24.200","Ascend","BE::sendJV: -57094"]
["$","2022-02-24","03:02:25.200","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:02:26.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:29.200","Ascend","getting Elmo acceleration limit"]
["$","2022-02-24","03:02:28.600","Ascend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:02:28.800","Ascend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","03:02:29.400","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:30.100","Ascend","SBE41 Message",22.92,54.860487999999997,32.15,155.5,null,null,null,null,null,null,null,null,"   22.92, 11.4698, 33.5083  ",22.92,23.843316999999999,6.1962000000000003E-2,6.6667000000000004E-2,6.1667E-2,0.18675600000000001,3000]
["$","2022-02-24","03:02:31.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:32.200","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-58779;"]
["$","2022-02-24","03:02:34.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   22.17, 11.4723, 33.5072  "]
["$","2022-02-24","03:02:35.200","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:02:36.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:37.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:38.700","Ascend","System Data (dBar %full Volts mAmps): ",21.360001,54.598908000000002,32.1,245,459.44032900000002,67171.623359999998,null,32.125,195,1373.9373760000001,6717.0280249999996,null,null,null,null,null,null,null,null,null,1230.420044,12.12,37.994999,12.12]
["$","2022-02-24","03:02:39.400","Ascend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","03:02:40.400","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:02:41.100","Ascend","SBE41 Message",20.77,54.538406999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   20.77, 11.4730, 33.5086  ",20.77,21.780604,6.2459000000000001E-2,6.6666000000000003E-2,6.5000000000000002E-2,0.18701100000000001,3000]
["$","2022-02-24","03:02:42.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:44.200","Ascend","BE::sendJV: -55787"]
["$","2022-02-24","03:02:45.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:46.500","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:02:48.500","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:02:49.100","Ascend","Optode post: 4330,2707,194.736,11.398,37.415,36.723,45.653,8.930,849.5,665.7,415.8  "]
["$","2022-02-24","03:02:48.900","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:51.200","Ascend","getting Elmo acceleration limit"]
["$","2022-02-24","03:02:50.600","Ascend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:02:51.400","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-55456;"]
["$","2022-02-24","03:02:52.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-54753;"]
["$","2022-02-24","03:02:53.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:55.300","Ascend","Vel PID Values",18.059999000000001,54.139116000000001,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,0.06,6.5106999999999998E-2,2.3E-5,2.1332E-2,6.7940500000000004,6.7940500000000004,55656,1]
["$","2022-02-24","03:02:56.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:57.500","Ascend","[MSC] Data: 0x8ADF,A,02/24/2022 03:03:02,1645671768,19.64,11.4907,33.5051,62,6,0,0,12.93,37.94,11.500,5.650e-01,17481.00,899.00,1017.16,4.77,33.51,19.89,7.231e-04,36,77,2AA82F663318359D37063798378237163681360335B635B2360D36C6380539C43BE13E9141BA454949344D6F51DB56355A795E2C6154639764CD64E063D161A05EB55AF856F552D64EBB4AD547534424414C3EEC,1112.4  "]
["$","2022-02-24","03:02:58.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:00.100","Ascend","SBE41 Message",17.09,54.029670000000003,32.15,155.5,null,null,null,null,null,null,null,null,"   17.09, 11.4985, 33.5074  ",17.09,18.05396,6.5172999999999995E-2,7.0000000000000007E-2,6.3333E-2,0.19245999999999999,3000]
["$","2022-02-24","03:03:00.700","Ascend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:03:01.900","Ascend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:03:02.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:03.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:04.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:06.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   15.88, 11.5034, 33.5056  "]
["$","2022-02-24","03:03:06.300","Ascend","Vel PID Values",15.88,53.842283999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,6.5766000000000005E-2,5.3999999999999998E-5,2.2821999999999999E-2,6.7181059999999997,6.7181059999999997,55034,1]
["$","2022-02-24","03:03:08.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:10.100","Ascend","BE::sendJV: -55793"]
["$","2022-02-24","03:03:10.200","Ascend","Vel PID Values",15.11,53.760922000000001,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.3334000000000001E-2,6.5676999999999999E-2,-5.1999999999999997E-5,2.3361E-2,6.810746,6.810746,55793,1]
["$","2022-02-24","03:03:11.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-55644;"]
["$","2022-02-24","03:03:13","Ascend","getting Elmo acceleration limit"]
["$","2022-02-24","03:03:13.300"]
["$","2022-02-24","03:03:12.400","Ascend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","03:03:13.400","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:14.400","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:15.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:17.100","Ascend","BE::sendJV: -55403"]
["$","2022-02-24","03:03:18.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:20.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   13.12, 11.5312, 33.5006  "]
["$","2022-02-24","03:03:21","Ascend","[MSC] Post NO3: 18.80"]
["$","2022-02-24","03:03:21.400","Ascend","[MSC] TX: T2,1645671793,11.5346,33.5002,14.7100"]
["$","2022-02-24","03:03:22.400","Ascend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","03:03:23.200","Ascend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","03:03:24.300","Ascend","Vel PID Values",12.34,53.331170999999998,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.3333E-2,6.5616999999999995E-2,4.3000000000000002E-5,2.5250999999999999E-2,6.7409410000000003,6.7409410000000003,55221,1]
["$","2022-02-24","03:03:25.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:27.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:27.700","Ascend","Wrote to msg file: AscendPt:,2022-Feb-24T03:03:11Z,14.71,11.5346,33.500,11.477,35.143,8.933,-0.953072,18.80,347,551,546,0.0268,0.0239,0.0084,0.2246  "]
["$","2022-02-24","03:03:29.200","Ascend","Vel PID Values",11.28,53.180154999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,6.6792000000000004E-2,2.4600000000000002E-4,2.5919999999999999E-2,6.4853579999999997,6.4853579999999997,53128,1]
["$","2022-02-24","03:03:30.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-52514;"]
["$","2022-02-24","03:03:32.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   10.66, 11.5616, 33.4983  "]
["$","2022-02-24","03:03:32.600","Ascend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:03:33.800","Ascend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","03:03:34.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:35.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51167;"]
["$","2022-02-24","03:03:37.400","Ascend","Radiometer post: SATFI40545",2.2200000000000001E-2,2.3900000000000001E-2,1.03E-2,0.21529999999999999]
["$","2022-02-24","03:03:37.800","Ascend","Vel PID Values",9.58,52.970896000000003,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,6.9060999999999997E-2,2.3800000000000001E-4,2.6969E-2,6.3115370000000004,6.3115370000000004,51704,1]
["$","2022-02-24","03:03:37.800","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:38.600","Ascend","[MSC] TX: T1,1645671817,11.5682,33.4946,9.7800"]
["$","2022-02-24","03:03:39.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:41.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51716;"]
["$","2022-02-24","03:03:42.600","Ascend","System Data (dBar %full Volts mAmps): ",8.5,52.824891000000001,32.075000000000003,220,477.58809200000002,67695.705979999999,null,32.075000000000003,421,1387.89906,6769.4497179999998,null,null,null,null,null,null,null,null,null,1228.3000489999999,12.15,37.807999000000002,12.15]
["$","2022-02-24","03:03:43.300","Ascend","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","03:03:44.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:45.300","Ascend","BE::sendJV: -51081"]
["$","2022-02-24","03:03:46.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    7.65, 11.5678, 33.4950  "]
["$","2022-02-24","03:03:46.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:48.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:50.100","Ascend","BE::sendJV: -49568"]
["$","2022-02-24","03:03:50.200","Ascend","Vel PID Values",6.74,52.646537000000002,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.3332999999999995E-2,7.1785000000000002E-2,2.9399999999999999E-4,2.8622999999999999E-2,6.0508480000000002,6.0508480000000002,49568,1]
["$","2022-02-24","03:03:51.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-49575;"]
["$","2022-02-24","03:03:52.200","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-48415;"]
["$","2022-02-24","03:03:55.100","Ascend","getting Elmo deacceleration limit"]
["$","2022-02-24","03:03:54","Ascend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","03:03:55.100","Ascend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","03:03:56.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    5.37, 11.5683, 33.4957  "]
["$","2022-02-24","03:03:57.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:58.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:00.300","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:04:00.500","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:00.700","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:02","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    4.02, 11.5678, 33.4970  "]
["$","2022-02-24","03:04:03.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:04.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:05.200","Ascend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","03:04:06.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:04:07","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    2.92, 11.5666, 33.4967  "]
["$","2022-02-24","03:04:08","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    2.72, 11.5673, 33.4965  "]
["$","2022-02-24","03:04:09.200","Ascend","Vel PID Values",2.5099999999999998,52.202494000000002,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.0000000000000007E-2,7.4422000000000002E-2,-1.84E-4,3.0931E-2,6.2243899999999996,6.2243899999999996,50990,1]
["$","2022-02-24","03:04:10.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-50607;"]
["$","2022-02-24","03:04:12.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    1.84, 11.5700, 33.4951  "]
["$","2022-02-24","03:04:13.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:04:14.200","Ascend","Vel PID Values",1.51,52.049824999999998,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,5.3332999999999998E-2,7.3058999999999999E-2,-6.3000000000000003E-4,3.1539999999999999E-2,6.6906230000000004,6.6906230000000004,54809,1]
["$","2022-02-24","03:04:15.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-52402;"]
["$","2022-02-24","03:04:15.500","Set Bellows","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","03:04:15.600","Set Bellows","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","03:04:16.100","Set Bellows","SBE41 Message",1.02,51.933847,32.15,155.5,null,null,null,null,null,null,null,null,"    1.02, 11.5706, 33.4951  ",1.02,2.0717690000000002,7.4800000000000005E-2,7.3332999999999995E-2,8.1667000000000003E-2,0.221723,3000]
["$","2022-02-24","03:04:17.500","Set Bellows","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","03:04:26","Set Bellows","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:26.200","Set Bellows","Pump motor not faulted"]
["$","2022-02-24","03:04:30.300","Set Bellows","Checking Global Issues."]
["$","2022-02-24","03:04:36.300","Set Bellows","System Data (dBar %full Volts mAmps): ",1.02,50.997993999999998,31.975000000000001,1055,498.21090700000002,68136.515599999999,null,32.024999999999999,184,1399.117463,6813.5172490000004,null,null,null,null,null,null,null,null,null,1225.579956,12.18,38.097999999999999,12.18]
["$","2022-02-24","03:04:37.400","Set Bellows","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","03:04:46.200","Set Bellows","BE::sendJV: -200000"]
["$","2022-02-24","03:04:46.700","Set Bellows","Twitter msg",null,null,null,null,null,null,"0.68175;"]
["$","2022-02-24","03:04:47.700","Set Bellows","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:04:56.300","Set Bellows","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:04:58.100","Set Bellows","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","03:04:58.100","Set Bellows","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:05:05.100","Set Bellows","Checking Global Issues."]
["$","2022-02-24","03:05:08.200","Set Bellows","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:05:09.600","Set Bellows","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","03:05:19.100","Set Bellows","Pump motor not faulted"]
["$","2022-02-24","03:05:19.500","Set Bellows","Twitter msg",null,null,null,null,null,null,"0.40324;"]
["$","2022-02-24","03:05:22.800","Set Bellows","Checking Global Issues."]
["$","2022-02-24","03:05:29.900","Set Bellows","Checking Global Issues."]
["$","2022-02-24","03:05:31","Set Bellows","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","03:05:36.800","Set Bellows","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:05:40","Dump CPData","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:05:40","Dump CPData","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","03:05:41.200","Dump CPData","Set new CTD WFR timeout to: 00:00:05"]
["$","2022-02-24","03:05:42.200","Dump CPData","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","03:05:43.200","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:43.400","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:43.900","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:44.200","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:44.300","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:44.400","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:44.600","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:44.800","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:44.900","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:45.100","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:45.300","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:45.500","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:45.700","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:45.800","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:46","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:46.200","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:46.300","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:46.500","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:46.700","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:46.900","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:47.100","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:47.200","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:47.400","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:47.500","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:47.700","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:47.700","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:47.900","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:48.100","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:48.300","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:48.400","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:48.600","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:48.800","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:49","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:49.100","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:49.300","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:49.500","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:49.600","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:49.800","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:50","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:50.200","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:50.400","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:50.500","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:50.700","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:50.900","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:51.100","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:51.200","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:51.400","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:51.600","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:51.800","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:52","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:52.100","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:53.800","Dump CPData","getting Elmo deacceleration limit"]
["$","2022-02-24","03:05:53.200","Dump CPData","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","03:05:54.300","Dump CPData","Appending CP Data:  nbins = 23"]
["$","2022-02-24","03:05:54.500","Dump CPData","Trying again for da response"]
["$","2022-02-24","03:05:54.700","Dump CPData","Sending da wait command"]
["$","2022-02-24","03:05:54.900","Dump CPData","Sending da wait command"]
["$","2022-02-24","03:05:55.200","Dump CPData","Sending da wait command"]
["$","2022-02-24","03:05:55.400","Dump CPData","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   36.03,  10.7294,  33.6674, 12  "]
["$","2022-02-24","03:05:55.700","Dump CPData","Sending da wait command"]
["$","2022-02-24","03:05:55.900","Dump CPData","Appending CP Data: 00142D3182D80A  "]
["$","2022-02-24","03:05:56.200","Dump CPData","Appending CP Data: 00782D1482DD0A  "]
["$","2022-02-24","03:05:56.100","Dump CPData","CP Message",null,null,null,null,null,null,null,null,null,null,null,null,"00DD2CD182E30A  "]
["$","2022-02-24","03:05:56.200","Dump CPData","CP Message",null,null,null,null,null,null,null,null,null,null,null,null,"012C2B9783220B  "]
["$","2022-02-24","03:05:56.300","Dump CPData","CP Message",null,null,null,null,null,null,null,null,null,null,null,null,"01402B0983480B  "]
["$","2022-02-24","03:05:56.400","Dump CPData","CP Message",null,null,null,null,null,null,null,null,null,null,null,null,"01A5298B839812  "]
["$","2022-02-24","03:05:58.200","Dump CPData","Checking Global Issues."]
["$","2022-02-24","03:05:58.300","Surface Ops","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","03:06:19.300","Surface Ops","Attempting GPS time synch, try number: 0;  Set system time to: 02/24/2022 03:06:18"]
["$","2022-02-24","03:06:04.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:06:05.700","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:06:19.700","Surface Ops","SBE41 Message",-0.18,44.875093999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.18,-0.18,0.71076700000000004,7.2878999999999999E-2,-3.333E-3,0,4.3914000000000002E-2,3000]
["$","2022-02-24","03:06:24.900","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","03:06:25.900","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System Control,4330,2707,0,0,0  "]
["$","2022-02-24","03:06:26.400","Surface Ops","Sending Optode Get ConfigXML"]
["$","2022-02-24","03:06:30.300","Surface Ops","Sci Logger sending FastPressure to CTD"]
["$","2022-02-24","03:06:27.500","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CalDataAPress[hPa],4330,2707,993.137  "]
["$","2022-02-24","03:06:28","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog1 Coef,4330,2707,0.000000E+00,1.000000E+00  "]
["$","2022-02-24","03:06:28.700","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"<NodeConfig ID=\"4330-2707\" SerialNo=\"2707\" ProdNo=\"4330\" ProdName=\"Optode Sensor\" Descr=\"Optode Sensor #2707\" Adr=\"3234560\" IsSensor=\"true\" ProtocolVer=\"6\" ConfigVer=\"12\" NodeTypeID=\"2040\">  "]
["$","2022-02-24","03:06:29.800","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"5\" Descr=\"HW Version 3\" Type=\"VT_BSTR\" Access=\"R3W4\">Rev4</Property>  "]
["$","2022-02-24","03:06:33.900","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:06:32.400","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"3\" Descr=\"Flow Control\" Type=\"VT_I4\" Access=\"R3W3\" StandAlone=\"true\" Enum=\"None=0;Xon/Xoff=2\">2</Property>  "]
["$","2022-02-24","03:06:32.500","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"3\" Descr=\"PhaseCoef\" Type=\"VT_ARRAY|VT_R4\" Access=\"R1W3\">6.919999E-01;1.000000E+00;0.000000E+00;0.000000E+00</Property>  "]
["$","2022-02-24","03:06:34.400","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"13\" Descr=\"CalDataZero\" Type=\"VT_ARRAY|VT_R4\" Unit=\"Deg\" Format=\"%0.3f\" Access=\"R1W3\">6.158697E+01;2.215172E+01</Property>  "]
["$","2022-02-24","03:06:35.500","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"0\" Descr=\"Enable Text\" Type=\"VT_BOOL\" Access=\"R1W2\" StandAlone=\"true\">false</Property>  "]
["$","2022-02-24","03:06:37","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,<PropertyCategory ID=\"5\" Descr=\"Output Settings\">  "]
["$","2022-02-24","03:06:37.800","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",</ConfigCategory>  "]
["$","2022-02-24","03:06:38.600","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:06:39.600","Surface Ops","SBE41 Message",-0.02,44.874322999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.02,-0.02,-0.17777799999999999,0.123889,-5.3332999999999998E-2,-2.8333000000000001E-2,3.7759000000000001E-2,3000]
["$","2022-02-24","03:06:42.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:06:45.600","Surface Ops","SBE41 Message",-0.12,44.876963000000003,32.15,155.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.173565,7.6988000000000001E-2,-1.6667000000000001E-2,1.6667000000000001E-2,3.5309E-2,3000]
["$","2022-02-24","03:06:51.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:06:55.300"]
["$","2022-02-24","03:06:57","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:00.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:04.600","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.12,44.845080000000003,0.47499999999999998,0,570.31009400000005,69289.577950000006,null,32.15,119.5,1422.67309,6928.8234830000001,null,null,null,null,null,null,null,null,null,1217.3199460000001,12.26,38.139000000000003,12.26]
["$","2022-02-24","03:07:09.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:13.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:18.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:21.600","Surface Ops","SBE41 Message",-0.05,44.851087999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-0.110623,1.544E-3,-4.3333000000000003E-2,-2.5000000000000001E-2,2.3911999999999999E-2,3000]
["$","2022-02-24","03:07:24.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","03:07:25.900","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","03:07:30.800","Surface Ops","SBE41 Message",7.0000000000000007E-2,44.842841,32.15,155.5,null,null,null,null,null,null,null,null,7.0000000000000007E-2,7.0000000000000007E-2,-0.139458,-4.4559999999999999E-3,-0.05,-3.5000000000000003E-2,2.1239999999999998E-2,3000]
["$","2022-02-24","03:07:31.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:32.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:32.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:32.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:33.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:33.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:33.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:33.700","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.19]
["$","2022-02-24","03:07:33.700"]
["$","2022-02-24","03:07:33.700","Surface Ops","SBE41 Message",-0.19,44.850333999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.19,-0.19,-0.13746800000000001,-2.751E-3,8.6666999999999994E-2,1.8332999999999999E-2,2.0392E-2,3000]
["$","2022-02-24","03:07:34.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:35.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:36.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:36.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:36.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:36.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:36.600","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.19,44.838317000000004,0.3,0,570.31140600000003,69551.753570000001,null,32.15,124,1426.6281899999999,6955.0410449999999,null,null,null,null,null,null,null,null,null,1217.369995,12.29,37.897998999999999,12.29]
["$","2022-02-24","03:07:36.700","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:07:38.100","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:07:38.100","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:07:36.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","03:07:38.100"]
["$","2022-02-24","03:07:36.800","Surface Ops","SBE41 Message",-0.05,44.838317000000004,32.15,155.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-0.11693099999999999,1.3999999999999999E-4,-4.6667E-2,0.02,1.9546999999999998E-2,3000]
["$","2022-02-24","03:07:38.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:39.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:39.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:39.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:39.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","03:07:40.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:40.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:40.800","Surface Ops","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","03:07:41.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:42.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:42.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:42.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:42.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.18]
["$","2022-02-24","03:07:42.700"]
["$","2022-02-24","03:07:42.600","Surface Ops","SBE41 Message",-0.18,44.839756000000001,32.15,155.5,null,null,null,null,null,null,null,null,-0.18,-0.18,-9.1131000000000004E-2,1.897E-3,4.3333000000000003E-2,-1.6670000000000001E-3,1.8678E-2,3000]
["$","2022-02-24","03:07:43.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:44.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:45.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:45.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:45.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:45.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:45.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","03:07:45.800"]
["$","2022-02-24","03:07:45.800","Surface Ops","SBE41 Message",-0.15,44.843766000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-6.9980000000000001E-2,8.8900000000000003E-4,-0.01,1.6667000000000001E-2,1.7817E-2,3000]
["$","2022-02-24","03:07:46.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:47.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:47.200","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.15,44.843577000000003,0.27500000000000002,0,570.31140600000003,69638.921589999998,null,32.15,125,1427.9298550000001,6963.7578469999999,null,null,null,null,null,null,null,null,null,1217.369995,12.29,37.887999999999998,12.29]
["$","2022-02-24","03:07:47.300","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:07:48.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:48.700","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:07:48.700","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:07:47.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:47.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:48.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:48.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.01]
["$","2022-02-24","03:07:48.800"]
["$","2022-02-24","03:07:48.600","Surface Ops","SBE41 Message",0.01,44.843577000000003,32.15,155.5,null,null,null,null,null,null,null,null,0.01,0.01,-6.6231999999999999E-2,-2.496E-3,-5.3332999999999998E-2,-3.1667000000000001E-2,1.6969000000000001E-2,3000]
["$","2022-02-24","03:07:48.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:49.700","Surface Ops","Starting Surface Optode and OCR Samples number 4 of 5"]
["$","2022-02-24","03:07:50.700","Surface Ops","SciLogger is writing previous sample before starting new one"]
["$","2022-02-24","03:07:50.800","Surface Ops","Wrote to msg file: AirCal:,2022-Feb-24T03:07:24Z,NaN,NaN,NaN,11.518,31.297,8.937,,,604,509,545,0.0221,0.0240,0.0089,0.1885  "]
["$","2022-02-24","03:07:50.800","Surface Ops","[ERROR] Missed CTD message 13"]
["$","2022-02-24","03:07:50.800","Surface Ops","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:07:51.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:51.800","Surface Ops","Sci Logger sending FastPressure to CTD"]
["$","2022-02-24","03:07:51.800","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:51.800","Surface Ops","Sci Logger sending sample Optode"]
["$","2022-02-24","03:07:51.800","Surface Ops","Sending Optode Do Sample"]
["$","2022-02-24","03:07:51.800","Surface Ops","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:07:51.800","Surface Ops","Sending radiometer pollSample"]
["$","2022-02-24","03:07:50.500","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:50.500","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:50.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:51.900","Surface Ops","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","03:07:51.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:51.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","03:07:52"]
["$","2022-02-24","03:07:51.600","Surface Ops","SBE41 Message",-0.17,44.830075000000001,32.15,155.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-8.4474999999999995E-2,-5.6829999999999997E-3,0.06,3.333E-3,1.6140999999999999E-2,3000]
["$","2022-02-24","03:07:52","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:53","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:53.700","Surface Ops","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",3.0300000000000001E-2,2.0199999999999999E-2,6.7999999999999996E-3,0.21440000000000001]
["$","2022-02-24","03:07:53.700","Surface Ops","Radiometer post: SATFI40545",3.0300000000000001E-2,2.0199999999999999E-2,6.7999999999999996E-3,0.21440000000000001]
["$","2022-02-24","03:07:53.700","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,305.004,11.070,32.096,31.404,40.342,8.938,692.8,663.2,426.3  "]
["$","2022-02-24","03:07:53.800","Surface Ops","Optode post: 4330,2707,305.004,11.070,32.096,31.404,40.342,8.938,692.8,663.2,426.3  "]
["$","2022-02-24","03:07:53.700","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","03:07:53.700","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:53.700","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:54","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:54.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:54.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:54.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","03:07:54.700"]
["$","2022-02-24","03:07:54.600","Surface Ops","SBE41 Message",-0.08,44.826033000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.108695,-5.8690000000000001E-3,-0.03,1.4999999999999999E-2,1.5332E-2,3000]
["$","2022-02-24","03:07:55","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:56","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:57","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:57.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:57.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:57.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:57.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","03:07:57.800"]
["$","2022-02-24","03:07:57.800","Surface Ops","SBE41 Message",-0.09,44.843089999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.118794,-2.7330000000000002E-3,3.333E-3,-1.3332999999999999E-2,1.4529E-2,3000]
["$","2022-02-24","03:07:58","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:58","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.09,44.837879999999998,0.25,0,570.31140600000003,69727.835659999997,null,32.15,123.5,1429.2641799999999,6972.6492539999999,null,null,null,null,null,null,null,null,null,1217.3900149999999,12.3,38.584000000000003,12.3]
["$","2022-02-24","03:07:58.100","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:07:59.500","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:07:59.600","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:07:59.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:59.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:59.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:00.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:00.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:00.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:00.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","03:08:00.700"]
["$","2022-02-24","03:08:00.600","Surface Ops","SBE41 Message",-0.09,44.840736999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.111139,1.3960000000000001E-3,0,1.6670000000000001E-3,1.3724999999999999E-2,3000]
["$","2022-02-24","03:08:01.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:02.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:03.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:03.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:03.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:03.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:03.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","03:08:03.800"]
["$","2022-02-24","03:08:03.800","Surface Ops","SBE41 Message",-0.08,44.841365000000003,32.15,155.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-9.9902000000000005E-2,3.8670000000000002E-3,-3.333E-3,-1.6670000000000001E-3,1.2909E-2,3000]
["$","2022-02-24","03:08:04.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:05.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:05.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:05.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:06.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:06.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:06.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:06.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","03:08:06.700"]
["$","2022-02-24","03:08:06.600","Surface Ops","SBE41 Message",-0.12,44.836950999999999,32.15,155.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-9.6648999999999999E-2,3.6519999999999999E-3,1.3332999999999999E-2,5.0000000000000001E-3,1.2081E-2,3000]
["$","2022-02-24","03:08:07.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:08.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:08.600","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.12,44.836323999999998,0.25,0,570.31140600000003,69814.197809999998,null,32.15,121.5,1430.551811,6981.2854699999998,null,null,null,null,null,null,null,null,null,1217.4499510000001,12.31,38.563000000000002,12.31]
["$","2022-02-24","03:08:08.700","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:08:09.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:10.100","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:08:10.100","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:08:09.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:09.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:09.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.16]
["$","2022-02-24","03:08:10.200"]
["$","2022-02-24","03:08:09.800","Surface Ops","SBE41 Message",-0.16,44.836323999999998,32.15,155.5,null,null,null,null,null,null,null,null,-0.16,-0.16,-9.6406000000000006E-2,1.542E-3,1.3332999999999999E-2,1.3332999999999999E-2,1.1224E-2,3000]
["$","2022-02-24","03:08:10.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:11.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:11.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:11.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:12.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:12.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:12.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:12.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","03:08:12.700"]
["$","2022-02-24","03:08:12.600","Surface Ops","SBE41 Message",-0.1,44.832689000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-9.3483999999999998E-2,-7.5799999999999999E-4,-0.02,-3.333E-3,1.031E-2,3000]
["$","2022-02-24","03:08:13.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:14.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:15.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:15.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:15.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:15.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:15.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","03:08:15.800"]
["$","2022-02-24","03:08:15.800","Surface Ops","SBE41 Message",-0.14000000000000001,44.833925999999998,32.15,155.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-9.3195E-2,-1.903E-3,1.3332999999999999E-2,-3.333E-3,9.273E-3,3000]
["$","2022-02-24","03:08:16.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:16.900","Surface Ops","Starting Surface Optode and OCR Samples number 5 of 5"]
["$","2022-02-24","03:08:17.900","Surface Ops","SciLogger is writing previous sample before starting new one"]
["$","2022-02-24","03:08:17.900","Surface Ops","Wrote to msg file: AirCal:,2022-Feb-24T03:07:51Z,NaN,NaN,NaN,11.070,31.404,8.938,,,604,509,545,0.0303,0.0202,0.0068,0.2144  "]
["$","2022-02-24","03:08:17.900","Surface Ops","[ERROR] Missed CTD message 14"]
["$","2022-02-24","03:08:17.900","Surface Ops","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:08:18.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:18.900","Surface Ops","Sci Logger sending FastPressure to CTD"]
["$","2022-02-24","03:08:18.900","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:19","Surface Ops","Sci Logger sending sample Optode"]
["$","2022-02-24","03:08:19","Surface Ops","Sending Optode Do Sample"]
["$","2022-02-24","03:08:19","Surface Ops","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:08:19","Surface Ops","Sending radiometer pollSample"]
["$","2022-02-24","03:08:17.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:17.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:18","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:19.100","Surface Ops","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","03:08:18.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:18.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.01]
["$","2022-02-24","03:08:19.200"]
["$","2022-02-24","03:08:18.600","Surface Ops","SBE41 Message",-0.01,44.836128000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.01,-0.01,-0.101286,-1.681E-3,-4.3333000000000003E-2,-1.4999999999999999E-2,7.9369999999999996E-3,3000]
["$","2022-02-24","03:08:19.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:19.200","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.01,44.851562999999999,0.22500000000000001,0,570.31140600000003,69901.500140000004,null,32.15,136.5,1431.8452130000001,6990.015703,null,null,null,null,null,null,null,null,null,1217.469971,12.31,38.487000000000002,12.31]
["$","2022-02-24","03:08:19.300","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:08:20.700","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:08:20.700","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:08:20.800","Surface Ops","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",2.8500000000000001E-2,2.47E-2,6.4999999999999997E-3,0.22459999999999999]
["$","2022-02-24","03:08:20.800","Surface Ops","Radiometer post: SATFI40545",2.8500000000000001E-2,2.47E-2,6.4999999999999997E-3,0.22459999999999999]
["$","2022-02-24","03:08:19.900","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,307.327,10.893,32.091,31.399,40.336,8.937,692.2,662.9,431.9  "]
["$","2022-02-24","03:08:20.900","Surface Ops","Optode post: 4330,2707,307.327,10.893,32.091,31.399,40.336,8.937,692.2,662.9,431.9  "]
["$","2022-02-24","03:08:19.900","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","03:08:20.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:20.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:20.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:21.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:21.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:21.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","03:08:21.700"]
["$","2022-02-24","03:08:21.600","Surface Ops","SBE41 Message",-0.14000000000000001,44.832262,32.15,155.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.11433699999999999,-6.7000000000000002E-4,4.3333000000000003E-2,0,6.1190000000000003E-3,3000]
["$","2022-02-24","03:08:21.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:22.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:23.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:24.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:24.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:24.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:24.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","03:08:24.800"]
["$","2022-02-24","03:08:24.800","Surface Ops","SBE41 Message",-0.17,44.838577999999998,32.15,155.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-0.121716,5.4699999999999996E-4,0.01,2.6667E-2,4.3420000000000004E-3,3000]
["$","2022-02-24","03:08:24.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:25.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:26.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:26.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:26.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:27.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:27.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:27.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","03:08:27.700"]
["$","2022-02-24","03:08:27.600","Surface Ops","SBE41 Message",-0.14000000000000001,44.835521,32.15,155.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.11605699999999999,1.6739999999999999E-3,-0.01,0,2.6340000000000001E-3,3000]
["$","2022-02-24","03:08:27.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:28.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:29.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:30","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.14000000000000001,44.830483999999998,0.22500000000000001,0,570.31140600000003,69989.474029999998,null,32.15,127,1433.1702250000001,6998.8130920000003,null,null,null,null,null,null,null,null,null,1217.4499510000001,12.32,37.867001000000002,12.32]
["$","2022-02-24","03:08:30","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:08:30.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:31.400","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:08:31.500","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:08:30.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:30.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:30.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.06]
["$","2022-02-24","03:08:31.600"]
["$","2022-02-24","03:08:30.800","Surface Ops","SBE41 Message",-0.06,44.830483999999998,32.15,155.5,null,null,null,null,null,null,null,null,-0.06,-0.06,-0.103739,2.2759999999999998E-3,-2.6667E-2,-1.8332999999999999E-2,1.1199999999999999E-3,3000]
["$","2022-02-24","03:08:31.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:32.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:33.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:33.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:33.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:33.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:33.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.19]
["$","2022-02-24","03:08:33.700"]
["$","2022-02-24","03:08:33.600","Surface Ops","SBE41 Message",-0.19,44.832946999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.19,-0.19,-0.10134799999999999,1.707E-3,4.3333000000000003E-2,8.3330000000000001E-3,1.2400000000000001E-4,3000]
["$","2022-02-24","03:08:34.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:35.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:36.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:36.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:36.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:36.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:36.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","03:08:36.800"]
["$","2022-02-24","03:08:36.800","Surface Ops","SBE41 Message",-0.1,44.845024000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.11466800000000001,2.1100000000000001E-4,-0.03,6.6670000000000002E-3,-3.88E-4,3000]
["$","2022-02-24","03:08:37.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:38.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:38.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:38.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:39.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:39.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:39.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:39.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","03:08:39.700"]
["$","2022-02-24","03:08:39.600","Surface Ops","SBE41 Message",-0.05,44.841509000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-0.128332,-8.0400000000000003E-4,-1.6667000000000001E-2,-2.3333E-2,-5.1599999999999997E-4,3000]
["$","2022-02-24","03:08:40.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:40.600","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.05,44.840778999999998,0.22500000000000001,0,570.31140600000003,70076.776360000003,null,32.15,121.5,1434.475563,7007.5433249999996,null,null,null,null,null,null,null,null,null,1217.5200199999999,12.32,38.167000000000002,12.32]
["$","2022-02-24","03:08:40.700","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:08:42.100","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:08:42.100","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:08:42.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:42.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:42.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:42.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:42.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","03:08:42.800"]
["$","2022-02-24","03:08:42.800","Surface Ops","SBE41 Message",-0.14000000000000001,44.843020000000003,32.15,155.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.12953400000000001,-3.9800000000000002E-4,0.03,6.6670000000000002E-3,-4.8000000000000001E-4,3000]
["$","2022-02-24","03:08:43.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:44","Surface Ops","Surface sampling finished"]
["$","2022-02-24","03:08:44","Surface Ops","[MSC] Starting config data collection."]
["$","2022-02-24","03:08:44.100","Surface Ops","[MSC] TX: W"]
["$","2022-02-24","03:08:44.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:44.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:44.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:45.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:45.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:45.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:45.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","03:08:45.700"]
["$","2022-02-24","03:08:45.600","Surface Ops","SBE41 Message",-7.0000000000000007E-2,44.839143999999997,32.15,155.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.124518,9.2000000000000003E-4,-2.3333E-2,3.333E-3,-4.1100000000000002E-4,3000]
["$","2022-02-24","03:08:46.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:47","Surface Ops","[MSC] Timeout for CommandWake"]
["$","2022-02-24","03:08:47.100","Surface Ops","[MSC] TX: W"]
["$","2022-02-24","03:08:47.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:47.200","Surface Ops","[MSC] RX: "]
["$","2022-02-24","03:08:48.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:48.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:48.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:48.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:48.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","03:08:48.800"]
["$","2022-02-24","03:08:48.800","Surface Ops","SBE41 Message",-0.17,44.836244000000001,32.15,155.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-0.11884,2E-3,3.3333000000000002E-2,5.0000000000000001E-3,-3.4299999999999999E-4,3000]
["$","2022-02-24","03:08:49.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:50.100","Surface Ops","[MSC] Timeout for CommandWake"]
["$","2022-02-24","03:08:50.100","Surface Ops","[MSC] TX: W"]
["$","2022-02-24","03:08:50.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:50.200","Surface Ops","[MSC] RX: ACK  "]
["$","2022-02-24","03:08:50.300","Surface Ops","[MSC] TX: MODE,1"]
["$","2022-02-24","03:08:50.500","Surface Ops","[MSC] RX: ACK,MODE,1  "]
["$","2022-02-24","03:08:50.600","Surface Ops","[MSC] TX: ACK "]
["$","2022-02-24","03:08:50.600","Surface Ops","[MSC] TX: C"]
["$","2022-02-24","03:08:50.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:50.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:50.800","Surface Ops","[MSC] RX: H, Datalogger Serial Num , SN:0003  "]
["$","2022-02-24","03:08:50.900","Surface Ops","[MSC] RX: H, Application      Name , CPF_MAIN.C  "]
["$","2022-02-24","03:08:50.900","Surface Ops","[MSC] RX: H, App Build        Date , Nov 20 2020, 13:19:41  "]
["$","2022-02-24","03:08:51","Surface Ops","[MSC] RX: H, Power Up Time   (GMT) , 02/24/2022 00:57:06  "]
["$","2022-02-24","03:08:51","Surface Ops","[MSC] RX: H, Current  Time   (GMT) , 02/24/2022 03:08:50  "]
["$","2022-02-24","03:08:51.100","Surface Ops","[MSC] RX: H, Alarm    Time   (GMT) , 02/24/2022 10:57:11  "]
["$","2022-02-24","03:08:51.100","Surface Ops","[MSC] RX: H, Power Active  Timeout , 10  "]
["$","2022-02-24","03:08:51.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:51.100","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.17,44.841253000000002,0.2,0,570.31140600000003,70163.272830000002,null,32.15,130.5,1435.831005,7016.1929710000004,null,null,null,null,null,null,null,null,null,1217.5,12.33,38.354999999999997,12.33]
["$","2022-02-24","03:08:51.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:51.200","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:08:52.700","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:08:52.700","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:08:52.700","Surface Ops","[MSC] RX: H, Persistor CF2-1M Info , S/N:15079 - BIOS:4.03 - PicoDOS:4.03  "]
["$","2022-02-24","03:08:52.700","Surface Ops","[MSC] RX: H, Compact FLASH    Size , 256614400  "]
["$","2022-02-24","03:08:52.700","Surface Ops","[MSC] RX: H, Compact FLASH    Left , 90.92%  "]
["$","2022-02-24","03:08:51.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:52.800","Surface Ops","[MSC] RX: H, Power Cycle   Counter , 6  "]
["$","2022-02-24","03:08:52.800","Surface Ops","[MSC] RX: H, System Reset  Counter , 6  "]
["$","2022-02-24","03:08:52.800","Surface Ops","[MSC] RX: H, System Error  Counter , 0  "]
["$","2022-02-24","03:08:52.800","Surface Ops","[MSC] RX: H, Last System     Error , 0  "]
["$","2022-02-24","03:08:52.800","Surface Ops","[MSC] RX: H, Last System ErrorTime , 01/01/1970 00:00:00  "]
["$","2022-02-24","03:08:52.900","Surface Ops","[MSC] RX: H, ISUS  Error   Counter , 0  "]
["$","2022-02-24","03:08:52.900","Surface Ops","[MSC] RX: H, Last ISUS       Error , 0  "]
["$","2022-02-24","03:08:52.900","Surface Ops","[MSC] RX: H, Last ISUS Error  Time , 01/01/1970 00:00:00  "]
["$","2022-02-24","03:08:52.900","Surface Ops","[MSC] RX: H, ISUS Sample   Counter , 66  "]
["$","2022-02-24","03:08:52.900","Surface Ops","[MSC] RX: H, Last Sample Rec. Time , 02/24/2022 03:04:12  "]
["$","2022-02-24","03:08:51.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","03:08:53"]
["$","2022-02-24","03:08:51.600","Surface Ops","SBE41 Message",-0.14000000000000001,44.841253000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.10957600000000001,1.91E-3,-0.01,1.1667E-2,-2.8699999999999998E-4,3000]
["$","2022-02-24","03:08:53","Surface Ops","[MSC] RX: H, Fiberlite    Odometer , 05:24:28  "]
["$","2022-02-24","03:08:53","Surface Ops","[MSC] RX: H, Fiberlite      Cycles , 7430  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Spec Intensity LampON , 5000  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Spec Integration Time , 375  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Spec Pre  scans taken , 2  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Spec Lite scans taken , 3  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Spec Dark scans taken , 1  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Calibration      Date , 11/24/2020  "]
["$","2022-02-24","03:08:53.200","Surface Ops","[MSC] RX: H, Sw Calibration   Temp , 19.94  "]
["$","2022-02-24","03:08:53.200","Surface Ops","[MSC] RX: H, Wavelength Fit  Range , 217.295 <-> 239.828  "]
["$","2022-02-24","03:08:53.200","Surface Ops","[MSC] RX: H, Pixel Fit       Range , 36 <-> 64  "]
["$","2022-02-24","03:08:53.200","Surface Ops","[MSC] RX: H, Fitted Concentrations , 2  "]
["$","2022-02-24","03:08:53.200","Surface Ops","[MSC] RX: H, Baseline        Model , (ax + b)  "]
["$","2022-02-24","03:08:53.300","Surface Ops","[MSC] RX: H, Br Temp  Compensation , ENABLED  "]
["$","2022-02-24","03:08:53.300","Surface Ops","[MSC] RX: H, Bromide Term in Model , will be FIXED (to external CTD value)  "]
["$","2022-02-24","03:08:53.300","Surface Ops","[MSC] RX: H, Zeiss Coefficient Vals, 1.885090e+02,7.959960e-01,1.113850e-04,-3.090260e-07,0.000000e+00  "]
["$","2022-02-24","03:08:53.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:54.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:54.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:54.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:54.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:54.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","03:08:54.800"]
["$","2022-02-24","03:08:54.800","Surface Ops","SBE41 Message",-0.1,44.833660999999999,32.15,155.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.10148,4.1599999999999997E-4,-1.3332999999999999E-2,-1.1667E-2,-2.5099999999999998E-4,3000]
["$","2022-02-24","03:08:55.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:56.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:56.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:56.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:57.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:57.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:57.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:57.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","03:08:57.700"]
["$","2022-02-24","03:08:57.600","Surface Ops","SBE41 Message",-0.12,44.842804999999998,32.15,155.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.10377,-1.518E-3,6.6670000000000002E-3,-3.333E-3,-2.33E-4,3000]
["$","2022-02-24","03:08:58.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:59.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:00.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:00.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:00.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:00.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:00.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","03:09:00.800"]
["$","2022-02-24","03:09:00.800","Surface Ops","SBE41 Message",-0.15,44.837401,32.15,155.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-0.11532299999999999,-2.4039999999999999E-3,0.01,8.3330000000000001E-3,-2.2100000000000001E-4,3000]
["$","2022-02-24","03:09:00.900","Surface Ops","[MSC] TX: SE,?"]
["$","2022-02-24","03:09:01.100","Surface Ops","[MSC] RX: ACK,SE?,0  "]
["$","2022-02-24","03:09:01.100","Surface Ops","[MSC] ERRORS AVAILABLE: 0"]
["$","2022-02-24","03:09:01.100","Surface Ops","[MSC] TX: W"]
["$","2022-02-24","03:09:01.200","Surface Ops","[MSC] RX: ACK  "]
["$","2022-02-24","03:09:01.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:01.300","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.15,44.838766999999997,0.2,0,570.31140600000003,70246.545819999999,null,32.15,133.5,1437.1638869999999,7024.5202710000003,null,null,null,null,null,null,null,null,null,1217.469971,12.33,38.577998999999998,12.33]
["$","2022-02-24","03:09:01.400","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:09:02.800","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:09:02.800","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:09:02.800","Surface Ops","[MSC] TX: MODE,2"]
["$","2022-02-24","03:09:02.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:02.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:09:02.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:03.100","Surface Ops","[MSC] RX: ACK,MODE,2  "]
["$","2022-02-24","03:09:03.100","Surface Ops","[MSC] TX: ACK "]
["$","2022-02-24","03:09:03.100","Surface Ops","[MSC] TX: C"]
["$","2022-02-24","03:09:03.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:03.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:03.400","Surface Ops","[MSC] RX: H, Datalogger Serial Num , SN:0003  "]
["$","2022-02-24","03:09:03.400","Surface Ops","[MSC] RX: H, Application      Name , CPF_MAIN.C  "]
["$","2022-02-24","03:09:03.500","Surface Ops","[MSC] RX: H, App Build        Date , Nov 20 2020, 13:19:41  "]
["$","2022-02-24","03:09:03.500","Surface Ops","[MSC] RX: H, Power Up Time   (GMT) , 02/24/2022 00:57:06  "]
["$","2022-02-24","03:09:03.500","Surface Ops","[MSC] RX: H, Current  Time   (GMT) , 02/24/2022 03:09:03  "]
["$","2022-02-24","03:09:03.600","Surface Ops","[MSC] RX: H, Alarm    Time   (GMT) , 02/24/2022 10:57:11  "]
["$","2022-02-24","03:09:03.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","03:09:03.700"]
["$","2022-02-24","03:09:03.600","Surface Ops","SBE41 Message",-7.0000000000000007E-2,44.826835000000003,32.15,155.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.126138,-1.745E-3,-2.6667E-2,-8.3330000000000001E-3,-1.93E-4,3000]
["$","2022-02-24","03:09:03.700","Surface Ops","[MSC] RX: H, Power Active  Timeout , 10  "]
["$","2022-02-24","03:09:03.800","Surface Ops","[MSC] RX: H, Persistor CF2-1M Info , S/N:15079 - BIOS:4.03 - PicoDOS:4.03  "]
["$","2022-02-24","03:09:03.800","Surface Ops","[MSC] RX: H, Compact FLASH    Size , 256614400  "]
["$","2022-02-24","03:09:03.800","Surface Ops","[MSC] RX: H, Compact FLASH    Left , 90.92%  "]
["$","2022-02-24","03:09:03.800","Surface Ops","[MSC] RX: H, Power Cycle   Counter , 6  "]
["$","2022-02-24","03:09:03.800","Surface Ops","[MSC] RX: H, System Reset  Counter , 6  "]
["$","2022-02-24","03:09:03.900","Surface Ops","[MSC] RX: H, System Error  Counter , 0  "]
["$","2022-02-24","03:09:03.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:03.900","Surface Ops","[MSC] RX: H, Last System     Error , 0  "]
["$","2022-02-24","03:09:04","Surface Ops","[MSC] RX: H, Last System ErrorTime , 01/01/1970 00:00:00  "]
["$","2022-02-24","03:09:04","Surface Ops","[MSC] RX: H, DURA  Error   Counter , 0  "]
["$","2022-02-24","03:09:04","Surface Ops","[MSC] RX: H, Last DURA       Error , 0  "]
["$","2022-02-24","03:09:04.100","Surface Ops","[MSC] RX: H, Last DURA Error  Time , 01/01/1970 00:00:00  "]
["$","2022-02-24","03:09:04.100","Surface Ops","[MSC] RX: H, DURA Sample   Counter , 66  "]
["$","2022-02-24","03:09:04.200","Surface Ops","[MSC] RX: H, Last Sample Rec. Time , 02/24/2022 03:04:21  "]
["$","2022-02-24","03:09:04.200","Surface Ops","[MSC] RX: H, AtoD Reads per Sample , 10  "]
["$","2022-02-24","03:09:04.200","Surface Ops","[MSC] RX: H, AtoD Reading    Delay , 100  "]
["$","2022-02-24","03:09:04.300","Surface Ops","[MSC] RX: H, Samps per AtoD  Recal , 250  "]
["$","2022-02-24","03:09:04.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:05.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:06.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:06.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:06.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:06.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.13]
["$","2022-02-24","03:09:06.800"]
["$","2022-02-24","03:09:06.800","Surface Ops","SBE41 Message",-0.13,44.833951999999996,32.15,155.5,null,null,null,null,null,null,null,null,-0.13,-0.13,-0.12845000000000001,-1.9699999999999999E-4,0.02,-3.333E-3,-1.4799999999999999E-4,3000]
["$","2022-02-24","03:09:06.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:07.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:08.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:08.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:09:08.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:09.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:09.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:09.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","03:09:09.700"]
["$","2022-02-24","03:09:09.600","Surface Ops","SBE41 Message",0,44.836542000000001,32.15,155.5,null,null,null,null,null,null,null,null,0,0,-0.124519,1.343E-3,-4.3333000000000003E-2,-1.1667E-2,-9.5000000000000005E-5,3000]
["$","2022-02-24","03:09:09.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:10.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:11.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:11.900","Surface Ops","System Data (dBar %full Volts mAmps): ",0,44.847689000000003,0.2,0,570.31140600000003,70333.579530000003,null,32.15,135,1438.5552680000001,7033.2236419999999,null,null,null,null,null,null,null,null,null,1217.4499510000001,12.34,37.681998999999998,12.34]
["$","2022-02-24","03:09:12","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:09:12.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:13.400","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:09:13.400","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:09:12.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:12.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:12.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","03:09:13.500"]
["$","2022-02-24","03:09:12.800","Surface Ops","SBE41 Message",-0.09,44.847689000000003,32.15,155.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.120277,2.137E-3,0.03,-6.6670000000000002E-3,-3.6999999999999998E-5,3000]
["$","2022-02-24","03:09:13.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:13.600","Surface Ops","[MSC] TX: SE,?"]
["$","2022-02-24","03:09:13.800","Surface Ops","[MSC] RX: ACK,SE?,0  "]
["$","2022-02-24","03:09:13.800","Surface Ops","[MSC] ERRORS AVAILABLE: 0"]
["$","2022-02-24","03:09:13.800","Surface Ops","IModem Sending SBDD2 cmd"]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->  <--  "]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->0  <--  "]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:09:14","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->  <--  "]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OK  "]
["$","2022-02-24","03:09:14","Surface Ops","IModem correct response: IModem Looking for IModem-->OK<--  IModem Got-->OK  <--  "]
["$","2022-02-24","03:09:14","Surface Ops","IModem Sending CREG cmd"]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem invalid response: IModem Looking for IModem-->+CREG:<--  IModem Got-->  <--  "]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+CREG:000,001  "]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem correct response: IModem Looking for IModem-->+CREG:<--  IModem Got-->+CREG:000,001  <--  "]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OK  "]
["$","2022-02-24","03:09:15.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:17.200","Surface Ops","Trying GPS get position try num: 0 of 2",-0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UBX,00,030917.00,3652.73138,N,12156.35823,W,-34.383,G3,4.7,5.8,1.771,83.14,-0.222,,1.26,2.07,1.52,7,0,0*70  "]
["$","2022-02-24","03:09:17.300","Surface Ops","Got Position: lat = 3652.73138","N  lon = 12156.35823","W   num sats = 7"]
["$","2022-02-24","03:09:17.300","Surface Ops","Succesful GPS getPosition"]
["$","2022-02-24","03:09:15.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:15.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:15.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","03:09:17.400"]
["$","2022-02-24","03:09:15.600","Surface Ops","SBE41 Message",-7.0000000000000007E-2,44.834071999999999,32.15,155.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.114066,1.7960000000000001E-3,-6.6670000000000002E-3,1.1667E-2,2.4000000000000001E-5,3000]
["$","2022-02-24","03:09:17.400","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:17.400","Surface Ops","Ending SciLogger Sample Cycle"]
["$","2022-02-24","03:09:17.400","Surface Ops","SciLogger endSampleCycle is writing samples"]
["$","2022-02-24","03:09:17.500","Surface Ops","Wrote to msg file: AirCal:,2022-Feb-24T03:08:19Z,NaN,NaN,NaN,10.893,31.399,8.937,,,604,509,545,0.0285,0.0247,0.0065,0.2246  "]
["$","2022-02-24","03:09:17.500","Surface Ops","[ERROR] Missed CTD message 15"]

{"sheet":"Copy of all data","index":1,"n_rows":32198,"n_cols":52,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["$","Date","Time","State","Comment","Pressure","BelPos","PumpVolts","PumpMilliamps","PumpoCoulombs","PumpJoules","PumpMotor","HotelVolts","HotelMilliamps","HotelCoulombs","HotelJoules","CTDTemp","CTDSal","RawPress","LPFPress","LPFVel","DiffVel","Diff2 Vel","SlopeLPFPress.","CTDSamplePeriod","LPS331Press","LPS331Temp","SHT21Humid","SHT21Temp","pidSP","pidPV","pidY1","pidY2","pidI","pid_v","pid_u","pid_uCPS","pid_h","FLBB","Topt","Tphase","Rphase","NO3","pHVrs","OCRtext","OCRCh1","OCRCh2","OCRCh3","OCRCH4","GPS","IridModem","MSC"]
["$","2022-02-24","00:45:43","Surface Ops","Opened new engr log file: \\SD\\data\\2022-2-23T16-59-6\\CPF003.004.eng"]
["$","2022-02-24","00:45:43.100","Surface Ops","Opening new .dura file: \\SD\\data\\2022-2-23T16-59-6\\CPF003.004.dura"]
["$","2022-02-24","00:45:43.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:43.600","Surface Ops","Opening new .isus file: \\SD\\data\\2022-2-23T16-59-6\\CPF003.004.isus"]
["$","2022-02-24","00:45:43.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:43.700","Surface Ops","Skipping over SendFilesViaRudics"]
["$","2022-02-24","00:45:43.700","Surface Ops","2022-02-24T00:45:43Z,,Lat,3652.79313","N,,Lon,12156.36559","W,GPS TOF,004542.00,Num Sats,5,Surface Ops,Console set SV.ForceRecoveryState false,ProfileNum,3,NAK SBD,SQ,5,MO Stat,-,,Mission TO,02:00:00,Park Time,02:00:00,Park P,85,Prof Num,3 of 20,Max P,-100.000,BBVolts,32.375,Can P,1218.1,Can Hum,38.8,BBHealth,0FFF"]
["$","2022-02-24","00:45:43.700","Surface Ops","IModem Sending SBDWT cmd"]
["$","2022-02-24","00:45:43.700","Surface Ops","Sent SBDWT Command"]
["$","2022-02-24","00:45:43.800","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","00:45:43.800","Surface Ops","IModem invalid response: IModem Looking for IModem-->READY<--  IModem Got-->  <--  "]
["$","2022-02-24","00:45:43.800","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"READY  "]
["$","2022-02-24","00:45:43.800","Surface Ops","IModem correct response: IModem Looking for IModem-->READY<--  IModem Got-->READY  <--  "]
["$","2022-02-24","00:45:43.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:45:43.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","00:45:43.900","Surface Ops","IModem Sending loadSBDWT cmd"]
["$","2022-02-24","00:45:44.100","Surface Ops","IModem Loaded SBDWT Buffer with->2022-02-24T00:45:43Z,,Lat,3652.79313","N,,Lon,12156.36559","W,GPS TOF,004542.00,Num Sats,5,Surface Ops,Console set SV.ForceRecoveryState false,ProfileNum,3,NAK SBD,SQ,5,MO Stat,-,,Mission TO,02:00:00,Park Time,02:00:00,Park P,85,Prof Num,3 of 20,Max P,-100.000,BBVolts,32.375,Can P,1218.1,Can Hum,38.8,BBHealth,0FFF<-"]
["$","2022-02-24","00:45:44.300","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","00:45:44.300","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->  <--  "]
["$","2022-02-24","00:45:44.300","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","00:45:44.400","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->0  <--  "]
["$","2022-02-24","00:45:44.300","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","00:45:44.400","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->  <--  "]
["$","2022-02-24","00:45:44.300","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OK  "]
["$","2022-02-24","00:45:44.400","Surface Ops","IModem correct response: IModem Looking for IModem-->OK<--  IModem Got-->OK  <--  "]
["$","2022-02-24","00:45:44.400","Surface Ops","IModem Sending SBDIX cmd"]
["$","2022-02-24","00:45:44.500","Surface Ops","IModem Sent SBDIX Command"]
["$","2022-02-24","00:45:44.700","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:45.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:45:45.200","Surface Ops","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:45:45.700","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:46.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:46.700","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:46.700","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:45:47","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.06]
["$","2022-02-24","00:45:47","Surface Ops","SBE41 Message",0.06,44.822620999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.06,0.06,-0.128243,-3.7529999999999998E-3,-8.6666999999999994E-2,-1.3332999999999999E-2,-1.95E-4,3000]
["$","2022-02-24","00:45:47.700","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:47.700","Surface Ops","System Data (dBar %full Volts mAmps): ",0.06,44.833466999999999,0.2,0,614.53313200000002,70487.231639999998,null,32.375,146,1443.958674,7048.5754209999996,null,null,null,null,null,null,null,null,null,1218.099976,12.48,37.881999999999998,12.48]
["$","2022-02-24","00:45:47.800","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","00:45:49.200","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","00:45:49.200","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","00:45:49.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:49.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:49.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:45:49.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:45:50.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.24]
["$","2022-02-24","00:45:50.200","Surface Ops","SBE41 Message",-0.24,44.83381,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.24,-0.24,-0.13390099999999999,-4.4710000000000001E-3,0.1,6.6670000000000002E-3,-1.6200000000000001E-4,3000]
["$","2022-02-24","00:45:50.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:51.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:52","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:45:52","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:45:52.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:52.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:52.700","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:45:53.100","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.16]
["$","2022-02-24","00:45:53.100","Surface Ops","SBE41 Message",-0.16,44.822532000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.16,-0.16,-0.124348,-2.8059999999999999E-3,-2.6667E-2,3.6666999999999998E-2,-1.4300000000000001E-4,3000]
["$","2022-02-24","00:45:53.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:54.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:55.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:55.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:55.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:45:55.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:45:56.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:45:56.200","Surface Ops","SBE41 Message",-0.09,44.830872999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.10817400000000001,-4.1599999999999997E-4,-2.3333E-2,-2.5000000000000001E-2,-1.6000000000000001E-4,3000]
["$","2022-02-24","00:45:56.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:57.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","00:45:57.500","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","00:45:57.600","Surface Ops","IModem got invalid SBDIX response:   "]
["$","2022-02-24","00:45:57.600","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+SBDIX: 0, 0, 0, 0, 0, 0  "]
["$","2022-02-24","00:45:57.600","Surface Ops","IModem SBDIX Response: +SBDIX: 0, 0, 0, 0, 0, 0     sbdixMOStatus = 0   sbdixMTStatus = 0   sbdixMTQueued = 0"]
["$","2022-02-24","00:45:57.600","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","00:45:57.600","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OK  "]
["$","2022-02-24","00:45:57.700","Surface Ops","IModem SBDIX try num: 1"]
["$","2022-02-24","00:45:58.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:45:58.700","Surface Ops","Sending Elmo Echo Off command"]
["$","2022-02-24","00:46:00.700","Surface Ops","Setting Elmo current and acc limits"]
["$","2022-02-24","00:46:00.700","Surface Ops","Setting Elmo Acceleration limit = AC[1]=1e9;"]
["$","2022-02-24","00:46:00.700","Surface Ops","Setting Elmo Deacceleration limit = DC=1e9;"]
["$","2022-02-24","00:46:00.700","Surface Ops","Sending Elmo CL[1]=4.76 command"]
["$","2022-02-24","00:46:01.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:46:01.700","Surface Ops","Sending Elmo PL1[1]=13.5 command"]
["$","2022-02-24","00:46:02.700","Surface Ops","Sending Elmo PL2[1]=2 command"]
["$","2022-02-24","00:46:04.100","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:04.100","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:04.600","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","00:46:06.600","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:06.600","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:06.600","Surface Ops","Normal State Exit"]
["$","2022-02-24","00:46:06.600","Init Profile","Setting Execution Constraint = 600000"]
["$","2022-02-24","00:46:06.600","Init Profile","State Entry"]
["$","2022-02-24","00:45:58","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:45:58","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:45:58.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:45:59","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:45:59","Init Profile","SBE41 Message",-0.12,44.83719,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-9.9048999999999998E-2,5.6599999999999999E-4,0.01,-6.6670000000000002E-3,-2.12E-4,3000]
["$","2022-02-24","00:46:01","Init Profile","Twitter msg"]
["$","2022-02-24","00:46:01","Init Profile","Twitter msg",null,null,null,null,null,null,"\u0002?;"]
["$","2022-02-24","00:46:01","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1]=4.76;"]
["$","2022-02-24","00:46:01","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:01.700","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1]=13.5;"]
["$","2022-02-24","00:46:01.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:01.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:01.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:02.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:46:02.200","Init Profile","SBE41 Message",-0.12,44.83719,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.107136,-5.6499999999999996E-4,0,5.0000000000000001E-3,-2.7700000000000001E-4,3000]
["$","2022-02-24","00:46:02.700","Init Profile","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:02.700","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:02.900","Init Profile","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:02.900","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:03.100","Init Profile","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:03.100","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:03.300","Init Profile","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:03.300","Init Profile","Twitter msg",null,null,null,null,null,null,"33603584;"]
["$","2022-02-24","00:46:03.500","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:03.500","Init Profile","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:03.700","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:03.700","Init Profile","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:03.900","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:03.900","Init Profile","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:04.200","Init Profile","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:04.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:04.200","Init Profile","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:04.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:04.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:04.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:05.200","Init Profile","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:05.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.18]
["$","2022-02-24","00:46:05.200","Init Profile","SBE41 Message",-0.18,44.83719,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.18,-0.18,-0.12615899999999999,-2.16E-3,0.02,0.01,-3.2499999999999999E-4,3000]
["$","2022-02-24","00:46:05.200","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:05.400","Init Profile","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:05.400","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:05.600","Init Profile","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:05.600","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:05.800","Init Profile","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:05.800","Init Profile","Twitter msg",null,null,null,null,null,null,"33603584;"]
["$","2022-02-24","00:46:06","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:06","Init Profile","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:06.200","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:06.200","Init Profile","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:06.400","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:06.400","Init Profile","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:07.700","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:46:06.600","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:46:06.700","Init Profile","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:07.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:07.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:08.100","Init Profile","Initializing SBE 41 LPF"]
["$","2022-02-24","00:46:08.100","Init Profile","[MSC] Powering up MSC"]
["$","2022-02-24","00:46:08.100","Init Profile","[MSC] Resetting Sequencers"]
["$","2022-02-24","00:46:08.100","Init Profile","Sending SBE41 stopProfile"]
["$","2022-02-24","00:46:09.100","Init Profile","Power cycling SBE41"]
["$","2022-02-24","00:46:09.100","Init Profile","Power Cycling SBE41"]
["$","2022-02-24","00:46:09.100","Init Profile","Powering Down CTD"]
["$","2022-02-24","00:46:10.200","Init Profile","Powering Up CTD"]
["$","2022-02-24","00:46:10.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:11.200","Init Profile","Profile number = 4"]
["$","2022-02-24","00:46:11.200","Init Profile","Writing Header to msg File"]
["$","2022-02-24","00:46:11.600","Init Profile","[MSC] Starting config data collection."]
["$","2022-02-24","00:46:08.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>stopprofile  "]
["$","2022-02-24","00:46:09.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:10.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:11","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.19]
["$","2022-02-24","00:46:11","Init Profile","SBE41 Message",-0.19,44.83719,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.19,-0.19,-0.18,0,3.333E-3,1.6670000000000001E-3,0,3000]
["$","2022-02-24","00:46:11.700","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:11.700","Init Profile","System Data (dBar %full Volts mAmps): ",-0.19,44.826158999999997,32.375,10,2.4920999999999999E-2,29.951415999999998,null,32.375,175.5,0.62866599999999995,2.9817100000000001,null,null,null,null,null,null,null,null,null,1218.0500489999999,12.49,38.180999999999997,12.49]
["$","2022-02-24","00:46:11.800","Init Profile","Pump motor not faulted"]
["$","2022-02-24","00:46:13.200","Init Profile","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:13.200","Init Profile","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:13.300","Init Profile","[MSC] TX: W"]
["$","2022-02-24","00:46:11.800","Init Profile","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:11.800","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:12","Init Profile","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:12","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:12.200","Init Profile","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:12.200","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:12.400","Init Profile","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:12.400","Init Profile","Twitter msg",null,null,null,null,null,null,"33604352;"]
["$","2022-02-24","00:46:12.600","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:12.600","Init Profile","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:12.800","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:12.800","Init Profile","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:12.900","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:12.900","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:13","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:13","Init Profile","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:13.200","Init Profile","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:13.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:13.200","Init Profile","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:13.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:13.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:13.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:13.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:14.100","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.18]
["$","2022-02-24","00:46:14.100","Init Profile","SBE41 Message",-0.18,44.829211000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.18,-0.18,-0.18002099999999999,0,-3.333E-3,0,0,3000]
["$","2022-02-24","00:46:14.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:15.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:16.200","Init Profile","[MSC] Timeout for CommandWake"]
["$","2022-02-24","00:46:16.300","Init Profile","[MSC] TX: W"]
["$","2022-02-24","00:46:16.400","Init Profile","[MSC] RX: "]
["$","2022-02-24","00:46:16.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:16.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:16.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:16.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:17.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:46:17.200","Init Profile","SBE41 Message",-0.14000000000000001,44.835759000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.18024000000000001,-1.9999999999999999E-6,-1.3332999999999999E-2,-8.3330000000000001E-3,0,3000]
["$","2022-02-24","00:46:17.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:18.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:19","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:19","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:19.300","Init Profile","[MSC] Timeout for CommandWake"]
["$","2022-02-24","00:46:19.300","Init Profile","[MSC] TX: W"]
["$","2022-02-24","00:46:19.400","Init Profile","[MSC] RX: ACK  "]
["$","2022-02-24","00:46:19.500","Init Profile","[MSC] TX: RTC,1645663579"]
["$","2022-02-24","00:46:19.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:19.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:19.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:19.800","Init Profile","[MSC] RX: ACK,RTC,1645663579,1645663579  "]
["$","2022-02-24","00:46:19.800","Init Profile","[MSC] TX: ACK "]
["$","2022-02-24","00:46:19.800","Init Profile","[MSC] TX: MODE,1"]
["$","2022-02-24","00:46:20.100","Init Profile","[MSC] RX: ACK,MODE,1  "]
["$","2022-02-24","00:46:20.100","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:46:20.100","Init Profile","SBE41 Message",-0.12,44.832031999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.18093600000000001,-9.9999999999999995E-7,-6.6670000000000002E-3,-0.01,9.9999999999999995E-7,3000]
["$","2022-02-24","00:46:20.100","Init Profile","[MSC] TX: ACK "]
["$","2022-02-24","00:46:20.200","Init Profile","[MSC] TX: C"]
["$","2022-02-24","00:46:20.400","Init Profile","[MSC] RX: H, Datalogger Serial Num , SN:0003  "]
["$","2022-02-24","00:46:20.500","Init Profile","[MSC] RX: H, Application      Name , CPF_MAIN.C  "]
["$","2022-02-24","00:46:20.500","Init Profile","[MSC] RX: H, App Build        Date , Nov 20 2020, 13:19:41  "]
["$","2022-02-24","00:46:20.600","Init Profile","[MSC] RX: H, Power Up Time   (GMT) , 02/23/2022 22:32:51  "]
["$","2022-02-24","00:46:20.600","Init Profile","[MSC] RX: H, Current  Time   (GMT) , 02/24/2022 00:46:19  "]
["$","2022-02-24","00:46:20.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:20.700","Init Profile","[MSC] RX: H, Alarm    Time   (GMT) , 02/24/2022 08:32:56  "]
["$","2022-02-24","00:46:20.700","Init Profile","[MSC] RX: H, Power Active  Timeout , 10  "]
["$","2022-02-24","00:46:20.800","Init Profile","[MSC] RX: H, Persistor CF2-1M Info , S/N:15079 - BIOS:4.03 - PicoDOS:4.03  "]
["$","2022-02-24","00:46:20.800","Init Profile","[MSC] RX: H, Compact FLASH    Size , 256614400  "]
["$","2022-02-24","00:46:20.800","Init Profile","[MSC] RX: H, Compact FLASH    Left , 90.94%  "]
["$","2022-02-24","00:46:20.900","Init Profile","[MSC] RX: H, Power Cycle   Counter , 5  "]
["$","2022-02-24","00:46:20.900","Init Profile","[MSC] RX: H, System Reset  Counter , 5  "]
["$","2022-02-24","00:46:20.900","Init Profile","[MSC] RX: H, System Error  Counter , 0  "]
["$","2022-02-24","00:46:21","Init Profile","[MSC] RX: H, Last System     Error , 0  "]
["$","2022-02-24","00:46:21","Init Profile","[MSC] RX: H, Last System ErrorTime , 01/01/1970 00:00:00  "]
["$","2022-02-24","00:46:21.100","Init Profile","[MSC] RX: H, ISUS  Error   Counter , 0  "]
["$","2022-02-24","00:46:21.100","Init Profile","[MSC] RX: H, Last ISUS       Error , 0  "]
["$","2022-02-24","00:46:21.100","Init Profile","[MSC] RX: H, Last ISUS Error  Time , 01/01/1970 00:00:00  "]
["$","2022-02-24","00:46:21.200","Init Profile","[MSC] RX: H, ISUS Sample   Counter , 46  "]
["$","2022-02-24","00:46:21.200","Init Profile","[MSC] RX: H, Last Sample Rec. Time , 02/24/2022 00:40:20  "]
["$","2022-02-24","00:46:21.300","Init Profile","[MSC] RX: H, Fiberlite    Odometer , 05:23:43  "]
["$","2022-02-24","00:46:21.300","Init Profile","[MSC] RX: H, Fiberlite      Cycles , 7410  "]
["$","2022-02-24","00:46:21.300","Init Profile","[MSC] RX: H, Spec Intensity LampON , 5000  "]
["$","2022-02-24","00:46:21.400","Init Profile","[MSC] RX: H, Spec Integration Time , 375  "]
["$","2022-02-24","00:46:21.400","Init Profile","[MSC] RX: H, Spec Pre  scans taken , 2  "]
["$","2022-02-24","00:46:21.400","Init Profile","[MSC] RX: H, Spec Lite scans taken , 3  "]
["$","2022-02-24","00:46:21.500","Init Profile","[MSC] RX: H, Spec Dark scans taken , 1  "]
["$","2022-02-24","00:46:21.500","Init Profile","[MSC] RX: H, Calibration      Date , 11/24/2020  "]
["$","2022-02-24","00:46:21.500","Init Profile","[MSC] RX: H, Sw Calibration   Temp , 19.94  "]
["$","2022-02-24","00:46:21.600","Init Profile","[MSC] RX: H, Wavelength Fit  Range , 217.295 <-> 239.828  "]
["$","2022-02-24","00:46:21.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:21.600","Init Profile","[MSC] RX: H, Pixel Fit       Range , 36 <-> 64  "]
["$","2022-02-24","00:46:21.700","Init Profile","[MSC] RX: H, Fitted Concentrations , 2  "]
["$","2022-02-24","00:46:21.700","Init Profile","[MSC] RX: H, Baseline        Model , (ax + b)  "]
["$","2022-02-24","00:46:21.700","Init Profile","[MSC] RX: H, Br Temp  Compensation , ENABLED  "]
["$","2022-02-24","00:46:21.800","Init Profile","[MSC] RX: H, Bromide Term in Model , will be FIXED (to external CTD value)  "]
["$","2022-02-24","00:46:21.900","Init Profile","[MSC] RX: H, Zeiss Coefficient Vals, 1.885090e+02,7.959960e-01,1.113850e-04,-3.090260e-07,0.000000e+00  "]
["$","2022-02-24","00:46:22.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:22.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:22.600","Init Profile","System Data (dBar %full Volts mAmps): ",-0.12,44.820202999999999,32.375,10,0.13247500000000001,119.53704,null,32.375,184.5,2.6298249999999999,11.940272999999999,null,null,null,null,null,null,null,null,null,1218.130005,12.5,38.203999000000003,12.5]
["$","2022-02-24","00:46:22.700","Init Profile","Pump motor not faulted"]
["$","2022-02-24","00:46:24.100","Init Profile","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:24.100","Init Profile","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:22.700","Init Profile","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:22.700","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:22.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:22.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:22.900","Init Profile","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:22.900","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:23.100","Init Profile","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:23.100","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:23.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","00:46:23.200","Init Profile","SBE41 Message",-0.1,44.820202999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.181171,3.3000000000000003E-5,-6.6670000000000002E-3,-6.6670000000000002E-3,3.0000000000000001E-6,3000]
["$","2022-02-24","00:46:23.300","Init Profile","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:23.300","Init Profile","Twitter msg",null,null,null,null,null,null,"33604352;"]
["$","2022-02-24","00:46:23.500","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:23.500","Init Profile","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:23.700","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:23.700","Init Profile","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:23.900","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:23.900","Init Profile","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:24.200","Init Profile","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:24.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:24.200","Init Profile","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:24.200","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:24.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:25.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:25.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:25.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:25.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:26.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.19]
["$","2022-02-24","00:46:26.200","Init Profile","SBE41 Message",-0.19,44.831905999999996,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.19,-0.19,-0.17721999999999999,1.21E-4,0.03,1.1667E-2,-9.9999999999999995E-7,3000]
["$","2022-02-24","00:46:26.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:27.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:28","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:28","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:28.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:28.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:28.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:29","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:46:29","Init Profile","SBE41 Message",-0.09,44.827361000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.16519300000000001,1.2899999999999999E-4,-3.3333000000000002E-2,-1.6670000000000001E-3,-1.9000000000000001E-5,3000]
["$","2022-02-24","00:46:29.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:30.400","Init Profile","[MSC] TX: SE,?"]
["$","2022-02-24","00:46:30.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:30.600","Init Profile","[MSC] RX: ACK,SE?,0  "]
["$","2022-02-24","00:46:30.700","Init Profile","[MSC] ERRORS AVAILABLE: 0"]
["$","2022-02-24","00:46:30.700","Init Profile","[MSC] TX: W"]
["$","2022-02-24","00:46:30.800","Init Profile","[MSC] RX: ACK  "]
["$","2022-02-24","00:46:30.900","Init Profile","[MSC] TX: MODE,2"]
["$","2022-02-24","00:46:31.100","Init Profile","[MSC] RX: ACK,MODE,2  "]
["$","2022-02-24","00:46:31.200","Init Profile","[MSC] TX: ACK "]
["$","2022-02-24","00:46:31.200","Init Profile","[MSC] TX: C"]
["$","2022-02-24","00:46:31.400","Init Profile","[MSC] RX: H, Datalogger Serial Num , SN:0003  "]
["$","2022-02-24","00:46:31.500","Init Profile","[MSC] RX: H, Application      Name , CPF_MAIN.C  "]
["$","2022-02-24","00:46:31.500","Init Profile","[MSC] RX: H, App Build        Date , Nov 20 2020, 13:19:41  "]
["$","2022-02-24","00:46:31.600","Init Profile","[MSC] RX: H, Power Up Time   (GMT) , 02/23/2022 22:32:51  "]
["$","2022-02-24","00:46:31.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:31.600","Init Profile","[MSC] RX: H, Current  Time   (GMT) , 02/24/2022 00:46:30  "]
["$","2022-02-24","00:46:31.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:31.700","Init Profile","[MSC] RX: H, Alarm    Time   (GMT) , 02/24/2022 08:32:56  "]
["$","2022-02-24","00:46:31.700","Init Profile","[MSC] RX: H, Power Active  Timeout , 10  "]
["$","2022-02-24","00:46:31.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:31.800","Init Profile","[MSC] RX: H, Persistor CF2-1M Info , S/N:15079 - BIOS:4.03 - PicoDOS:4.03  "]
["$","2022-02-24","00:46:31.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:31.800","Init Profile","[MSC] RX: H, Compact FLASH    Size , 256614400  "]
["$","2022-02-24","00:46:31.900","Init Profile","[MSC] RX: H, Compact FLASH    Left , 90.94%  "]
["$","2022-02-24","00:46:31.900","Init Profile","[MSC] RX: H, Power Cycle   Counter , 5  "]
["$","2022-02-24","00:46:31.900","Init Profile","[MSC] RX: H, System Reset  Counter , 5  "]
["$","2022-02-24","00:46:32","Init Profile","[MSC] RX: H, System Error  Counter , 0  "]
["$","2022-02-24","00:46:32","Init Profile","[MSC] RX: H, Last System     Error , 0  "]
["$","2022-02-24","00:46:32","Init Profile","[MSC] RX: H, Last System ErrorTime , 01/01/1970 00:00:00  "]
["$","2022-02-24","00:46:32.100","Init Profile","[MSC] RX: H, DURA  Error   Counter , 0  "]
["$","2022-02-24","00:46:32.100","Init Profile","[MSC] RX: H, Last DURA       Error , 0  "]
["$","2022-02-24","00:46:32.200","Init Profile","[MSC] RX: H, Last DURA Error  Time , 01/01/1970 00:00:00  "]
["$","2022-02-24","00:46:32.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.23]
["$","2022-02-24","00:46:32.200","Init Profile","SBE41 Message",-0.23,44.826250999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.23,-0.23,-0.14768200000000001,-2.9399999999999999E-4,4.6667E-2,6.6670000000000002E-3,-5.7000000000000003E-5,3000]
["$","2022-02-24","00:46:32.300","Init Profile","[MSC] RX: H, DURA Sample   Counter , 46  "]
["$","2022-02-24","00:46:32.300","Init Profile","[MSC] RX: H, Last Sample Rec. Time , 02/24/2022 00:40:28  "]
["$","2022-02-24","00:46:32.300","Init Profile","[MSC] RX: H, AtoD Reads per Sample , 10  "]
["$","2022-02-24","00:46:32.300","Init Profile","[MSC] RX: H, AtoD Reading    Delay , 100  "]
["$","2022-02-24","00:46:32.300","Init Profile","[MSC] RX: H, Samps per AtoD  Recal , 250  "]
["$","2022-02-24","00:46:32.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:33.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:33.600","Init Profile","System Data (dBar %full Volts mAmps): ",-0.23,44.817672999999999,32.375,5,0.21248500000000001,209.525598,null,32.375,186.5,4.6481669999999999,20.939129000000001,null,null,null,null,null,null,null,null,null,1218.150024,12.49,38.502997999999998,12.49]
["$","2022-02-24","00:46:33.700","Init Profile","Pump motor not faulted"]
["$","2022-02-24","00:46:34.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:35.100","Init Profile","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:35.100","Init Profile","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:33.700","Init Profile","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:33.700","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:33.900","Init Profile","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:33.900","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:34","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:34","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:34.100","Init Profile","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:34.100","Init Profile","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:34.300","Init Profile","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:34.300","Init Profile","Twitter msg",null,null,null,null,null,null,"33604352;"]
["$","2022-02-24","00:46:34.500","Init Profile","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:34.500","Init Profile","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:34.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:34.700","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:34.700","Init Profile","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:34.900","Init Profile","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:34.900","Init Profile","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:35","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","00:46:35","Init Profile","SBE41 Message",-0.17,44.817672999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-0.13459699999999999,-1.413E-3,-0.02,1.3332999999999999E-2,-1.0900000000000001E-4,3000]
["$","2022-02-24","00:46:35.100","Init Profile","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:35.100","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:35.100","Init Profile","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:35.100","Init Profile","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:35.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:36.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:37.100","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:37.100","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:37.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:37.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:37.700","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:38.100","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.21]
["$","2022-02-24","00:46:38.100","Init Profile","SBE41 Message",-0.21,44.819037000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.21,-0.21,-0.13330400000000001,-2.9099999999999998E-3,1.3332999999999999E-2,-3.333E-3,-1.6000000000000001E-4,3000]
["$","2022-02-24","00:46:38.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:39.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:40.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:40.600","Init Profile","CTD Sending fast pressure"]
["$","2022-02-24","00:46:40.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:40.800","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:41.200","Init Profile","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:46:41.200","Init Profile","SBE41 Message",-0.08,44.824097000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.142341,-3.9240000000000004E-3,-4.3333000000000003E-2,-1.4999999999999999E-2,-1.9699999999999999E-4,3000]
["$","2022-02-24","00:46:41.400","Init Profile","[MSC] TX: SE,?"]
["$","2022-02-24","00:46:41.600","Init Profile","Checking Global Issues."]
["$","2022-02-24","00:46:41.700","Init Profile","[MSC] RX: ACK,SE?,0  "]
["$","2022-02-24","00:46:41.700","Init Profile","[MSC] ERRORS AVAILABLE: 0"]
["$","2022-02-24","00:46:41.700","Init Profile","Normal State Exit"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Setting Execution Constraint = 900000"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","State Entry"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:46:41.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:46:41.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:42.100","Decrease Buoyancy Fast","Decreasing Buoyancy to pressure = 0.30 at 200000 cps"]
["$","2022-02-24","00:46:42.100","Decrease Buoyancy Fast","Initializing SBE 41 LPF"]
["$","2022-02-24","00:46:42.100","Decrease Buoyancy Fast","Checking global issues before power down"]
["$","2022-02-24","00:46:42.100","Decrease Buoyancy Fast","Disabling unneeded power"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","[MSC] Powering down MSC"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","Powering down GPS"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","[MSC] Powering down MSC"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","Powering down FLBB"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","Powering down 4330 Optode"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","Powering down OCR504"]
["$","2022-02-24","00:46:42.200","Decrease Buoyancy Fast","Powering down Bluetooth"]
["$","2022-02-24","00:46:43.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:45.200","Decrease Buoyancy Fast","Checking global issues after power down"]
["$","2022-02-24","00:46:45.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:45.300","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.08,44.818860000000001,32.375,10,0.29774099999999998,305.02091799999999,null,32.375,142,6.6663779999999999,30.488661,null,null,null,null,null,null,null,null,null,1218.099976,12.51,38.823002000000002,12.51]
["$","2022-02-24","00:46:45.400","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:46:46.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:43.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:44","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:46:44","Decrease Buoyancy Fast","SBE41 Message",-0.15,44.818860000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-8.0001000000000003E-2,0,2.3333E-2,1.1667E-2,0,3000]
["$","2022-02-24","00:46:45.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:45.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:45.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:45.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:45.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:45.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:46:46","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:46","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"33604352;"]
["$","2022-02-24","00:46:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:46.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:46.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:46.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:46.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:46.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:47.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","00:46:47.200","Decrease Buoyancy Fast","SBE41 Message",-0.05,44.818860000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-8.0147999999999997E-2,-1.9999999999999999E-6,-3.3333000000000002E-2,-5.0000000000000001E-3,0,3000]
["$","2022-02-24","00:46:47.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:47.400","Decrease Buoyancy Fast","Decrease buoyancy is opening valve"]
["$","2022-02-24","00:46:47.400","Decrease Buoyancy Fast","BE::openMV: Starting valve open"]
["$","2022-02-24","00:46:49.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","BE::sendJV: 200000"]
["$","2022-02-24","00:46:49.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:49.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"JV=200000;"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:46:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:46:50.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:46:50.200","Decrease Buoyancy Fast","SBE41 Message",-0.14000000000000001,44.836132999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-8.1617999999999996E-2,-1.2999999999999999E-5,0.03,-1.6670000000000001E-3,1.9999999999999999E-6,3000]
["$","2022-02-24","00:46:50.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:51.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:52","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:52","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:46:52.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:52.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:52.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:53","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.11]
["$","2022-02-24","00:46:53","Decrease Buoyancy Fast","SBE41 Message",-0.11,44.910612999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.11,-0.11,-8.6555000000000007E-2,-6.9999999999999999E-6,-0.01,0.01,1.0000000000000001E-5,3000]
["$","2022-02-24","00:46:53.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:54.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:55.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:55.300","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.11,45.161051,32.25,1135,6.4047070000000001,387.488045,null,32.274999999999999,158.5,8.2337799999999994,38.735373000000003,null,null,null,null,null,null,null,null,null,1219.01001,12.51,38.084000000000003,12.51]
["$","2022-02-24","00:46:55.400","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:46:55.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:46:55.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:46:55.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197657;"]
["$","2022-02-24","00:46:55.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:46:55.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.68450;"]
["$","2022-02-24","00:46:55.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:55.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:55.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:46:55.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"2.07450;"]
["$","2022-02-24","00:46:56","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:46:56","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:46:56.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.01]
["$","2022-02-24","00:46:56.200","Decrease Buoyancy Fast","SBE41 Message",0.01,45.161051,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.01,0.01,-9.4257999999999995E-2,1.5899999999999999E-4,-0.04,-2.5000000000000001E-2,2.6999999999999999E-5,3000]
["$","2022-02-24","00:46:56.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:46:56.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:46:56.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:46:56.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:46:56.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:46:56.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:46:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:46:57.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:58.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:46:58.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:46:58.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:46:58.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:46:59.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.23]
["$","2022-02-24","00:46:59.100","Decrease Buoyancy Fast","SBE41 Message",-0.23,45.516581000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.23,-0.23,-0.100286,6.1600000000000001E-4,0.08,0.02,5.0000000000000002E-5,3000]
["$","2022-02-24","00:46:59.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:00.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:01.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:01.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:01.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:01.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:02.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.01]
["$","2022-02-24","00:47:02.200","Decrease Buoyancy Fast","SBE41 Message",-0.01,45.800851999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.01,-0.01,-0.10185,1.2440000000000001E-3,-7.3332999999999995E-2,3.333E-3,7.3999999999999996E-5,3000]
["$","2022-02-24","00:47:02.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:03.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:04","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:04","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:04.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:04.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:04.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:05","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:47:05","Decrease Buoyancy Fast","SBE41 Message",-0.14000000000000001,46.106814,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-9.8904000000000006E-2,1.714E-3,4.3333000000000003E-2,-1.4999999999999999E-2,9.2999999999999997E-5,3000]
["$","2022-02-24","00:47:05.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:06.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:06.300","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.14000000000000001,46.310864000000002,32.225000000000001,1085,18.669792999999999,477.34229099999999,null,32.225000000000001,157,9.9348379999999992,47.720798000000002,null,null,null,null,null,null,null,null,null,1220.48999,12.51,38.050998999999997,12.51]
["$","2022-02-24","00:47:06.400","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:47:07.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:47:06.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:47:06.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196423;"]
["$","2022-02-24","00:47:06.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:47:06.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.72395;"]
["$","2022-02-24","00:47:06.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:47:06.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1.98416;"]
["$","2022-02-24","00:47:07","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:47:07","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","00:47:07.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:47:07.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:47:07.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:47:07.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:47:07.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:47:07.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:47:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:08.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:08.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:47:08.200","Decrease Buoyancy Fast","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:47:08.200","Decrease Buoyancy Fast","SBE41 Message",-0.14000000000000001,46.391285000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-9.4349000000000002E-2,1.6739999999999999E-3,0,2.1666999999999999E-2,1.06E-4,3000]
["$","2022-02-24","00:47:09.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:10.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:10.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:10.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:11","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:47:11","Decrease Buoyancy Fast","SBE41 Message",-0.08,46.713799000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-9.4411999999999996E-2,9.8900000000000008E-4,-0.02,-0.01,1.17E-4,3000]
["$","2022-02-24","00:47:11.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:12.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:13.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:13.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:14.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:14.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:47:14.200","Decrease Buoyancy Fast","SBE41 Message",-0.15,47.132662000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-9.9584000000000006E-2,7.2999999999999999E-5,2.3333E-2,1.6670000000000001E-3,1.34E-4,3000]
["$","2022-02-24","00:47:15.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:16.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:16.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:16.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:17.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","00:47:17.100","Decrease Buoyancy Fast","SBE41 Message",-0.1,47.325462000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.104979,-4.0700000000000003E-4,-1.6667000000000001E-2,3.333E-3,1.5699999999999999E-4,3000]
["$","2022-02-24","00:47:17.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:17.200","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.1,47.476422999999997,32.200000000000003,1130,30.736822,566.65929300000005,null,32.25,156,11.628418999999999,56.652498000000001,null,null,null,null,null,null,null,null,null,1222.079956,12.51,38.459999000000003,12.51]
["$","2022-02-24","00:47:17.300","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:47:17.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:47:17.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197505;"]
["$","2022-02-24","00:47:17.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:47:17.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.20629;"]
["$","2022-02-24","00:47:17.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:47:17.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.02729;"]
["$","2022-02-24","00:47:17.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:47:17.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"79741712;"]
["$","2022-02-24","00:47:18.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:47:18.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:47:18.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:47:18.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:47:18.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:47:18.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:47:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:19","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:19.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:20","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:20.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:47:20.200","Decrease Buoyancy Fast","SBE41 Message",-0.12,47.736158000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.110177,-1.95E-4,6.6670000000000002E-3,-5.0000000000000001E-3,1.84E-4,3000]
["$","2022-02-24","00:47:21","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:22","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:22.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:22.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:23","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:23","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","00:47:23","Decrease Buoyancy Fast","SBE41 Message",-0.05,47.981763999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-0.115027,5.1599999999999997E-4,-2.3333E-2,-8.3330000000000001E-3,2.1599999999999999E-4,3000]
["$","2022-02-24","00:47:24","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:25","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:25.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:26","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:26.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:47:26.200","Decrease Buoyancy Fast","SBE41 Message",-0.09,48.412565999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.117079,1.3159999999999999E-3,1.3332999999999999E-2,-5.0000000000000001E-3,2.4800000000000001E-4,3000]
["$","2022-02-24","00:47:27","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:28","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:28","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.09,48.589958000000003,32.25,1130,42.680557,655.707672,null,32.25,156,13.31413,65.557336000000006,null,null,null,null,null,null,null,null,null,1223.5500489999999,12.54,38.382998999999998,12.54]
["$","2022-02-24","00:47:28.100","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:47:28.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:47:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:28.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:47:28.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196705;"]
["$","2022-02-24","00:47:28.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:47:28.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.11642;"]
["$","2022-02-24","00:47:28.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:47:28.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.71379;"]
["$","2022-02-24","00:47:28.600","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:28.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:47:28.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:47:28.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:47:28.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:47:29","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.23]
["$","2022-02-24","00:47:29","Decrease Buoyancy Fast","SBE41 Message",-0.23,48.589958000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.23,-0.23,-0.115735,1.74E-3,4.6667E-2,0.03,2.7599999999999999E-4,3000]
["$","2022-02-24","00:47:29.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:47:29.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:47:29.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:47:29.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:47:29.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:30","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:31","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:31.500","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:31.500","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:31.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:31.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:32","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:32","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.21]
["$","2022-02-24","00:47:32","Decrease Buoyancy Fast","SBE41 Message",-0.21,49.024785000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.21,-0.21,-0.10975,1.572E-3,-6.6670000000000002E-3,0.02,2.9399999999999999E-4,3000]
["$","2022-02-24","00:47:33","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:34","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:34.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:34.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:34.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:35","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:35.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.22]
["$","2022-02-24","00:47:35.200","Decrease Buoyancy Fast","SBE41 Message",-0.22,49.319819000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.22,-0.22,-0.101577,8.9300000000000002E-4,3.333E-3,-1.6670000000000001E-3,2.9999999999999997E-4,3000]
["$","2022-02-24","00:47:36","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:37","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:37","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:37","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:37.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:37.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:38","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:38.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.11]
["$","2022-02-24","00:47:38.100","Decrease Buoyancy Fast","SBE41 Message",-0.11,49.655622999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.11,-0.11,-0.105013,-1.9900000000000001E-4,-3.6666999999999998E-2,-1.6667000000000001E-2,3.0899999999999998E-4,3000]
["$","2022-02-24","00:47:39","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:39","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.11,49.675153999999999,32.174999999999997,1030,54.624293000000002,745.83054100000004,null,32.200000000000003,155.5,15.021089999999999,74.569623000000007,null,null,null,null,null,null,null,null,null,1225.089966,12.53,37.930999999999997,12.53]
["$","2022-02-24","00:47:39.100","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:47:39.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:47:39.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"195820;"]
["$","2022-02-24","00:47:39.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:47:39.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.49682;"]
["$","2022-02-24","00:47:40.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:39.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:47:39.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.10167;"]
["$","2022-02-24","00:47:39.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:47:39.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:47:39.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:47:39.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:47:40.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:47:40.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:47:40.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:47:40.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:47:40.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:40.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:41.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","00:47:41.200","Decrease Buoyancy Fast","SBE41 Message",-0.17,49.804412999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-0.13144700000000001,-1.1999999999999999E-3,0.02,-8.3330000000000001E-3,3.4900000000000003E-4,3000]
["$","2022-02-24","00:47:41.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:42.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:43.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:43.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:43.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:44.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.16]
["$","2022-02-24","00:47:44.100","Decrease Buoyancy Fast","SBE41 Message",-0.16,50.149845999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.16,-0.16,-0.168514,-8.2700000000000004E-4,-3.333E-3,8.3330000000000001E-3,4.3199999999999998E-4,3000]
["$","2022-02-24","00:47:44.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:45.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:46.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:46.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:47.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:47:47.200","Decrease Buoyancy Fast","SBE41 Message",-0.09,50.463326000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.18921199999999999,1.6540000000000001E-3,-2.3333E-2,-1.3332999999999999E-2,5.3499999999999999E-4,3000]
["$","2022-02-24","00:47:47.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:48.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:49.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:49.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:49.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:49.900","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.09,50.752968000000003,32.225000000000001,1160,66.564093999999997,835.28185399999995,null,32.25,156.5,16.715720999999998,83.514753999999996,null,null,null,null,null,null,null,null,null,1226.650024,12.53,38.528998999999999,12.53]
["$","2022-02-24","00:47:50","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:47:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:47:50","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197243;"]
["$","2022-02-24","00:47:50","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:47:50","Decrease Buoyancy Fast","SBE41 Message",-0.15,50.752968000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-0.18359900000000001,5.084E-3,0.02,-1.6670000000000001E-3,6.2399999999999999E-4,3000]
["$","2022-02-24","00:47:50.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:47:50.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.61254;"]
["$","2022-02-24","00:47:50.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:47:50.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"2.46768;"]
["$","2022-02-24","00:47:50.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:47:50.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","00:47:50.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:47:50.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:47:51","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:47:51","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:47:51.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:47:51.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:47:51.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:47:51.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:52.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","00:47:52.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:53.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:54.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:47:54.200","Decrease Buoyancy Fast","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:47:54.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:55.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:55.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:55.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:56","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:47:56","Decrease Buoyancy Fast","SBE41 Message",-0.08,51.341512999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.16617699999999999,7.1929999999999997E-3,-2.3333E-2,-1.6670000000000001E-3,6.8400000000000004E-4,3000]
["$","2022-02-24","00:47:56.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:57.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:58.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:47:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:47:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:47:58.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:47:59.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:47:59.200","Decrease Buoyancy Fast","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:47:59.200","Decrease Buoyancy Fast","SBE41 Message",-0.08,51.659756000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.151534,6.4460000000000003E-3,0,-1.1667E-2,7.18E-4,3000]
["$","2022-02-24","00:47:59.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:00.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:00.900","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.08,51.839185000000001,32.15,1050,79.192502000000005,925.00179000000003,null,32.200000000000003,157,18.414549000000001,92.486748000000006,null,null,null,null,null,null,null,null,null,1228.160034,12.54,38.383999000000003,12.54]
["$","2022-02-24","00:48:00.900","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:01.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:01","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:01","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"195013;"]
["$","2022-02-24","00:48:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:01.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:01.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.06292;"]
["$","2022-02-24","00:48:01.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:01.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1.33122;"]
["$","2022-02-24","00:48:01.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:01.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"79741712;"]
["$","2022-02-24","00:48:01.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:01.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:01.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:02","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:02","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:02","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:48:02","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,51.839185000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.13977000000000001,3.078E-3,-3.333E-3,-1.6670000000000001E-3,7.3300000000000004E-4,3000]
["$","2022-02-24","00:48:02.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:02.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:02.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:02.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:03.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:04.300","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:04.300","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:04.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:04.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:04.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:05","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:48:05","Decrease Buoyancy Fast","SBE41 Message",-0.12,52.257353000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.126999,-1.126E-3,1.6667000000000001E-2,6.6670000000000002E-3,7.27E-4,3000]
["$","2022-02-24","00:48:05.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:06.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:07.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:07.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:08.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.11]
["$","2022-02-24","00:48:08.200","Decrease Buoyancy Fast","SBE41 Message",-0.11,52.539012,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.11,-0.11,-0.11290699999999999,-4.0749999999999996E-3,-3.333E-3,6.6670000000000002E-3,7.0100000000000002E-4,3000]
["$","2022-02-24","00:48:08.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:09.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:10.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:10.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:10.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:11","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.18]
["$","2022-02-24","00:48:11","Decrease Buoyancy Fast","SBE41 Message",-0.18,52.830970000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.18,-0.18,-9.8955000000000001E-2,-4.9950000000000003E-3,2.3333E-2,0.01,6.5700000000000003E-4,3000]
["$","2022-02-24","00:48:11.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:11.800","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.18,52.909388999999997,32.200000000000003,1155,91.965190000000007,1015.124659,null,32.174999999999997,153.5,20.123739,101.49903500000001,null,null,null,null,null,null,null,null,null,1229.719971,12.56,38.574001000000003,12.56]
["$","2022-02-24","00:48:11.900","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:13.300","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:13.400","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:11.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:11.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"195727;"]
["$","2022-02-24","00:48:12.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:12.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.26283;"]
["$","2022-02-24","00:48:12.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:12.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1.86312;"]
["$","2022-02-24","00:48:12.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:12.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"46187280;"]
["$","2022-02-24","00:48:12.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:12.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:12.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:13","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:13.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:13.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:13.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:13.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:13.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:13.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:13.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:13.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:14.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.11]
["$","2022-02-24","00:48:14.200","Decrease Buoyancy Fast","SBE41 Message",-0.11,52.979253,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.11,-0.11,-9.0315999999999994E-2,-4.8149999999999998E-3,-2.3333E-2,0,6.0099999999999997E-4,3000]
["$","2022-02-24","00:48:14.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:15.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:16.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:16.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:16.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:17.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","00:48:17.100","Decrease Buoyancy Fast","SBE41 Message",0,53.399253999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0,0,-9.3354000000000006E-2,-4.5960000000000003E-3,-3.6666999999999998E-2,-0.03,5.4900000000000001E-4,3000]
["$","2022-02-24","00:48:17.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:18.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:19.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:19.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:20.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:48:20.200","Decrease Buoyancy Fast","SBE41 Message",-0.08,53.658524999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.10709200000000001,-4.1669999999999997E-3,2.6667E-2,-5.0000000000000001E-3,5.1400000000000003E-4,3000]
["$","2022-02-24","00:48:20.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:21.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:22.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:22.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:22.700","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:22.700","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.08,53.988062999999997,32.15,1050,104.61327300000001,1104.3073489999999,null,32.225000000000001,156,21.811024,110.417304,null,null,null,null,null,null,null,null,null,1231.3100589999999,12.56,38.884998000000003,12.56]
["$","2022-02-24","00:48:22.800","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:22.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:22.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"194762;"]
["$","2022-02-24","00:48:23","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:23","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.74971;"]
["$","2022-02-24","00:48:23","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:48:23","Decrease Buoyancy Fast","SBE41 Message",-0.14000000000000001,53.988062999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.120505,-2.7529999999999998E-3,0.02,2.3333E-2,4.9299999999999995E-4,3000]
["$","2022-02-24","00:48:23.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:23.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-1.80043;"]
["$","2022-02-24","00:48:23.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:23.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:48:23.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:23.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:23.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:23.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:24","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:24","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:24.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:25.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:25.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:26.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:48:26.200","Decrease Buoyancy Fast","SBE41 Message",-0.08,54.279539999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.11851399999999999,-3.6400000000000001E-4,-0.02,0,4.6799999999999999E-4,3000]
["$","2022-02-24","00:48:26.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:27.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:28.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:28.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:28.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:29","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:48:29","Decrease Buoyancy Fast","SBE41 Message",-0.12,54.521110999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-9.8710000000000006E-2,1.774E-3,1.3332999999999999E-2,-3.333E-3,4.1800000000000002E-4,3000]
["$","2022-02-24","00:48:29.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:30.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:31.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:31.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:31.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:31.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:32.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:48:32.200","Decrease Buoyancy Fast","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:48:32.200","Decrease Buoyancy Fast","SBE41 Message",-0.12,54.799463000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-8.0685999999999994E-2,2.088E-3,0,6.6670000000000002E-3,3.4499999999999998E-4,3000]
["$","2022-02-24","00:48:32.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:33.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:33.700","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.12,55.011890000000001,32.200000000000003,1180,117.17741100000001,1194.0272849999999,null,32.174999999999997,160,23.513787000000001,119.389297,null,null,null,null,null,null,null,null,null,1232.790039,12.56,38.011001999999998,12.56]
["$","2022-02-24","00:48:33.700","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:34.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:33.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:33.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"198063;"]
["$","2022-02-24","00:48:34","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:34","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.38084;"]
["$","2022-02-24","00:48:34","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:34","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:34.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:34.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.93212;"]
["$","2022-02-24","00:48:34.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:34.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"96518928;"]
["$","2022-02-24","00:48:34.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:34.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:34.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:34.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:34.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:35","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:35","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:35","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:48:35","Decrease Buoyancy Fast","SBE41 Message",-0.15,55.011890000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-8.2055000000000003E-2,2.9500000000000001E-4,0.01,5.0000000000000001E-3,2.7500000000000002E-4,3000]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:35.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:35.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:36.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:37.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:37.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:37.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:37.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:37.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:38.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:48:38.100","Decrease Buoyancy Fast","SBE41 Message",-0.08,55.400098,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-9.5448000000000005E-2,-2.0330000000000001E-3,-2.3333E-2,-6.6670000000000002E-3,2.2100000000000001E-4,3000]
["$","2022-02-24","00:48:38.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:39.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:40.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:40.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:41.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.16]
["$","2022-02-24","00:48:41.200","Decrease Buoyancy Fast","SBE41 Message",-0.16,55.721471000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.16,-0.16,-0.106507,-2.9870000000000001E-3,2.6667E-2,1.6670000000000001E-3,1.8000000000000001E-4,3000]
["$","2022-02-24","00:48:41.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:42.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:43.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:43.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:43.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:44.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","00:48:44.100","Decrease Buoyancy Fast","SBE41 Message",-0.14000000000000001,55.956040000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.11397699999999999,-1.9109999999999999E-3,-6.6670000000000002E-3,0.01,1.46E-4,3000]
["$","2022-02-24","00:48:44.600","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:44.600","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.14000000000000001,56.050801,32.174999999999997,1170,129.7022,1284.1501539999999,null,32.225000000000001,157.5,25.222714,128.40158400000001,null,null,null,null,null,null,null,null,null,1234.380005,12.58,38.553001000000002,12.58]
["$","2022-02-24","00:48:44.700","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:46.100","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:46.100","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:44.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:44.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"199230;"]
["$","2022-02-24","00:48:44.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:44.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.71885;"]
["$","2022-02-24","00:48:45.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:45.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.748429e-04;"]
["$","2022-02-24","00:48:45.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:45.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"96518928;"]
["$","2022-02-24","00:48:45.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:45.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:45.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:45.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:45.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:45.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:46.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:46.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:46.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:47.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:48:47.200","Decrease Buoyancy Fast","SBE41 Message",-0.08,56.161847000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.120007,4.7899999999999999E-4,-0.02,-1.3332999999999999E-2,1.17E-4,3000]
["$","2022-02-24","00:48:47.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:48.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:49.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:49.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:49.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:50","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:48:50","Decrease Buoyancy Fast","SBE41 Message",-0.15,56.555619,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-0.123269,2.6389999999999999E-3,2.3333E-2,1.6670000000000001E-3,9.0000000000000006E-5,3000]
["$","2022-02-24","00:48:50.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:51.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:52.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:52.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:53.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","00:48:53.200","Decrease Buoyancy Fast","SBE41 Message",-0.1,56.853907999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.125218,3.2629999999999998E-3,-1.6667000000000001E-2,3.333E-3,6.3999999999999997E-5,3000]
["$","2022-02-24","00:48:53.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:54.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:55","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:55","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:48:55.500","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:55.500","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.1,57.184972999999999,32.174999999999997,1255,142.11812399999999,1373.198533,null,32.15,155.5,26.911442000000001,137.306422,null,null,null,null,null,null,null,null,null,1235.959961,12.58,39.173999999999999,12.58]
["$","2022-02-24","00:48:55.600","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:48:55.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:48:55.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:48:55.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196866;"]
["$","2022-02-24","00:48:55.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:55.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:48:55.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.06470;"]
["$","2022-02-24","00:48:56","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:48:56","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-1.10416;"]
["$","2022-02-24","00:48:56","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","00:48:56","Decrease Buoyancy Fast","SBE41 Message",-0.15,57.184972999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-0.126799,2.555E-3,1.6667000000000001E-2,0,4.3000000000000002E-5,3000]
["$","2022-02-24","00:48:56.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:48:56.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","00:48:56.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:48:56.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:48:56.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:48:56.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:48:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:48:56.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:48:57","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:48:57.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:58.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:48:58.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:48:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:48:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:48:59.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:48:59.200","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,57.440992999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.125113,1.6750000000000001E-3,-2.6667E-2,-5.0000000000000001E-3,2.6999999999999999E-5,3000]
["$","2022-02-24","00:48:59.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:00.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:01.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:01.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:01.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:02","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:49:02","Decrease Buoyancy Fast","SBE41 Message",-0.12,57.697634000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.121397,1.0449999999999999E-3,1.6667000000000001E-2,-5.0000000000000001E-3,1.2999999999999999E-5,3000]
["$","2022-02-24","00:49:02.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:03.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:04.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:04.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:04.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:04.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:05.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","00:49:05.200","Decrease Buoyancy Fast","SBE41 Message",-0.05,58.000996000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-0.11996800000000001,4.1599999999999997E-4,-2.3333E-2,-3.333E-3,-3.0000000000000001E-6,3000]
["$","2022-02-24","00:49:05.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:06.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:06.500","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.05,58.193772000000003,32.174999999999997,1155,154.51830799999999,1463.05278,null,32.200000000000003,155,28.613417999999999,146.27841599999999,null,null,null,null,null,null,null,null,null,1237.5,12.58,38.918998999999999,12.58]
["$","2022-02-24","00:49:06.500","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:49:07.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:49:06.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:49:06.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196054;"]
["$","2022-02-24","00:49:06.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:49:06.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.99357;"]
["$","2022-02-24","00:49:07","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:49:07","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.74678;"]
["$","2022-02-24","00:49:07","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:07","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:07.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:49:07.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"96518928;"]
["$","2022-02-24","00:49:07.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:49:07.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:49:07.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:49:07.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:49:07.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:49:07.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.11]
["$","2022-02-24","00:49:08","Decrease Buoyancy Fast","SBE41 Message",-0.11,58.193772000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.11,-0.11,-0.118953,-1.3200000000000001E-4,0.02,-1.6670000000000001E-3,-2.4000000000000001E-5,3000]
["$","2022-02-24","00:49:08.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:09.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:10.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:10.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:10.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:11","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","00:49:11","Decrease Buoyancy Fast","SBE41 Message",-0.1,58.541772000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.113371,-4.2400000000000001E-4,-3.333E-3,8.3330000000000001E-3,-5.8999999999999998E-5,3000]
["$","2022-02-24","00:49:11.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:12.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:13.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:13.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:14.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:49:14.200","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,58.906404999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.103365,-6.5899999999999997E-4,-0.01,-6.6670000000000002E-3,-1.07E-4,3000]
["$","2022-02-24","00:49:14.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:15.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:16.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:16.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:16.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:17","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.04]
["$","2022-02-24","00:49:17","Decrease Buoyancy Fast","SBE41 Message",-0.04,59.166539999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.04,-0.04,-9.3922000000000005E-2,-1.067E-3,-0.01,-0.01,-1.6000000000000001E-4,3000]
["$","2022-02-24","00:49:17.400","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:17.400","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.04,59.330317000000001,32.15,1060,166.97751500000001,1553.041338,null,32.15,157.5,30.320903000000001,155.27727200000001,null,null,null,null,null,null,null,null,null,1239.030029,12.59,39.318001000000002,12.59]
["$","2022-02-24","00:49:17.500","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:49:18.900","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:49:18.900","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:49:17.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:49:17.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"194223;"]
["$","2022-02-24","00:49:17.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:49:17.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.73562;"]
["$","2022-02-24","00:49:17.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:49:17.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.62581;"]
["$","2022-02-24","00:49:18.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:49:18.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","00:49:18.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:49:18.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:49:18.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:49:18.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:49:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:49:18.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:49:19","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:49:19","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:19","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:49:19","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:19.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:19.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:20.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:49:20.200","Decrease Buoyancy Fast","SBE41 Message",-0.08,59.353662999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-8.9493000000000003E-2,-1.6440000000000001E-3,1.3332999999999999E-2,1.6670000000000001E-3,-2.12E-4,3000]
["$","2022-02-24","00:49:20.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:21.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:22.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:22.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:22.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:23","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:49:23","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,59.796044999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-8.8497000000000006E-2,-2.2009999999999998E-3,-3.333E-3,5.0000000000000001E-3,-2.5700000000000001E-4,3000]
["$","2022-02-24","00:49:23.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:24.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:25.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:25.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:26.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","00:49:26.200","Decrease Buoyancy Fast","SBE41 Message",0,59.977243999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0,0,-8.412E-2,-2.398E-3,-2.3333E-2,-1.3332999999999999E-2,-3.01E-4,3000]
["$","2022-02-24","00:49:26.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:27.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:28","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:28.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:28.300","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",0,60.288666999999997,32.15,1190,179.26489900000001,1642.0897170000001,null,32.200000000000003,156,32.012253999999999,164.19554099999999,null,null,null,null,null,null,null,null,null,1240.599976,12.6,38.334000000000003,12.6]
["$","2022-02-24","00:49:28.400","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:49:28.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:49:28.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:49:28.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197115;"]
["$","2022-02-24","00:49:28.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:49:28.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1.11942;"]
["$","2022-02-24","00:49:28.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:28.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:49:28.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1.03083;"]
["$","2022-02-24","00:49:29","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:49:29","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:49:29","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.02]
["$","2022-02-24","00:49:29","Decrease Buoyancy Fast","SBE41 Message",0.02,60.288666999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.02,0.02,-7.4582999999999997E-2,-2.1289999999999998E-3,-6.6670000000000002E-3,-1.4999999999999999E-2,-3.5199999999999999E-4,3000]
["$","2022-02-24","00:49:29.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:49:29.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:49:29.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:49:29.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:49:29.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:49:29.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:49:29.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:30.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:31.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:31.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:31.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:31.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:32.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:49:32.100","Decrease Buoyancy Fast","SBE41 Message",-0.09,60.598512999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-6.5625000000000003E-2,-1.776E-3,3.6666999999999998E-2,1.4999999999999999E-2,-4.1300000000000001E-4,3000]
["$","2022-02-24","00:49:32.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:33.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:34.200","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:34.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:34.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:34.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:35.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","00:49:35.200","Decrease Buoyancy Fast","SBE41 Message",-0.12,60.86647,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-5.7674000000000003E-2,-1.7080000000000001E-3,0.01,2.3333E-2,-4.8899999999999996E-4,3000]
["$","2022-02-24","00:49:35.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:36.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:37","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:37","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:37.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:37.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:37.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:38","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","00:49:38","Decrease Buoyancy Fast","SBE41 Message",0,61.165126000000001,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0,0,-4.4837000000000002E-2,-1.9949999999999998E-3,-0.04,-1.4999999999999999E-2,-5.8799999999999998E-4,3000]
["$","2022-02-24","00:49:38.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:39.300","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:39.300","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",0,61.333185,32.125,1080,191.61655300000001,1732.0782750000001,null,32.15,156,33.718034000000003,173.19439600000001,null,null,null,null,null,null,null,null,null,1242.209961,12.6,37.902999999999999,12.6]
["$","2022-02-24","00:49:39.400","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:49:40.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:49:39.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:49:39.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196392;"]
["$","2022-02-24","00:49:39.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:49:39.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.96612;"]
["$","2022-02-24","00:49:39.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:49:39.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.46999;"]
["$","2022-02-24","00:49:40","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:49:40","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","00:49:40.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:49:40.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:49:40.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:49:40.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:49:40.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:49:40.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:49:40.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:41.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:41.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:49:41.200","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,61.507972000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-3.2650999999999999E-2,-2.6719999999999999E-3,2.3333E-2,-8.3330000000000001E-3,-6.9499999999999998E-4,3000]
["$","2022-02-24","00:49:42.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:43","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:43.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:43.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:43.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:44","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","00:49:44","Decrease Buoyancy Fast","SBE41 Message",-0.09,61.691792999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-3.6065E-2,-3.4870000000000001E-3,6.6670000000000002E-3,1.4999999999999999E-2,-7.6000000000000004E-4,3000]
["$","2022-02-24","00:49:44.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:45.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:46.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:46.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:46.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:47.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:47.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","00:49:47.200","Decrease Buoyancy Fast","SBE41 Message",-0.17,62.109158999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-5.2559000000000002E-2,-3.5739999999999999E-3,2.6667E-2,1.6667000000000001E-2,-7.5100000000000004E-4,3000]
["$","2022-02-24","00:49:48.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:49","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:49.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:49.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:49.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:50","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","00:49:50","Decrease Buoyancy Fast","SBE41 Message",-0.08,62.285446,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-6.3098000000000001E-2,-2.3530000000000001E-3,-0.03,-1.6670000000000001E-3,-6.9499999999999998E-4,3000]
["$","2022-02-24","00:49:50.100","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:50.200","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.08,62.436242999999997,32.174999999999997,1130,203.83966599999999,1821.3952770000001,null,32.174999999999997,155,35.412533000000003,182.12609699999999,null,null,null,null,null,null,null,null,null,1243.75,12.6,39.165000999999997,12.6]
["$","2022-02-24","00:49:50.200","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:49:51.600","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:49:51.700","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:49:50.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:49:50.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196434;"]
["$","2022-02-24","00:49:50.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:49:50.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-1.03954;"]
["$","2022-02-24","00:49:50.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:49:50.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.03864;"]
["$","2022-02-24","00:49:50.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:49:50.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","00:49:51.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:49:51.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:49:51.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:49:51.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:49:51.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:49:51.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:49:51.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:49:51.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:51.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:49:51.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:49:52","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:52.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:52.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:53","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:53.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.04]
["$","2022-02-24","00:49:53.200","Decrease Buoyancy Fast","SBE41 Message",0.04,62.674703999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.04,0.04,-6.5087999999999993E-2,-3.97E-4,-0.04,-3.5000000000000003E-2,-6.3500000000000004E-4,3000]
["$","2022-02-24","00:49:54","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:55","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:55","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:55","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:49:55.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:55.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:56","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:56","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:49:56","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,62.971617000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-7.4315999999999993E-2,1.366E-3,3.6666999999999998E-2,-1.6670000000000001E-3,-5.7799999999999995E-4,3000]
["$","2022-02-24","00:49:57","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:58","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:58.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:49:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:49:58.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:49:59","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:49:59.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","00:49:59.200","Decrease Buoyancy Fast","SBE41 Message",-0.05,63.207141,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-9.0900999999999996E-2,2.6649999999999998E-3,-6.6670000000000002E-3,1.4999999999999999E-2,-5.1400000000000003E-4,3000]
["$","2022-02-24","00:50:00","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:01","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:01","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-0.05,63.430210000000002,32.174999999999997,1170,216.04704000000001,1910.4436559999999,null,32.174999999999997,156.5,37.103228999999999,191.030934,null,null,null,null,null,null,null,null,null,1245.3599850000001,12.61,38.168998999999999,12.61]
["$","2022-02-24","00:50:01.100","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:50:01.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:01","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:01.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:01.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"196897;"]
["$","2022-02-24","00:50:01.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:01.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-0.32136;"]
["$","2022-02-24","00:50:01.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:01.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.31309;"]
["$","2022-02-24","00:50:01.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:01.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:01.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","00:50:01.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:01.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:02","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.03]
["$","2022-02-24","00:50:02","Decrease Buoyancy Fast","SBE41 Message",-0.03,63.430210000000002,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.03,-0.03,-9.3081999999999998E-2,3.4979999999999998E-3,-6.6670000000000002E-3,-6.6670000000000002E-3,-4.5899999999999999E-4,3000]
["$","2022-02-24","00:50:02.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:02.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:02.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:02.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:02.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:03","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:04","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:04.500","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:04.500","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:04.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:04.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:05","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:05","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.09]
["$","2022-02-24","00:50:05","Decrease Buoyancy Fast","SBE41 Message",0.09,63.800210999999997,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.09,0.09,-7.1984000000000006E-2,3.5239999999999998E-3,-0.04,-2.3333E-2,-4.4299999999999998E-4,3000]
["$","2022-02-24","00:50:06","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:07","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:07.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:07.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:08","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:08.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:50:08.200","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,64.114885999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-4.7541E-2,2.3960000000000001E-3,5.3332999999999998E-2,6.6670000000000002E-3,-4.7100000000000001E-4,3000]
["$","2022-02-24","00:50:09","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:10","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:10","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:10.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:10.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:11","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:11.100","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","00:50:11.100","Decrease Buoyancy Fast","SBE41 Message",-7.0000000000000007E-2,64.442313999999996,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-3.6160999999999999E-2,2.9100000000000003E-4,0,2.6667E-2,-5.2700000000000002E-4,3000]
["$","2022-02-24","00:50:12","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:12","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",-7.0000000000000007E-2,64.509366999999997,32.15,1175,228.35672099999999,2000.566525,null,32.174999999999997,153,38.811762999999999,200.04322099999999,null,null,null,null,null,null,null,null,null,1247.01001,12.62,38.004002,12.62]
["$","2022-02-24","00:50:12.100","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:12.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:12.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197708;"]
["$","2022-02-24","00:50:12.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:12.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.76077;"]
["$","2022-02-24","00:50:12.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:12.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.46275;"]
["$","2022-02-24","00:50:13.700","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:12.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:12.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","00:50:12.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:12.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:13.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:13.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:13.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:13.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:13.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:13.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:13.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:14.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","00:50:14.200","Decrease Buoyancy Fast","SBE41 Message",-0.05,64.587228999999994,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-2.801E-2,-2.209E-3,-6.6670000000000002E-3,-3.333E-3,-5.9999999999999995E-4,3000]
["$","2022-02-24","00:50:14.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:15.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:16","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:16.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:16.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:16.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:17","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.02]
["$","2022-02-24","00:50:17","Decrease Buoyancy Fast","SBE41 Message",-0.02,64.910131000000007,32.325000000000003,154.5,null,null,null,null,null,null,null,null,-0.02,-0.02,-1.5001E-2,-4.4270000000000004E-3,-0.01,-8.3330000000000001E-3,-6.8199999999999999E-4,3000]
["$","2022-02-24","00:50:17.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:18.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:19.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:19.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:19.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:20.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.01]
["$","2022-02-24","00:50:20.200","Decrease Buoyancy Fast","SBE41 Message",0.01,65.185338999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.01,0.01,-1.1454000000000001E-2,-5.6059999999999999E-3,-0.01,-0.01,-7.4399999999999998E-4,3000]
["$","2022-02-24","00:50:20.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:21.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:22","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:22.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:22.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:22.900","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:22.900","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",0.01,65.570761000000005,32.174999999999997,1155,240.51949999999999,2089.883527,null,32.15,156.5,40.508361000000001,208.97492199999999,null,null,null,null,null,null,null,null,null,1248.48999,12.62,38.801997999999998,12.62]
["$","2022-02-24","00:50:23","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:23","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:23","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"197349;"]
["$","2022-02-24","00:50:23","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.03]
["$","2022-02-24","00:50:23","Decrease Buoyancy Fast","SBE41 Message",0.03,65.570761000000005,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.03,0.03,-2.5864999999999999E-2,-5.1050000000000002E-3,-6.6670000000000002E-3,-8.3330000000000001E-3,-7.67E-4,3000]
["$","2022-02-24","00:50:23.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:23.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-1.20743;"]
["$","2022-02-24","00:50:23.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:23.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"-1.21772;"]
["$","2022-02-24","00:50:23.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:23.600","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","00:50:23.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:23.800","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:24","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:24","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:24.200","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:24.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:24.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:25.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:25.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","00:50:25.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:26.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:27.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:27.200","Decrease Buoyancy Fast","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:50:27.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:28.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:28.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:28.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:29","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.16]
["$","2022-02-24","00:50:29","Decrease Buoyancy Fast","SBE41 Message",0.16,66.085576000000003,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.16,0.16,-4.0897999999999997E-2,-3.0990000000000002E-3,-4.3333000000000003E-2,-2.5000000000000001E-2,-7.6400000000000003E-4,3000]
["$","2022-02-24","00:50:29.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:30.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:31.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:31.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:31.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:31.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:32.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.25]
["$","2022-02-24","00:50:32.200","Decrease Buoyancy Fast","SBE41 Message",0.25,66.310615999999996,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.25,0.25,-3.7883E-2,-6.5700000000000003E-4,-0.03,-3.6666999999999998E-2,-7.85E-4,3000]
["$","2022-02-24","00:50:32.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:33.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:33.800","Decrease Buoyancy Fast","System Data (dBar %full Volts mAmps): ",0.25,66.570903999999999,32.15,1040,252.71638100000001,2179.603462,null,32.15,157,42.206926000000003,217.94691499999999,null,null,null,null,null,null,null,null,null,1250.130005,12.62,38.501998999999998,12.62]
["$","2022-02-24","00:50:33.900","Decrease Buoyancy Fast","Pump motor not faulted"]
["$","2022-02-24","00:50:34.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:35.300","Decrease Buoyancy Fast","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:35.300","Decrease Buoyancy Fast","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:33.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:33.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"194354;"]
["$","2022-02-24","00:50:34","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:34","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:34.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:34.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"0.05560;"]
["$","2022-02-24","00:50:34.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:34.300","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.21171;"]
["$","2022-02-24","00:50:34.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:34.500","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","00:50:34.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:34.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:34.700","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:34.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:34.900","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:35","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.36]
["$","2022-02-24","00:50:35","Decrease Buoyancy Fast","SBE41 Message",0.36,66.570903999999999,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.36,0.36,-1.6070000000000001E-2,1.188E-3,-3.6666999999999998E-2,-3.3333000000000002E-2,-8.5300000000000003E-4,3000]
["$","2022-02-24","00:50:35.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:35.100","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:35.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:35.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:35.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:35.400","Decrease Buoyancy Fast","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:35.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:36.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:37.300","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:37.300","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:37.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:37.700","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:37.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:38","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.42]
["$","2022-02-24","00:50:38","Decrease Buoyancy Fast","SBE41 Message",0.42,66.931781999999998,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.42,0.42,2.1349E-2,1.779E-3,-0.02,-2.8333000000000001E-2,-9.6000000000000002E-4,3000]
["$","2022-02-24","00:50:38.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:39.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:40.600","Decrease Buoyancy Fast","CTD Sending fast pressure"]
["$","2022-02-24","00:50:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:40.800","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:40.800","Decrease Buoyancy Fast","Checking Global Issues."]
["$","2022-02-24","00:50:41.200","Decrease Buoyancy Fast","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.56000000000000005]
["$","2022-02-24","00:50:41.200","Decrease Buoyancy Fast","SBE41 Message",0.56000000000000005,67.205616000000006,32.325000000000003,154.5,null,null,null,null,null,null,null,null,0.56000000000000005,0.56000000000000005,7.8839000000000006E-2,2.7E-4,-4.6667E-2,-3.3333000000000002E-2,-1.1150000000000001E-3,3000]
["$","2022-02-24","00:50:41.300","Decrease Buoyancy Fast","2022-Feb-24T00:50:41Z,Exiting Dec Buocy depth > threshold 0.3 dBar,0.56,67.21,32.15,155.50"]
["$","2022-02-24","00:50:41.300","Decrease Buoyancy Fast","Normal State Exit"]
["$","2022-02-24","00:50:41.300","Descend","Setting Execution Constraint = 1800000"]
["$","2022-02-24","00:50:41.400","Descend","State Entry"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"~?;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,":?;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:50:41.300","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"~?;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,":?;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","00:50:41.400","Descend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:50:41.900","Descend","BE::openMV: Starting valve open"]
["$","2022-02-24","00:50:41.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:42.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:43","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:43","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:43.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:43.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:43.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:43.900","Descend","System Data (dBar %full Volts mAmps): ",0.56000000000000005,67.366259999999997,32.274999999999999,5,261.00328200000001,2262.0705889999999,null,32.274999999999999,148.5,43.743112000000004,226.18019699999999,null,null,null,null,null,null,null,null,null,1251.26001,12.63,38.935001,12.63]
["$","2022-02-24","00:50:44","Descend","Pump motor not faulted"]
["$","2022-02-24","00:50:45.400","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:45.400","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:44","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:44","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:44","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.76]
["$","2022-02-24","00:50:44","Descend","SBE41 Message",0.76,67.366259999999997,32.15,155.5,null,null,null,null,null,null,null,null,0.76,0.76,0.15839400000000001,-3.9449999999999997E-3,-6.6667000000000004E-2,-5.6667000000000002E-2,-1.34E-3,3000]
["$","2022-02-24","00:50:44.200","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:44.200","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:44.400","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:44.400","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:44.600","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:44.600","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:50:44.800","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:44.800","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:45","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:45","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:45.200","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:45.200","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:45.400","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:45.400","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:45.400","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:45.400","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:46.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:46.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:46.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:46.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","00:50:47.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:48.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:48.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:48.200","Descend","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:50:49.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:49.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:49.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:50","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,1.27]
["$","2022-02-24","00:50:50","Descend","SBE41 Message",1.27,67.384682999999995,32.15,155.5,null,null,null,null,null,null,null,null,1.27,1.27,0.25160900000000003,-1.0200000000000001E-2,-0.17,-0.11833299999999999,-1.658E-3,3000]
["$","2022-02-24","00:50:50.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:51.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:52.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:52.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:52.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:52.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:53.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:53.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,1.52]
["$","2022-02-24","00:50:53.200","Descend","SBE41 Message",1.52,67.373531999999997,32.15,155.5,null,null,null,null,null,null,null,null,1.52,1.52,0.35157500000000003,-1.6917999999999999E-2,-8.3333000000000004E-2,-0.126667,-2.062E-3,3000]
["$","2022-02-24","00:50:54.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:54.200","Descend","System Data (dBar %full Volts mAmps): ",1.52,67.371357000000003,32.299999999999997,5,261.06623999999999,2346.283762,null,32.299999999999997,147,45.247686999999999,234.61494500000001,null,null,null,null,null,null,null,null,null,1251.290039,12.64,39.055999999999997,12.64]
["$","2022-02-24","00:50:54.300","Descend","Pump motor not faulted"]
["$","2022-02-24","00:50:55.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:55.700","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:50:55.700","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:50:54.300","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:50:54.300","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:54.500","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:50:54.500","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:54.700","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:50:54.700","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:50:54.900","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:50:54.900","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:50:55","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:55","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:50:55.100","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:50:55.100","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:50:55.300","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:50:55.300","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:50:55.500","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:50:55.500","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:50:55.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:55.700","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:50:55.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:55.700","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:50:55.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:50:56","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,1.78]
["$","2022-02-24","00:50:56","Descend","SBE41 Message",1.78,67.371357000000003,32.15,155.5,null,null,null,null,null,null,null,null,1.78,1.78,0.47111900000000001,-2.2915000000000001E-2,-8.6666999999999994E-2,-8.5000000000000006E-2,-2.5730000000000002E-3,3000]
["$","2022-02-24","00:50:56.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:57.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:58.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:58.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:50:58.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:50:58.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:50:59.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:50:59.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,2.0699999999999998]
["$","2022-02-24","00:50:59.200","Descend","SBE41 Message",2.0699999999999998,67.369152,32.15,155.5,null,null,null,null,null,null,null,null,2.0699999999999998,2.0699999999999998,0.64299399999999995,-2.8049999999999999E-2,-9.6667000000000003E-2,-9.1666999999999998E-2,-3.2450000000000001E-3,3000]
["$","2022-02-24","00:51:00.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:01","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:01","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:01.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:01.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:01.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:02.100","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,2.3199999999999998]
["$","2022-02-24","00:51:02.100","Descend","SBE41 Message",2.3199999999999998,67.377156999999997,32.15,155.5,null,null,null,null,null,null,null,null,2.3199999999999998,2.3199999999999998,0.88953300000000002,-3.3603000000000001E-2,-8.3333000000000004E-2,-0.09,-4.1520000000000003E-3,3000]
["$","2022-02-24","00:51:02.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:03.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:04.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:04.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:04.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:04.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:05.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:05.100","Descend","System Data (dBar %full Volts mAmps): ",2.3199999999999998,67.380388999999994,32.299999999999997,10,261.14625000000001,2436.27232,null,32.299999999999997,146.5,46.860734000000001,243.613801,null,null,null,null,null,null,null,null,null,1251.369995,12.63,39.112999000000002,12.63]
["$","2022-02-24","00:51:05.200","Descend","Pump motor not faulted"]
["$","2022-02-24","00:51:06.600","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:51:06.600","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:51:05.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,2.56]
["$","2022-02-24","00:51:05.200","Descend","SBE41 Message",2.56,67.380388999999994,32.15,155.5,null,null,null,null,null,null,null,null,2.56,2.56,1.189921,-4.2166000000000002E-2,-0.08,-8.1667000000000003E-2,-5.3439999999999998E-3,3000]
["$","2022-02-24","00:51:05.200","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:51:05.200","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:05.400","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:51:05.400","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:05.600","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:51:05.600","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:05.800","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:51:05.800","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:51:06","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:51:06","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:51:06.200","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:51:06.200","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:51:06.400","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:51:06.400","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:51:06.700","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:51:06.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:06.700","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:51:06.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:07.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:07.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:07.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:07.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","00:51:08.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:09.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:09.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:09.200","Descend","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","00:51:10.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:10.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:10.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:11","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,3.09]
["$","2022-02-24","00:51:11","Descend","SBE41 Message",3.09,67.385194999999996,32.15,155.5,null,null,null,null,null,null,null,null,3.09,3.09,1.4968490000000001,-5.5555E-2,-0.17666699999999999,-0.128333,-6.8360000000000001E-3,3000]
["$","2022-02-24","00:51:11.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:12.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:13.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:13.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:13.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:13.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:14.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:14.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,3.43]
["$","2022-02-24","00:51:14.200","Descend","SBE41 Message",3.43,67.373047,32.15,155.5,null,null,null,null,null,null,null,null,3.43,3.43,1.7842720000000001,-7.2261000000000006E-2,-0.113333,-0.14499999999999999,-8.5389999999999997E-3,3000]
["$","2022-02-24","00:51:15.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:16","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:16","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:16.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:16.100","Descend","System Data (dBar %full Volts mAmps): ",3.43,67.376509999999996,32.299999999999997,10,261.25117999999998,2526.3951889999998,null,32.325000000000003,143.5,48.500669000000002,252.61265700000001,null,null,null,null,null,null,null,null,null,1251.530029,12.64,38.758999000000003,12.64]
["$","2022-02-24","00:51:16.200","Descend","Pump motor not faulted"]
["$","2022-02-24","00:51:16.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:17.600","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:51:17.600","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:51:16.200","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:51:16.200","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:16.400","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:51:16.400","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:16.600","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:51:16.600","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:16.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:16.800","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:51:16.800","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:51:17","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:51:17","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:51:17","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,3.77]
["$","2022-02-24","00:51:17","Descend","SBE41 Message",3.77,67.376509999999996,32.15,155.5,null,null,null,null,null,null,null,null,3.77,3.77,2.060225,-8.7763999999999995E-2,-0.113333,-0.113333,-1.0416999999999999E-2,3000]
["$","2022-02-24","00:51:17.200","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:51:17.200","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:51:17.400","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:51:17.400","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:51:17.600","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:51:17.600","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:17.600","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:51:17.600","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:18","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:19","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:19.500","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:19.500","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:19.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:19.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:20","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,4.09]
["$","2022-02-24","00:51:20","Descend","SBE41 Message",4.09,67.377459999999999,32.15,155.5,null,null,null,null,null,null,null,null,4.09,4.09,2.3495210000000002,-9.7588999999999995E-2,-0.106667,-0.11,-1.2474000000000001E-2,3000]
["$","2022-02-24","00:51:20.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:21.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:22.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:22.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:22.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:22.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:23.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:23.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,4.4800000000000004]
["$","2022-02-24","00:51:23.200","Descend","SBE41 Message",4.4800000000000004,67.375208999999998,32.15,155.5,null,null,null,null,null,null,null,null,4.4800000000000004,4.4800000000000004,2.6757070000000001,-0.100634,-0.13,-0.11833299999999999,-1.4737E-2,3000]
["$","2022-02-24","00:51:24.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:25","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:25","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:25.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:25.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:25.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:26.100","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,4.71]
["$","2022-02-24","00:51:26.100","Descend","SBE41 Message",4.71,67.378809000000004,32.15,155.5,null,null,null,null,null,null,null,null,4.71,4.71,3.0375640000000002,-0.100412,-7.6666999999999999E-2,-0.10333299999999999,-1.7229999999999999E-2,3000]
["$","2022-02-24","00:51:26.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:26.100","Descend","System Data (dBar %full Volts mAmps): ",4.71,67.388374999999996,32.325000000000003,5,261.32725499999998,2608.4593810000001,null,32.325000000000003,146.5,49.966419999999999,260.83250700000002,null,null,null,null,null,null,null,null,null,1251.5600589999999,12.64,38.737000000000002,12.64]
["$","2022-02-24","00:51:26.200","Descend","Pump motor not faulted"]
["$","2022-02-24","00:51:27.600","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:51:27.600","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:51:26.200","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:51:26.200","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:26.400","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:51:26.400","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:26.600","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:51:26.600","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:26.800","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:51:26.800","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:51:27","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:51:27","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:51:27.200","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:51:27.200","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:51:27.400","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:51:27.400","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:51:27.700","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:51:27.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:27.700","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:51:27.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:28","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:28.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:28.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:28.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:29","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:29.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,5.05]
["$","2022-02-24","00:51:29.200","Descend","SBE41 Message",5.05,67.387358000000006,32.15,155.5,null,null,null,null,null,null,null,null,5.05,5.05,3.4069440000000002,-0.102191,-0.113333,-9.5000000000000001E-2,-1.993E-2,3000]
["$","2022-02-24","00:51:30","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:31","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:31","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:31","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:31.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:31.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:32","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:32","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,5.35]
["$","2022-02-24","00:51:32","Descend","SBE41 Message",5.35,67.383105,32.15,155.5,null,null,null,null,null,null,null,null,5.35,5.35,3.7616990000000001,-0.10806,-0.1,-0.106667,-2.2801999999999999E-2,3000]
["$","2022-02-24","00:51:33","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:34","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:34.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:34.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:34.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:35","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:35.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,5.71]
["$","2022-02-24","00:51:35.200","Descend","SBE41 Message",5.71,67.373375999999993,32.15,155.5,null,null,null,null,null,null,null,null,5.71,5.71,4.1002000000000001,-0.11565300000000001,-0.12,-0.11,-2.5808000000000001E-2,3000]
["$","2022-02-24","00:51:36","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:37","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:37","Descend","System Data (dBar %full Volts mAmps): ",5.71,67.383714999999995,32.325000000000003,5,261.41644600000001,2697.50776,null,32.325000000000003,146,51.55612,269.737345,null,null,null,null,null,null,null,null,null,1251.6099850000001,12.65,38.294998,12.65]
["$","2022-02-24","00:51:37.100","Descend","Pump motor not faulted"]
["$","2022-02-24","00:51:37.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:38.500","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:51:38.500","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:51:37","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:37","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:37.100","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:51:37.100","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:37.300","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:51:37.300","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:37.500","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:51:37.500","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:37.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:37.700","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:51:37.700","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:51:37.900","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:51:37.900","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:51:38","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,6.01]
["$","2022-02-24","00:51:38","Descend","SBE41 Message",6.01,67.383714999999995,32.15,155.5,null,null,null,null,null,null,null,null,6.01,6.01,4.4248830000000003,-0.121223,-0.1,-0.11,-2.8934999999999999E-2,3000]
["$","2022-02-24","00:51:38.100","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:51:38.100","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:51:38.300","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:51:38.300","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:51:38.500","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:51:38.500","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:38.500","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:51:38.500","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:39","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:40","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:40.400","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:40.400","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:40.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:40.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:41","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:41","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,6.37]
["$","2022-02-24","00:51:41","Descend","SBE41 Message",6.37,67.375658999999999,32.15,155.5,null,null,null,null,null,null,null,null,6.37,6.37,4.7383829999999998,-0.12248000000000001,-0.12,-0.11,-3.2152E-2,3000]
["$","2022-02-24","00:51:42","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:43","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:43.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:43.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:43.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:44","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:44.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,6.71]
["$","2022-02-24","00:51:44.200","Descend","SBE41 Message",6.71,67.373706999999996,32.15,155.5,null,null,null,null,null,null,null,null,6.71,6.71,5.0502370000000001,-0.119561,-0.113333,-0.11666700000000001,-3.5437000000000003E-2,3000]
["$","2022-02-24","00:51:45","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:46","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:46","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:46","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:46.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:46.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:47","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:47.100","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,7.07]
["$","2022-02-24","00:51:47.100","Descend","SBE41 Message",7.07,67.372551999999999,32.15,155.5,null,null,null,null,null,null,null,null,7.07,7.07,5.3694160000000002,-0.11482000000000001,-0.12,-0.11666700000000001,-3.8810999999999998E-2,3000]
["$","2022-02-24","00:51:48","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:48","Descend","System Data (dBar %full Volts mAmps): ",7.07,67.372733999999994,32.325000000000003,5,261.48465099999999,2787.6306300000001,null,32.325000000000003,143.5,53.162871000000003,278.74963200000002,null,null,null,null,null,null,null,null,null,1251.6099850000001,12.64,38.007998999999998,12.64]
["$","2022-02-24","00:51:48.100","Descend","Pump motor not faulted"]
["$","2022-02-24","00:51:49.500","Descend","getting Elmo acceleration limit"]
["$","2022-02-24","00:51:49.500","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:51:48.100","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:51:48.100","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:48.300","Descend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:51:48.300","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:48.500","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:51:48.500","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:48.700","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:51:49.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:48.700","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:51:48.900","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:51:48.900","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:51:49.100","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:51:49.100","Descend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:51:49.300","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:51:49.300","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:51:49.500","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:51:49.500","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:49.500","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:51:49.500","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:51:49.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:49.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:49.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:50.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,7.41]
["$","2022-02-24","00:51:50.200","Descend","SBE41 Message",7.41,67.387585999999999,32.15,155.5,null,null,null,null,null,null,null,null,7.41,7.41,5.6967179999999997,-0.111002,-0.113333,-0.11666700000000001,-4.2254E-2,3000]
["$","2022-02-24","00:51:50.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:51.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:52","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:52","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:52.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:52.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:52.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:53.100","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,7.71]
["$","2022-02-24","00:51:53.100","Descend","SBE41 Message",7.71,67.365510999999998,32.15,155.5,null,null,null,null,null,null,null,null,7.71,7.71,6.0302579999999999,-0.109287,-0.1,-0.106667,-4.5766000000000001E-2,3000]
["$","2022-02-24","00:51:53.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:54.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:55.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:55.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:55.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:55.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:56.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,8.09]
["$","2022-02-24","00:51:56.200","Descend","SBE41 Message",8.09,67.377598000000006,32.15,155.5,null,null,null,null,null,null,null,null,8.09,8.09,6.3700890000000001,-0.109502,-0.126667,-0.113333,-4.9304000000000001E-2,3000]
["$","2022-02-24","00:51:56.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:57.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:58","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:51:58","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:51:58.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:51:58.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:51:58.900","Descend","Checking Global Issues."]
["$","2022-02-24","00:51:59.400","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:51:59.800","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:52:03.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:52:08.800","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:10.500","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:52:11.800","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:16.800","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:22.300","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:52:22.400","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:52:25.700","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:31.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:52:32.400","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:52:34.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:52:38.600","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:42.900","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:52:44","Descend","SBE41 Message",13.63,67.387022000000002,32.15,155.5,null,null,null,null,null,null,null,null,13.63,13.63,11.873355,-0.11995500000000001,-0.106667,-0.11833299999999999,-0.100353,3000]
["$","2022-02-24","00:52:49.600","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:53.600","Descend","Checking Global Issues."]
["$","2022-02-24","00:52:54.700","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:52:56.400","Descend","Checking Global Issues."]
["$","2022-02-24","00:53:02.200","Descend","SBE41 Message",15.82,67.378823999999994,32.15,155.5,null,null,null,null,null,null,null,null,15.82,15.82,14.010498999999999,-0.12194099999999999,-0.13,-0.123333,-0.110816,3000]
["$","2022-02-24","00:53:05","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:53:06","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:53:11","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,16.82]
["$","2022-02-24","00:53:16.900","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:53:16.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:53:19","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:53:25.400","Descend","Checking Global Issues."]
["$","2022-02-24","00:53:26.900","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:53:28.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:53:34.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:53:37.400","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:53:38.600","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:53:43.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:53:47.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:53:49.100","Descend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:53:52","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:53:52","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:53:57.100","Descend","Checking Global Issues."]
["$","2022-02-24","00:54:00.700","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:54:00.700","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:54:05","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,23.07]
["$","2022-02-24","00:54:11.500","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:54:11","Descend","SBE41 Message",23.879999000000002,67.360870000000006,32.15,155.5,null,null,null,null,null,null,null,null,23.88,23.879999000000002,22.038558999999999,-0.116342,-0.13666700000000001,-0.13500000000000001,-0.11776499999999999,3000]
["$","2022-02-24","00:54:14","Descend","Checking Global Issues."]
["$","2022-02-24","00:54:19.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:54:21.700","Descend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:54:22.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:54:28.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:54:33.400","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:54:33.200","Descend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","00:54:37.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:54:42.600","Descend","Descend glide on"]
["$","2022-02-24","00:54:42.800","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:54:44","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,27.89]
["$","2022-02-24","00:54:46.700","Descend","Checking Global Issues."]
["$","2022-02-24","00:54:52.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:54:54.200","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:54:55.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:55:01.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:55:06.100","Descend","getting Elmo deacceleration limit"]
["$","2022-02-24","00:55:05.900","Descend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","00:55:10","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:55:15.500","Descend","Checking Global Issues."]
["$","2022-02-24","00:55:16.200","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:55:18.500","Descend","Checking Global Issues."]
["$","2022-02-24","00:55:25","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:55:26.600","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:55:28","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:55:32","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,34.020000000000003]
["$","2022-02-24","00:55:37.400","Descend","System Data (dBar %full Volts mAmps): ",34.290000999999997,67.378039999999999,32.35,5,263.18190499999997,4668.9287379999996,null,32.35,146,86.872904000000005,466.86601200000001,null,null,null,null,null,null,null,null,null,1251.290039,12.67,38.896000000000001,12.67]
["$","2022-02-24","00:55:38.300","Descend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:55:41.100","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,35.14]
["$","2022-02-24","00:55:46.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:55:48.800","Descend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:55:49.800","Descend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:55:49.800","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:55:55.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:55:59.300","Descend","System Data (dBar %full Volts mAmps): ",37.25,67.378048000000007,32.35,10,263.33798999999999,4849.0401650000003,null,32.35,147.5,90.085224999999994,484.87715400000002,null,null,null,null,null,null,null,null,null,1251.339966,12.67,38.740001999999997,12.67]
["$","2022-02-24","00:56:00.900","Descend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:56:04","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","00:56:08.300","Descend","Checking Global Issues."]
["$","2022-02-24","00:56:10.800","Descend","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:56:12.200","Descend","Checking Global Issues."]
["$","2022-02-24","00:56:18.300","Descend","Checking Global Issues."]
["$","2022-02-24","00:56:21.400","Descend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:56:22.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:56:26","Descend","SBE41 Message",40.720001000000003,67.372715999999997,32.15,155.5,null,null,null,null,null,null,null,null,40.72,40.720001000000003,38.803722,-0.13111999999999999,-0.12,-0.12,-0.12635399999999999,3000]
["$","2022-02-24","00:56:31.700","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:56:32.800","Descend","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","00:56:35.200","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,41.93]
["$","2022-02-24","00:56:40.800","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:56:43.600","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","00:56:44.500","Descend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:56:49.600","Descend","CTD Sending fast pressure"]
["$","2022-02-24","00:56:54","Descend","System Data (dBar %full Volts mAmps): ",44.110000999999997,67.370616999999996,32.35,10,263.72229800000002,5297.1025970000001,null,32.35,144,98.075959999999995,529.69682899999998,null,null,null,null,null,null,null,null,null,1251.3100589999999,12.65,38.728999999999999,12.65]
["$","2022-02-24","00:56:55.100","Descend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","00:56:58","Descend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","00:57:02.300","Descend","Normal State Exit"]
["$","2022-02-24","00:57:02.300","Anchor","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","00:57:02.400","Anchor","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","00:57:12.400","Anchor","[MSC] RX: "]
["$","2022-02-24","00:57:12.700","Anchor","[MSC] RX:   "]
["$","2022-02-24","00:57:13","Anchor","[MSC] RX:   Last Error     Time = Thu Jan  1 00:00:00 1970  "]
["$","2022-02-24","00:57:13.200","Anchor","[MSC] RX:   "]
["$","2022-02-24","00:57:13.300","Anchor","Optode: Disable text"]
["$","2022-02-24","00:57:15.200","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Last Calibration,4330,2707,2016-08-22  "]
["$","2022-02-24","00:57:16","Anchor","Sending Optode Get DataXML"]
["$","2022-02-24","00:57:18.100","Anchor","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S/N: 0545 "]
["$","2022-02-24","00:57:16.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:57:17.200","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output,4330,2707,O2Concentration  "]
["$","2022-02-24","00:57:17.700","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Geographic Position,4330,2707,60.323605,5.37225  "]
["$","2022-02-24","00:57:17.700","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","00:57:19.300","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"0\" Descr=\"System Control\" Type=\"VT_ARRAY|VT_I2\" Access=\"R3W4\">0;0;0</Property>  "]
["$","2022-02-24","00:57:20.200","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,</PropertyCategory>  "]
["$","2022-02-24","00:57:21.800","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"3\" Descr=\"PhaseCoef\" Type=\"VT_ARRAY|VT_R4\" Access=\"R1W3\">6.919999E-01;1.000000E+00;0.000000E+00;0.000000E+00</Property>  "]
["$","2022-02-24","00:57:21.800","Anchor","Checking Global Issues."]
["$","2022-02-24","00:57:23.800","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,<PropertyCategory ID=\"5\" Descr=\"Sample Settings\">  "]
["$","2022-02-24","00:57:24.900","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,</PropertyCategory>  "]
["$","2022-02-24","00:57:26.900","Anchor","Pump motor not faulted"]
["$","2022-02-24","00:57:27","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,</PropertyCategory>  "]
["$","2022-02-24","00:57:27.700","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:57:28.200","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,<Point ID=\"3\" Descr=\"Temperature\" Type=\"VT_R4\" Unit=\"Deg.C\" Format=\"%0.3f\" RangeMin=\"-5\" RangeMax=\"40\" />  "]
["$","2022-02-24","00:57:29.700","Anchor","Checking Global Issues."]
["$","2022-02-24","00:57:38","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:57:42.600","Anchor","Checking Global Issues."]
["$","2022-02-24","00:57:48.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","00:57:50.100","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","00:58:00.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","00:58:01","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:58:02.400","Anchor","Sending FLBB run command"]
["$","2022-02-24","00:58:07.900","Anchor","FLBB post: /99/99,99:99:99,695,105,700,1828,551  "]
["$","2022-02-24","00:58:10.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:58:11.200","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:58:15.200","Anchor","[MSC] TX: W"]
["$","2022-02-24","00:58:21.500","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:58:22.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:58:29.600","Anchor","[MSC] RX: 0x7A29,pH,02/24/2022 00:58:28,1645664287,44.81,10.6715,33.6818,46,6,0,13.15,38.69,11.672,4.580e-02,7.1234,3.550,-0.964262,0.000016,-0.920896,0.000017,+9.440e-10,+4.883e-11  "]
["$","2022-02-24","00:58:32.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","00:58:33.200","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:58:43.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","00:58:44.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:58:55.400","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","00:58:55.400","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","00:59:06.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","00:59:05.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","00:59:15.500","Anchor","Checking Global Issues."]
["$","2022-02-24","00:59:16.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","00:59:25.400","Anchor","Checking Global Issues."]
["$","2022-02-24","00:59:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","00:59:35.200","Anchor","Checking Global Issues."]
["$","2022-02-24","00:59:38.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","00:59:38.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","00:59:48.800","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","00:59:52.900","Anchor","Checking Global Issues."]
["$","2022-02-24","00:59:53.900","Anchor","Checking Global Issues."]
["$","2022-02-24","00:59:59.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:00:02.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:00:10.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:00:11.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:00:20.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:00:22.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:00:31.600","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:00:33","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:00:43.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:00:49.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:00:53.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:00:54.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:01:04","Anchor","System Data (dBar %full Volts mAmps): ",44.810001,67.371196999999995,32.35,5,265.55202700000001,7348.0358530000003,null,32.35,167,140.71572499999999,734.77672299999995,null,null,null,null,null,null,null,null,null,1251.150024,12.58,38.521999000000001,12.58]
["$","2022-02-24","01:01:05.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:01:13.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:01:16","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:01:25.800","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:01:26.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:01:32.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:01:37.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:01:42.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:01:47.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:01:56.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:01:58.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:02:00.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:02:09.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:02:10.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:02:20.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:02:21.600","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:02:27.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:02:32.400","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:02:41.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:02:43","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:02:52.600","Anchor","System Data (dBar %full Volts mAmps): ",44.810001,67.373515999999995,32.35,10,266.35605800000002,8238.6539539999994,null,32.35,166.5,158.82190900000001,823.83853299999998,null,null,null,null,null,null,null,null,null,1250.9399410000001,12.55,38.495998,12.55]
["$","2022-02-24","01:02:53.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:03:02.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:04","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:03:11.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:12.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:15.200","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:03:21.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:25.900","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:03:37.500","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:03:36.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:03:39.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:47.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:03:49.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:03:58","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:03:59.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:04:08.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:04:10.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:04:21","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:04:21.100","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:04:30.500","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:04:31.700","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:04:36.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:04:42.300","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:04:51.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:04:53","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:05:00.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:05:03.800","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:05:09.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:05:14.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:05:18.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:05:25.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:05:28.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:05:35.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:05:38.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:05:46.700","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:05:47.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:05:57.300","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:05:58.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:06:09.600","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:06:09.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:06:19","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:06:19.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:06:29.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:06:30.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:06:30.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:06:39.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:06:41.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:06:49.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:06:53.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:06:58.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:07:03","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:07:08.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:07:13.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:07:17","Anchor","Checking Global Issues."]
["$","2022-02-24","01:07:24.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:07:25.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:07:35","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:07:36.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:07:45.800","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:07:47.300","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:07:58.100","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:07:57.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:08:02.400","Anchor","Sci Logger sending sample FLBB"]
["$","2022-02-24","01:08:06.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:08:08.400","Anchor","[MSC] Starting ISUS Sample"]
["$","2022-02-24","01:08:07.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:08:14.400","Anchor","[MSC] TX: W"]
["$","2022-02-24","01:08:17.400","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:08:19.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:08:27.400","Anchor","[MSC] RX: 0xCACD,pH,02/24/2022 01:08:26,1645664888,44.58,10.6336,33.6886,47,6,0,12.83,39.07,11.672,4.580e-02,7.1234,3.550,-0.965220,0.000018,-0.920814,0.000008,+4.875e-09,-4.395e-09  "]
["$","2022-02-24","01:08:28.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:08:31.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:08:38.900","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:08:41.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:08:50.800","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:08:50.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:09:00.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:09:01.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:09:12.500","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:09:12.500","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:09:23.300","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:09:22.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:09:32.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:09:32.700","Anchor","System Data (dBar %full Volts mAmps): ",44.580002,67.365713999999997,32.325000000000003,5,269.00293499999998,11519.3413,null,32.35,166,226.46377200000001,1151.893836,null,null,null,null,null,null,null,null,null,1250.599976,12.43,38.375999,12.43]
["$","2022-02-24","01:09:33.800","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:09:43.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:09:44.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:09:52.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:09:55.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:10:01.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:10:06","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:10:11.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:10:16.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:10:21","Anchor","Checking Global Issues."]
["$","2022-02-24","01:10:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:10:28.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:10:38.100","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:10:39.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:10:48.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:10:50.200","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:11:01","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:11:01","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:11:10.500","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:11:11.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:11:21.200","Anchor","System Data (dBar %full Volts mAmps): ",44.580002,67.366134000000002,32.325000000000003,5,269.81877100000003,12409.42215,null,32.325000000000003,166,244.56903700000001,1240.9153530000001,null,null,null,null,null,null,null,null,null,1250.48999,12.43,38.175998999999997,12.43]
["$","2022-02-24","01:11:22.300","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:11:32.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:11:33.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:11:40.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:11:43.800","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:11:49.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:11:54.500","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:11:59.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:12:05.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:12:10.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:12:15.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:12:17.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:12:26.600","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:12:27.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:12:37.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:12:38.700","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:12:38.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:12:49.500","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:12:49.500","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:12:59","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:13:00.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:13:09.800","Anchor","System Data (dBar %full Volts mAmps): ",44.580002,67.356382999999994,32.325000000000003,5,270.68969600000003,13299.50301,null,32.325000000000003,166.5,262.63587200000001,1329.9234389999999,null,null,null,null,null,null,null,null,null,1250.410034,12.41,37.985999999999997,12.41]
["$","2022-02-24","01:13:11.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:13:19.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:13:21.500","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:13:29.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:13:32.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:13:38.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:13:43","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:13:49.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:13:53.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:13:57","Anchor","Checking Global Issues."]
["$","2022-02-24","01:14:04.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:14:06.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:14:15.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:14:16.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:14:26.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:14:27.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:14:38.100","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:14:38.100","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:14:47.500","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:14:48.700","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:14:58.400","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:14:59.400","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:15:08.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:10","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:15:18","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:20.900","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:15:27.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:30.800","Anchor","System Data (dBar %full Volts mAmps): ",44.580002,67.356983,32.325000000000003,10,271.731133,14456.326069999999,null,32.325000000000003,168,286.11726099999998,1445.592314,null,null,null,null,null,null,null,null,null,1250.380005,12.38,38.150002000000001,12.38]
["$","2022-02-24","01:15:35.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:42.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:15:45.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:52.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:15:55.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:15:57.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:16:03.700","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:16:04.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:16:14.300","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:16:15.800","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:16:26.600","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:16:26.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:16:36.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:16:37.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:16:46.800","Anchor","System Data (dBar %full Volts mAmps): ",44.580002,67.351833999999997,32.325000000000003,10,272.469583,15079.530409999999,null,32.325000000000003,166.5,298.84732100000002,1507.912748,null,null,null,null,null,null,null,null,null,1250.3000489999999,12.36,38.548000000000002,12.36]
["$","2022-02-24","01:16:47.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:16:56.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:16:58.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:17:06.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:17:10","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:17:15.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:17:20","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:17:25.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:17:30.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:17:34","Anchor","Checking Global Issues."]
["$","2022-02-24","01:17:41.900","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:17:42.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:17:52.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:17:53.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:18:02.400","Anchor","Sending Optode Do Sample"]
["$","2022-02-24","01:18:03","Anchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>pts  "]
["$","2022-02-24","01:18:03.800","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:18:05.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:18:12.900","Anchor","[MSC] TX: W"]
["$","2022-02-24","01:18:13.800","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:18:19.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:18:25.300","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:18:25.100","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:18:30.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:18:34.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:18:39.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:18:46.100","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:18:48.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:18:56.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:18:58.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:19:02.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:19:07.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:19:08.800","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:19:18.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:19:19.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:19:30.500","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:19:30.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:19:40.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:19:41.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:19:50.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:19:51.800","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:20:00.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:20:02.500","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:20:12.400","Anchor","System Data (dBar %full Volts mAmps): ",44.689999,67.350544999999997,32.325000000000003,10,274.446214,16766.077160000001,null,32.325000000000003,166,334.01956300000001,1676.567423,null,null,null,null,null,null,null,null,null,1250.170044,12.33,38.035998999999997,12.33]
["$","2022-02-24","01:20:13.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:20:18.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:20:24","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:20:28.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:20:34.600","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:20:38","Anchor","Checking Global Issues."]
["$","2022-02-24","01:20:45.900","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:20:46.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:20:56","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:20:57.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:21:06.800","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:21:08.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:21:19.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:21:18.500","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:21:28.400","Anchor","System Data (dBar %full Volts mAmps): ",44.689999,67.366877000000002,32.325000000000003,5,275.17679399999997,17389.012879999998,null,32.325000000000003,164,346.70568300000002,1738.860995,null,null,null,null,null,null,null,null,null,1250.089966,12.32,38.841000000000001,12.32]
["$","2022-02-24","01:21:29.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:21:39.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:21:40.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:21:49.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:21:50.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:21:57","Anchor","Checking Global Issues."]
["$","2022-02-24","01:22:01.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:22:06.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:22:12.500","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:22:16.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:22:23.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:22:24.200","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:22:25.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:22:33.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:22:35.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:22:44.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:22:45.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:22:55.300","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:23:02.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:23:07.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:23:07.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:23:17","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:23:18.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:23:27.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:23:28.500","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:23:36.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:23:39.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:23:46.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:23:50.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:23:56.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:24:01.100","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:24:01.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:24:11.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:24:14.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:24:22.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:24:23.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:24:33","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:24:34.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:24:45.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:24:45.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:24:56.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:24:56","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:25:05.600","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:25:06.800","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:25:10.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:25:17.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:25:25.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:25:28.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:25:35","Anchor","Checking Global Issues."]
["$","2022-02-24","01:25:38.800","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:25:39","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:25:49.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:25:49.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:25:53.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:26:00.300","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:26:03.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:26:10.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:26:21.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:26:21.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:26:23","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:26:33.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:26:33.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:26:44.700","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:26:44.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:26:53","Anchor","Checking Global Issues."]
["$","2022-02-24","01:26:55.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:27:04.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:06","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:27:14.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:16.600","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:27:23.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:27:32.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:37.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:27:42.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:48.800","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:27:52.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:27:59.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:28:00.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:28:04.500","Anchor","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",2.8400000000000002E-2,2.4299999999999999E-2,1.26E-2,0.22950000000000001]
["$","2022-02-24","01:28:08.100","Anchor","SciLogger: Setting get PH true"]
["$","2022-02-24","01:28:11.500","Anchor","[MSC] Timeout for CommandWake"]
["$","2022-02-24","01:28:11.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:28:17.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:28:22.500","Anchor","[MSC] Data: 0x505F,A,02/24/2022 01:28:20,1645666088,44.73,10.5894,33.6976,49,6,0,0,12.76,38.93,11.500,5.662e-01,18412.00,1126.00,1016.52,5.39,33.70,29.29,7.639e-04,36,77,288B2D58312233DA3588366636A9368B3636360535DD361636B1379839003AE83D5640344389475E4B8D501754B359585DCF61C5651E678068CC68EF67CC658D62715EA35A66562251D04DBA4A1646C143C54143,1030.6  "]
["$","2022-02-24","01:28:22.800","Anchor","[MSC] Done Sampling."]
["$","2022-02-24","01:28:29.300","Anchor","[MSC] Post pH: -0.965494"]
["$","2022-02-24","01:28:32.500","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:28:37.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:28:38.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:28:44.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:28:46.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:28:54","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:28:56.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:29:04.700","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:29:06.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:29:15.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:29:16.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:29:27.600","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:29:27.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:29:38.400","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:29:38.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:29:47.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:29:49.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:29:57.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:29:59.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:30:07.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:30:10.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:30:17.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:30:21","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:30:27.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:30:31.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:30:35","Anchor","Checking Global Issues."]
["$","2022-02-24","01:30:42.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:30:44.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:30:53.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:30:54.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:31:03.800","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:31:05.200","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:31:16.100","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:31:16.100","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:31:26.900","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:31:26.700","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:31:36.400","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:31:37.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:31:46.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:31:48.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:31:56","Anchor","Checking Global Issues."]
["$","2022-02-24","01:31:58.900","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:31:58.900","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:32:05.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:32:09.500","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:32:14.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:32:20.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:32:24.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:32:31","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:32:33.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:32:41.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:32:42.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:32:52.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:32:53.800","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:33:04.600","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:33:04.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:33:15.400","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:33:15.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:33:24.800","Anchor","System Data (dBar %full Volts mAmps): ",44.73,67.361643000000001,32.299999999999997,10,281.18276500000002,23264.19123,null,32.299999999999997,166.5,466.77642700000001,2326.3653989999998,null,null,null,null,null,null,null,null,null,1249.8000489999999,12.24,38.305,12.24]
["$","2022-02-24","01:33:25.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:33:35.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:33:36.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:33:44.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:33:47.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:33:53.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:33:58","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:34:03.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:34:08.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:34:13","Anchor","Checking Global Issues."]
["$","2022-02-24","01:34:19.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:34:20.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:34:30.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:34:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:34:40.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:34:42.300","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:34:53.100","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:34:51.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:35:02.500","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:35:03.800","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:35:13.300","Anchor","System Data (dBar %full Volts mAmps): ",44.73,67.356258999999994,32.299999999999997,5,282.00253600000002,24154.00347,null,32.299999999999997,167,484.782533,2415.346622,null,null,null,null,null,null,null,null,null,1249.670044,12.24,38.158999999999999,12.24]
["$","2022-02-24","01:35:14.400","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:35:14.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:35:24.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:35:25.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:35:33","Anchor","Checking Global Issues."]
["$","2022-02-24","01:35:35.900","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:35:42.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:35:46.600","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:35:51.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:35:57.400","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:36:05.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:36:08.100","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:36:10.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:36:18.700","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:36:20.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:36:29.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:36:31.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:36:41.600","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:36:41.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:36:52.500","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:36:52.300","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:37:01.800","Anchor","System Data (dBar %full Volts mAmps): ",44.73,67.362954000000002,32.299999999999997,5,282.81181400000003,25044.084320000002,null,32.299999999999997,165,502.87599399999999,2504.3547079999998,null,null,null,null,null,null,null,null,null,1249.6099850000001,12.22,38.789000999999999,12.22]
["$","2022-02-24","01:37:03.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:37:14.200","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:37:13.600","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:37:21.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:37:24.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:37:31.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:37:35.100","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:37:42.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:37:45.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:37:49.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:37:56.600","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:37:58.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:38:02.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:38:08.500","Anchor","FLBB Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"/99/99,99:99:99,695,92,700,1352,546  "]
["$","2022-02-24","01:38:08.600","Anchor","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","01:38:08.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:38:16","Anchor","Checking Global Issues."]
["$","2022-02-24","01:38:17.900","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:38:18.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:38:21.300","Anchor","[MSC] Starting pH sample"]
["$","2022-02-24","01:38:27.900","Anchor","[MSC] Done Sampling."]
["$","2022-02-24","01:38:29.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:38:35.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:38:39.700","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:38:45.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:38:50.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:38:55.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:39:01.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:39:03.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:39:11.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:39:13.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:39:22.500","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:39:23.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:39:33.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:39:39.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:39:45.400","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:39:45.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:39:54.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:39:56","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:40:05.600","Anchor","System Data (dBar %full Volts mAmps): ",44.75,67.353831,32.299999999999997,10,284.031633,26550.788270000001,null,32.299999999999997,166.5,534.37723600000004,2655.0251020000001,null,null,null,null,null,null,null,null,null,1249.5600589999999,12.21,38.112999000000002,12.21]
["$","2022-02-24","01:40:06.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:40:07.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:40:17.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:40:24.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:40:28.200","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:40:34.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:40:38.800","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:40:39.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:40:49.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:40:51.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:41:00.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:41:01.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:41:11","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:41:12.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:41:18.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:41:23.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:41:33.900","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:41:33.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:41:33.900","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:41:43.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:41:48.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:41:54.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:41:55.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:42:03.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:42:05.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:42:13.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:42:16.700","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:42:28.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:42:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:42:31.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:42:38","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:42:41.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:42:48.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:42:51.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:42:59.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:43:00.700","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:43:10.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:43:11.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:43:22.400","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:43:22.400","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:43:26.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:43:33","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:43:42.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:43:43.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:43:52.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:43:54.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:44:02.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:44:04.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:44:10.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:44:15.800","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:44:20","Anchor","Checking Global Issues."]
["$","2022-02-24","01:44:26.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:44:29.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:44:36.800","Anchor","System Data (dBar %full Volts mAmps): ",44.75,67.356791999999999,32.299999999999997,10,286.10794900000002,28775.52032,null,32.299999999999997,166.5,579.47578999999996,2877.4983080000002,null,null,null,null,null,null,null,null,null,1249.4799800000001,12.2,38.144001000000003,12.2]
["$","2022-02-24","01:44:38.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:44:47.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:44:49.200","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:44:49.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:44:58.600","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:45:00.100","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:45:10.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:45:10.700","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:45:20.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:45:21.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:45:31.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:45:32.200","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:45:40.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:45:42.800","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:45:49.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:45:53.500","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:45:59.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:46:04.400","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:46:09.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:46:14.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:46:17.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:46:25.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:46:27.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:46:36.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:46:37.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:46:47.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:46:48.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:46:59.400","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:46:59.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:47:08.900","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:47:10.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:47:19.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:47:20.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:47:26.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:47:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:47:38.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:47:42","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:47:48.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:47:52.900","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:47:56","Anchor","Checking Global Issues."]
["$","2022-02-24","01:48:02.500","Anchor","Sci Logger sending sample Radiometer"]
["$","2022-02-24","01:48:03.300","Anchor","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","01:48:03.300","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:48:04.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:48:06.800","Anchor","SBE41 Message",44.619999,67.348641000000001,32.15,155.5,null,null,null,null,null,null,null,null,"   44.62, 10.5763, 33.6997  ",44.619999,44.703921000000001,-0.105334,4.3333999999999998E-2,1.8332999999999999E-2,-3.326E-3,3000]
["$","2022-02-24","01:48:14.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:48:20.900","Anchor","[MSC] RX: 0x7C3B,A,02/24/2022 01:48:21,1645667286,44.62,10.5763,33.6997,51,6,0,0,12.72,38.96,11.500,5.678e-01,18220.00,1123.00,1014.69,4.93,33.70,29.40,7.825e-04,36,77,27A22C61301B32D7347E35573598357B352434F534EC351435A2369337FB39DD3C353EFF425B461D4A484EB6534A57E45C4C602E638265E467296748663663EE60F35D2558F254B150724C6E48D645824296401F,915.2  "]
["$","2022-02-24","01:48:21","Anchor","[MSC] Done Sampling."]
["$","2022-02-24","01:48:24.300","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:48:25.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:48:34.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:48:36","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:48:43.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:48:46.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:48:52.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:48:57.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:49:02.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:49:07.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:49:12.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:49:18.600","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:49:21.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:49:29.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:49:30.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:49:40.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:49:41.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:49:52.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:49:52.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:50:01.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:50:03","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:50:12.500","Anchor","System Data (dBar %full Volts mAmps): ",44.619999,67.364789999999999,32.274999999999999,5,288.55808000000002,31528.498640000002,null,32.274999999999999,167,636.30126600000006,3152.7827080000002,null,null,null,null,null,null,null,null,null,1249.369995,12.18,37.811999999999998,12.18]
["$","2022-02-24","01:50:13.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:50:23.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:50:24.300","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:50:32.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:50:35.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:50:41.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:50:45.800","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:50:50.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:50:56.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:50:56.600","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:51:07.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:51:07.300","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:51:09.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:51:17.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:51:19.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:51:28.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:51:30","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:51:40.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:51:40.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:51:51.700","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:51:51.500","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:52:01","Anchor","System Data (dBar %full Volts mAmps): ",44.619999,67.363602,32.274999999999999,5,289.37522799999999,32418.310870000001,null,32.274999999999999,166.5,654.40023599999995,3241.7639319999998,null,null,null,null,null,null,null,null,null,1249.290039,12.19,38.652999999999999,12.19]
["$","2022-02-24","01:52:02.300","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:52:10.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:52:13","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:52:20.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:52:23.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:52:30.600","Anchor","Checking Global Issues."]
["$","2022-02-24","01:52:34.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:52:39.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:52:44.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:52:48.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:52:55.800","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:52:58.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:53:06.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:53:09","Anchor","Checking Global Issues."]
["$","2022-02-24","01:53:17.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:53:18.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:53:29.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:53:29.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:53:40.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","01:53:40","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","01:53:49.600","Anchor","System Data (dBar %full Volts mAmps): ",44.619999,67.350908000000004,32.274999999999999,5,290.19237600000002,33308.794670000003,null,32.274999999999999,166.5,672.42641000000003,3330.7988799999998,null,null,null,null,null,null,null,null,null,1249.290039,12.19,38.453999000000003,12.19]
["$","2022-02-24","01:53:50.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:53:59.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:01.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:54:09.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:12.200","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:54:19.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:22.100","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:27","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:28","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:33.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:54:37.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:44.300","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","01:54:47.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:54:55","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:54:56.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:55:05.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:55:07.100","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:55:17.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:55:17.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:55:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:55:28.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:55:38.100","Anchor","System Data (dBar %full Volts mAmps): ",44.619999,67.356902000000005,32.274999999999999,5,290.974109,34198.606899999999,null,32.274999999999999,167.5,690.43723799999998,3419.7801030000001,null,null,null,null,null,null,null,null,null,1249.209961,12.17,37.945,12.17]
["$","2022-02-24","01:55:39.200","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:55:49","Anchor","Checking Global Issues."]
["$","2022-02-24","01:55:50.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:55:57.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:56:01.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","01:56:06.700","Anchor","Checking Global Issues."]
["$","2022-02-24","01:56:11.400","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:56:16.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:56:22","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:56:26.400","Anchor","Checking Global Issues."]
["$","2022-02-24","01:56:33.100","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:56:34.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:56:43.500","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:56:44.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","01:56:54.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:56:55.600","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:57:06.400","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:57:05.600","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:57:15.900","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:57:17.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:57:26.600","Anchor","System Data (dBar %full Volts mAmps): ",44.619999,67.352304000000004,32.274999999999999,10,291.77420599999999,35088.687760000001,null,32.274999999999999,166,708.54289700000004,3508.8016200000002,null,null,null,null,null,null,null,null,null,1249.290039,12.17,38.165999999999997,12.17]
["$","2022-02-24","01:57:27.700","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","01:57:37.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:57:39","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:57:45.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:57:46.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:57:49.200","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","01:57:56.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:57:59.900","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:58:02.400","Anchor","Sci Logger sending PTS to CTD"]
["$","2022-02-24","01:58:08","Anchor","FLBB post: /99/99,99:99:99,695,77,700,1351,546  "]
["$","2022-02-24","01:58:08.200","Anchor","[MSC] Starting ISUS Sample"]
["$","2022-02-24","01:58:09.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:58:11.300","Anchor","[MSC] RX: "]
["$","2022-02-24","01:58:20.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","01:58:21.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:58:24","Anchor","Checking Global Issues."]
["$","2022-02-24","01:58:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","01:58:32.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","01:58:41.900","Anchor","Checking Global Issues."]
["$","2022-02-24","01:58:43","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","01:58:51.800","Anchor","Checking Global Issues."]
["$","2022-02-24","01:58:53.700","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","01:59:05.100","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","01:59:04.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","01:59:09.500","Anchor","Checking Global Issues."]
["$","2022-02-24","01:59:15.200","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","01:59:19.300","Anchor","Checking Global Issues."]
["$","2022-02-24","01:59:25.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:59:29.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:59:35.200","Anchor","Checking Global Issues."]
["$","2022-02-24","01:59:38","Anchor","Checking Global Issues."]
["$","2022-02-24","01:59:47.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","01:59:48.600","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","01:59:58","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","01:59:59.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:00:10.200","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:00:09.400","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:00:19.600","Anchor","System Data (dBar %full Volts mAmps): ",44.759998000000003,67.349097,32.274999999999999,10,293.08846299999999,36507.149189999996,null,32.274999999999999,167,738.26634999999999,3650.6343320000001,null,null,null,null,null,null,null,null,null,1249.1800539999999,12.16,39.987999000000002,12.16]
["$","2022-02-24","02:00:20.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:00:30.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:00:31.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:00:40.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:00:41.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:00:42.200","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:00:49.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:00:52.900","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:00:59","Anchor","Checking Global Issues."]
["$","2022-02-24","02:01:03.700","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:01:08.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:01:15.200","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:01:16.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:01:25","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:01:26.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:01:35.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:01:37.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:01:47.100","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:01:47.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:01:58.800","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:01:58.600","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:02:08.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:02:09.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:02:19","Anchor","System Data (dBar %full Volts mAmps): ",44.759998000000003,67.363221999999993,32.274999999999999,5,293.98168500000003,37486.278429999998,null,32.274999999999999,167,758.17432499999995,3748.5472559999998,null,null,null,null,null,null,null,null,null,1249.130005,12.17,38.441001999999997,12.17]
["$","2022-02-24","02:02:19.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:02:27.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:02:30.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:02:37.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:02:41.400","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:02:47.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:02:52.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:02:53.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:03:02.900","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:03:05.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:03:13.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:03:15.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:03:24.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:03:25.200","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:03:36.500","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:03:36.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:03:47.300","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:03:47.100","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:03:56.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:03:58","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:04:04.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:04:07.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:04:08.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:04:17.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:04:19.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:04:26.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:04:30.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:04:40.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:04:40.700","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:04:44.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:04:51.400","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:04:54.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:05:02","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:05:03.300","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:05:12.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:05:14.100","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:05:23.600","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:05:25","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:05:35.800","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:05:35.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:05:43.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:05:46.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:05:56","Anchor","Checking Global Issues."]
["$","2022-02-24","02:05:57.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:06:05.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:06:07.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:06:08.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:06:18.400","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:06:23.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:06:29.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:06:33.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:06:39.900","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:06:43.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:06:51.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:06:52.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:07:01.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:07:02.700","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:07:12.100","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:07:13.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:07:24.300","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:07:24.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:07:24.100","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:07:33.800","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:07:35","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:07:44.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:07:45.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:07:55.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:07:56.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:08:01.400","Anchor","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","02:08:04.600","Anchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","02:08:06.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:08:07","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:08:11.100","Anchor","[MSC] TX: W"]
["$","2022-02-24","02:08:17.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:08:17.900","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:08:22.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:08:28.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:08:28.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:08:39.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:08:39.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:08:47.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:08:50.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:08:58.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:00.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:09:08.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:11.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:09:17.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:22.200","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:09:27.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:32.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:09:36.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:43.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:09:46.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:09:54.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:09:55.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:10:05","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:10:06.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:10:17.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:10:17.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:10:17.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:10:26.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:10:27.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:10:37.500","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.350326999999993,32.25,10,297.40504900000002,41574.310879999997,null,32.274999999999999,167,842.03296399999999,4157.3505009999999,null,null,null,null,null,null,null,null,null,1248.959961,12.15,38.694000000000003,12.15]
["$","2022-02-24","02:10:38.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:10:48.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:10:49.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:10:56.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:11:00.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:11:06","Anchor","Checking Global Issues."]
["$","2022-02-24","02:11:10.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:11:15.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:11:21.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:11:25.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:11:32.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:11:33.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:11:42.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:11:44.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:11:53.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:11:54.900","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:12:05.800","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:12:05.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:12:15.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:12:16.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:12:26","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.360930999999994,32.25,10,298.16842000000003,42464.12311,null,32.274999999999999,165,860.13586799999996,4246.3182930000003,null,null,null,null,null,null,null,null,null,1248.98999,12.15,38.782001000000001,12.15]
["$","2022-02-24","02:12:27.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:12:36.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:12:37.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:12:44.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:12:48.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:12:54.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:12:59.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:13:04.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:13:09.900","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:13:13.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:13:20.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:13:22.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:13:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:13:32.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:13:32.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:13:42.200","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:13:43.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:13:54.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:13:54.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:14:05.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:14:04.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:14:14.500","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.347303999999994,32.25,10,298.899,43353.935340000004,null,32.25,167,878.15391,4335.299516,null,null,null,null,null,null,null,null,null,1248.98999,12.15,38.847999999999999,12.15]
["$","2022-02-24","02:14:16","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:14:24.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:14:26.200","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:14:34.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:14:37.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:14:44","Anchor","Checking Global Issues."]
["$","2022-02-24","02:14:47.900","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:14:51.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:14:58.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:15:01.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:15:09","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:15:11.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:15:19.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:15:25.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:15:30.500","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:15:31.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:15:42.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:15:42.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:15:53.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:15:53.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:16:04.500","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:16:04.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:16:12.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:16:14.700","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:16:22.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:16:25.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:16:26.200","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:16:36.200","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:16:40.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:16:46.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:16:50.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:16:51.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:16:57.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:17:04.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:17:08.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:17:09.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:17:19","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:17:20.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:17:31.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:17:33.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:17:40.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:17:42","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:17:51.500","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.361530000000002,32.25,10,300.32343400000002,45133.828439999997,null,32.25,166.5,914.28403800000001,4513.288826,null,null,null,null,null,null,null,null,null,1248.910034,12.14,38.758999000000003,12.14]
["$","2022-02-24","02:17:52.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:18:01.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:18:04","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:18:03.400","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:18:06.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:18:09.900","Anchor","[MSC] Timeout for CommandWake"]
["$","2022-02-24","02:18:13","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:18:14.600","Anchor","[MSC] RX: ACK  "]
["$","2022-02-24","02:18:21.300","Anchor","[MSC] TX: T2,1645669086,10.5828,33.6989,44.7000"]
["$","2022-02-24","02:18:24.300","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:18:24.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:18:35.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:18:35.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:18:46.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:18:46.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:18:56","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:18:56.200","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:19:06.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:19:07.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:19:15.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:19:18.500","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:19:25.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:19:29.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:19:30","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:19:39.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:19:44.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:19:50.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:19:53","Anchor","Checking Global Issues."]
["$","2022-02-24","02:19:54","Anchor","Checking Global Issues."]
["$","2022-02-24","02:20:01.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:20:11.900","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.355819999999994,32.25,10,301.38323400000002,46285.279040000001,null,32.25,166.5,938.64120500000001,4628.4338859999998,null,null,null,null,null,null,null,null,null,1248.910034,12.15,37.941001999999997,12.15]
["$","2022-02-24","02:20:12","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:20:13.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:20:22.800","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:20:24.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:20:35.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:20:38.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:20:44.400","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.353274999999996,32.25,5,301.61539299999998,46552.155559999999,null,32.25,166.5,944.04789000000005,4655.1349689999997,null,null,null,null,null,null,null,null,null,1248.910034,12.13,37.752997999999998,12.13]
["$","2022-02-24","02:20:45.800","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:20:55.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:20:56.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:21:05.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:21:07.100","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:21:10","Anchor","Checking Global Issues."]
["$","2022-02-24","02:21:17.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:21:22.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:21:28.500","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:21:32.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:21:39.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:21:40","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:21:49.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:21:51.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:22:00.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:22:01.900","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:22:11.300","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:22:12.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:22:17.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:22:23.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:22:33","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.353628999999998,32.25,5,302.33154500000001,47442.102099999996,null,32.25,168,962.16023800000005,4744.1161929999998,null,null,null,null,null,null,null,null,null,1248.8599850000001,12.14,38.394001000000003,12.14]
["$","2022-02-24","02:22:34.300","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:22:43.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:22:44.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:22:53.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:22:55","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:23:02.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:23:06.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:23:11.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:23:12.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:23:17.100","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:23:27.200","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.344561999999996,32.25,10,302.70273700000001,47886.941070000001,null,32.25,165.5,971.17116099999998,4788.6000889999996,null,null,null,null,null,null,null,null,null,1248.910034,12.14,38.097000000000001,12.14]
["$","2022-02-24","02:23:27.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:23:30","Anchor","Checking Global Issues."]
["$","2022-02-24","02:23:38.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:23:39.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:23:49","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:23:50.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:24:00.700","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:24:01.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:24:12.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:24:11.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:24:21.600","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:24:22.800","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:24:32.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:24:33.200","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:24:41.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:24:44.100","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:24:51","Anchor","Checking Global Issues."]
["$","2022-02-24","02:24:54.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:25:00.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:25:05","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:25:08.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:25:16.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:25:18.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:25:26.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:25:28.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:25:37.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:25:39","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:25:49.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:25:49.800","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:26:00.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:26:00.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:26:10.100","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:26:10.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:26:19.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:21.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:26:29.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:30.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:32.600","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:26:39.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:46.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:48.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:26:53.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:26:58.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:27:04.800","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:27:08.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:27:15.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:27:16.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:27:26.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:27:27.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:27:36.900","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:27:38.300","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:27:49.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:27:49","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:27:58.500","Anchor","System Data (dBar %full Volts mAmps): ",44.700001,67.355626999999998,32.225000000000001,10,304.58362,50112.076050000003,null,32.25,166.5,1016.3320179999999,5011.1135869999998,null,null,null,null,null,null,null,null,null,1248.7700199999999,12.13,38.658000999999999,12.13]
["$","2022-02-24","02:27:59.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:28:02.400","Anchor","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","02:28:06.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:28:09.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:28:10.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:28:12.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:28:20.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:28:21.600","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:28:28.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:28:31.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:28:32.800","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:28:42.200","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:28:43.600","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:28:53","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:28:54.300","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:29:03.800","Anchor","System Data (dBar %full Volts mAmps): ",44.5,67.360138000000006,32.225000000000001,5,305.10433799999998,50647.440820000003,null,32.25,164.5,1028.2211890000001,5064.6366330000001,null,null,null,null,null,null,null,null,null,1248.75,12.13,38.382998999999998,12.13]
["$","2022-02-24","02:29:05.100","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:29:14.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:15.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:29:23.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:26.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:29:32.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:33.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:37.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:29:43.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:48","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:29:51.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:29:58.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:30:01","Anchor","Checking Global Issues."]
["$","2022-02-24","02:30:09.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:30:10.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:30:21.400","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:30:21.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:30:32.200","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:30:32.200","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:30:43","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:30:42.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:30:52.500","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:30:53.700","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:31:02.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:04.300","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:31:12.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:15","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:31:21.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:25.600","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:31:33.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:36.300","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:31:39.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:47.100","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:31:49.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:31:57.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:31:59.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:32:08.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:32:09.900","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:32:20.700","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:32:20.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:32:31.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:32:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:32:31.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:32:42","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:32:50.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:32:51.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:32:52.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:33:01.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:33:03.500","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:33:12.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:33:14.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:33:19.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:33:24.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:33:29.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:33:35.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:33:42","Anchor","Checking Global Issues."]
["$","2022-02-24","02:33:46.300","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:33:47.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:33:57","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:33:58.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:34:09.200","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:34:09.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:34:18.700","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:34:19.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:34:29.400","Anchor","System Data (dBar %full Volts mAmps): ",44.5,67.366268000000005,32.225000000000001,5,307.59119600000002,53317.952010000001,null,32.225000000000001,166,1082.4155290000001,5331.6877519999998,null,null,null,null,null,null,null,null,null,1248.75,12.14,38.591999000000001,12.14]
["$","2022-02-24","02:34:30.500","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:34:40.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:34:41.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:34:51.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:34:52","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:34:58","Anchor","Checking Global Issues."]
["$","2022-02-24","02:35:02.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:35:07.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:35:13.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:35:17.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:35:24.500","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:35:26.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:35:34.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:35:36.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:35:45.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:35:47","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:35:56.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:35:56.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:36:07.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:36:08.700","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:36:08.500","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:36:18","Anchor","System Data (dBar %full Volts mAmps): ",44.5,67.355423999999999,32.225000000000001,5,308.37161800000001,54208.435799999999,null,32.225000000000001,187,1100.4852490000001,5420.7361309999997,null,null,null,null,null,null,null,null,null,1248.6899410000001,12.13,38.790999999999997,12.13]
["$","2022-02-24","02:36:19.300","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:36:30.400","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:36:30","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:36:37.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:36:40.700","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:36:47.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:36:51.300","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:36:56.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:37:02.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:37:05.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:37:12.800","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:37:15.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:37:23.500","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:37:25","Anchor","Checking Global Issues."]
["$","2022-02-24","02:37:34.500","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:37:35.600","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:37:46.400","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:37:46.400","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:37:57.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:37:57","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:38:02.400","Anchor","Sending Optode Do Sample"]
["$","2022-02-24","02:38:03.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:38:08.400","Anchor","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","02:38:07.800","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:38:13.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:38:17.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:38:19.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:38:26.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:38:27.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:38:29.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:38:38.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:38:40","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:38:49.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:38:50.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:38:55.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:39:01.500","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:39:01.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:39:11.100","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:39:12.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:39:21.900","Anchor","System Data (dBar %full Volts mAmps): ",44.630001,67.353106999999994,32.225000000000001,5,309.71866499999999,55716.482859999996,null,32.225000000000001,168,1132.1298529999999,5571.5408369999996,null,null,null,null,null,null,null,null,null,1248.6400149999999,12.13,38.459000000000003,12.13]
["$","2022-02-24","02:39:23","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:39:34.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:39:33.700","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:39:40.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:39:44.500","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:39:50.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:39:55.200","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:40:00.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:40:06.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:40:09.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:40:16.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:40:18","Anchor","Checking Global Issues."]
["$","2022-02-24","02:40:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:40:28.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:40:38.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:40:39.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:40:50.200","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:40:50.200","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:40:59.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:41:00.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:41:10.400","Anchor","System Data (dBar %full Volts mAmps): ",44.630001,67.355540000000005,32.225000000000001,5,310.50958000000003,56606.429409999997,null,32.225000000000001,165,1150.1642899999999,5660.5220600000002,null,null,null,null,null,null,null,null,null,1248.6899410000001,12.13,38.216999000000001,12.13]
["$","2022-02-24","02:41:10.900","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:41:19.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:41:22.200","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:41:29.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:41:33","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:41:39","Anchor","Checking Global Issues."]
["$","2022-02-24","02:41:43.100","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:41:47.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:41:54.300","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:41:57.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:42:05","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:42:06.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:42:15.800","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:42:16.600","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:42:27.900","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:42:26.500","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:42:27.900","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:42:38.700","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:42:38.700","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:42:48.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:42:54.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:42:58.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:00","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:43:08.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:10.700","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:43:18.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:22.200","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:43:26.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:32.200","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:43:36.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:42.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:43:46.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:43:53.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:43:54.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:44:04.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:44:05.600","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:44:15","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:44:16.400","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:44:27.200","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:44:27.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:44:33.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:44:37.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:44:47.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:44:48.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:44:57.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:44:59.300","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:45:03.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:45:09.900","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:45:15.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:45:20.800","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:45:24.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:45:31.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:45:34.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:45:43.300","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:45:42.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:45:43.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:45:52.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:45:54.200","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:46:03.600","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:46:14.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:46:15.800","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:46:15.600","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:46:25.300","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:46:26.500","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:46:36","Anchor","System Data (dBar %full Volts mAmps): ",44.630001,67.356645,32.200000000000003,5,312.67508700000002,59276.940600000002,null,32.225000000000001,167,1204.463166,5927.5731800000003,null,null,null,null,null,null,null,null,null,1248.6099850000001,12.12,38.581001000000001,12.12]
["$","2022-02-24","02:46:37.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:46:41.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:46:47.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:46:54.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:46:58.400","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:47:04.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:47:09.300","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:47:14.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:47:19.700","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:47:22.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:47:30.600","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:47:32.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:47:41.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:47:42.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:47:52","Anchor","System Data (dBar %full Volts mAmps): ",44.630001,67.345500999999999,32.200000000000003,5,313.15645699999999,59899.742010000002,null,32.200000000000003,166.5,1217.0882959999999,5989.8533200000002,null,null,null,null,null,null,null,null,null,1248.6099850000001,12.12,38.847000000000001,12.12]
["$","2022-02-24","02:47:53.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:48:02.400","Anchor","Sending CTD PTS"]
["$","2022-02-24","02:48:03","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:48:03.800","Anchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","02:48:06.800","Anchor","Setting MSC time and CTD Values: 1645670886,33.70,10.578,44.71"]
["$","2022-02-24","02:48:12.900","Anchor","[MSC] Timeout for CommandWake"]
["$","2022-02-24","02:48:13.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:48:16.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:48:23.800","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.357984000000002,32.200000000000003,10,313.38599299999998,60160.70882,null,32.200000000000003,181.5,1223.211264,6015.9500019999996,null,null,null,null,null,null,null,null,null,1248.6400149999999,12.12,38.459000000000003,12.12]
["$","2022-02-24","02:48:24.900","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:48:27.700","Anchor","[MSC] Done Sampling."]
["$","2022-02-24","02:48:35.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:48:37.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:48:39.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:48:45.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:48:47.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:48:56.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:48:57.900","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:49:07.400","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:49:08.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:49:18.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:49:19.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:49:29","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.344905999999995,32.200000000000003,5,313.77554800000001,60694.999100000001,null,32.200000000000003,165.5,1234.2365930000001,6069.3924610000004,null,null,null,null,null,null,null,null,null,1248.6400149999999,12.13,38.205002,12.13]
["$","2022-02-24","02:49:30.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:49:39.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:49:40.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:49:50.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:49:51.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:49:57.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:50:02.200","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:50:07.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:50:13.100","Anchor","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","02:50:16.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:50:23.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:50:26.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:50:34.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:50:35.600","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:50:45","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:50:46.400","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:50:55.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:50:57.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:51:06.700","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:51:07.900","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:51:17.500","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.337872000000004,32.200000000000003,10,314.50481600000001,61584.811329999997,null,32.200000000000003,165.5,1252.365337,6158.3602529999998,null,null,null,null,null,null,null,null,null,1248.5600589999999,12.13,38.039000999999999,12.13]
["$","2022-02-24","02:51:18.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:51:28.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:51:29.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:51:37.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:51:40.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:51:46","Anchor","Checking Global Issues."]
["$","2022-02-24","02:51:50.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:51:55.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:51:58.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:52:01.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:52:04.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:52:12.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:52:14.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:52:22.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:52:24.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:52:33.700","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:52:34.900","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:52:45.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:52:45.800","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:52:56.600","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:52:56.400","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:53:06","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.341504999999998,32.200000000000003,10,315.28786200000002,62474.623570000003,null,32.200000000000003,167,1270.4042340000001,6247.3414769999999,null,null,null,null,null,null,null,null,null,1248.530029,12.12,38.625999,12.12]
["$","2022-02-24","02:53:07.500","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:53:15.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:53:17.900","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:53:25.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:53:28.600","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:53:35.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:53:39.400","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:53:44.400","Anchor","Checking Global Issues."]
["$","2022-02-24","02:53:49.900","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:53:53.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:54:00.700","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:54:03.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:54:11.400","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:54:15.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:54:22","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:54:23.500","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:54:34.300","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:54:34.300","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:54:45.100","Anchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:54:45.100","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:54:54.500","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.356866999999994,32.200000000000003,5,316.01713000000001,63364.570110000001,null,32.200000000000003,165,1288.452706,6336.336131,null,null,null,null,null,null,null,null,null,1248.589966,12.13,37.884998000000003,12.13]
["$","2022-02-24","02:54:55.600","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:55:04.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:06.400","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:55:14.200","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:17.100","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:55:17.500","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:55:23","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:27.700","Anchor","Twitter msg",null,null,null,null,null,null,"67158784;"]
["$","2022-02-24","02:55:32.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:38.400","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:55:42.700","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:49.200","Anchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:55:54.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:55:59.900","Anchor","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","02:56:01.100","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:56:10.500","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:56:12","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:56:22.800","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:56:24.100","Anchor","Checking Global Issues."]
["$","2022-02-24","02:56:32.200","Anchor","Pump motor not faulted"]
["$","2022-02-24","02:56:33.500","Anchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:56:43","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.350992000000005,32.200000000000003,5,316.89198900000002,64254.650970000002,null,32.200000000000003,166.5,1306.5857779999999,6425.3307860000004,null,null,null,null,null,null,null,null,null,1248.4799800000001,12.12,37.905997999999997,12.12]
["$","2022-02-24","02:56:44.100","Anchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:56:53.800","Anchor","Checking Global Issues."]
["$","2022-02-24","02:56:55","Anchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:57:04.800","Anchor","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.350209000000007,32.200000000000003,10,317.06643700000001,64433.016349999998,null,32.200000000000003,166,1310.2030010000001,6443.167324,null,null,null,null,null,null,null,null,null,1248.530029,12.12,37.883999000000003,12.12]
["$","2022-02-24","02:57:05.700","Anchor","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","02:57:11.600","Anchor","Checking Global Issues."]
["$","2022-02-24","02:57:16.100","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:57:19.500","Anchor","Checking Global Issues."]
["$","2022-02-24","02:57:26.800","Anchor","Twitter msg",null,null,null,null,null,null,"0;"]
["$","2022-02-24","02:57:29.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:57:35.300","Anchor","Checking Global Issues."]
["$","2022-02-24","02:57:38.800","Anchor","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","02:57:48.300","Anchor","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","02:57:49.700","Anchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:58:00.500","Anchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:58:00.500","Anchor","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","02:58:00.900","Anchor","Checking Global Issues."]
["$","2022-02-24","02:58:11.200","Anchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:58:17.200","Anchor","Normal State Exit"]
["$","2022-02-24","02:58:17.300","Start CP Mode","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","02:58:20.700","Start CP Mode","System Data (dBar %full Volts mAmps): ",44.709999000000003,67.337405000000004,32.200000000000003,10,317.693398,65055.952069999999,null,32.200000000000003,166.5,1322.8434769999999,6505.4743269999999,null,null,null,null,null,null,null,null,null,1248.5600589999999,12.13,38.470001000000003,12.13]
["$","2022-02-24","02:58:22.200","Start CP Mode","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:58:22.400","Start CP Mode","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","02:58:24","DeAnchor","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","02:58:24","DeAnchor","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","02:58:24.400","DeAnchor","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","02:58:32.500","DeAnchor","getting Elmo deacceleration limit"]
["$","2022-02-24","02:58:32.300","DeAnchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:58:35.400","DeAnchor","SBE41 Message",44.700001,66.815740000000005,32.15,155.5,null,null,null,null,null,null,null,null,"   44.70, 10.5779, 33.6992  ",44.700001,44.660772000000001,2.029E-3,-1.6666E-2,-1.6667000000000001E-2,2.3E-5,3000]
["$","2022-02-24","02:58:42.500","DeAnchor","getting Elmo acceleration limit"]
["$","2022-02-24","02:58:41.700","DeAnchor","Twitter msg",null,null,null,null,null,null,"29410064;"]
["$","2022-02-24","02:58:43.400","DeAnchor","SBE41 Message",44.66,66.373259000000004,32.15,155.5,null,null,null,null,null,null,null,null,"   44.66, 10.5779, 33.6998  ",44.66,44.637791999999997,9.4399999999999996E-4,-0.02,-1.6666E-2,7.1000000000000005E-5,3000]
["$","2022-02-24","02:58:49","DeAnchor","Checking Global Issues."]
["$","2022-02-24","02:58:51.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.60, 10.5785, 33.6996  "]
["$","2022-02-24","02:58:52.500","DeAnchor","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","02:58:57.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.56, 10.5797, 33.6991  "]
["$","2022-02-24","02:59:01.300","DeAnchor","SBE41 Message",44.75,65.107254999999995,32.15,155.5,null,null,null,null,null,null,null,null,"   44.75, 10.5791, 33.6990  ",44.75,44.575597999999999,1.9870000000000001E-3,-0.02,-0.02,1.16E-4,3000]
["$","2022-02-24","02:59:02.100","DeAnchor","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","02:59:05.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.58, 10.5790, 33.6995  "]
["$","2022-02-24","02:59:10.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.64, 10.5789, 33.6993  "]
["$","2022-02-24","02:59:11.700","DeAnchor","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","02:59:13.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.72, 10.5795, 33.6988  "]
["$","2022-02-24","02:59:18.400","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.54, 10.5786, 33.6995  "]
["$","2022-02-24","02:59:21.100","DeAnchor","Pump motor not faulted"]
["$","2022-02-24","02:59:22.300","DeAnchor","SBE41 Message",44.650002000000001,63.740324999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   44.65, 10.5789, 33.6994  ",44.650002000000001,44.584418999999997,-3.28E-4,-1.3334E-2,-1.4999999999999999E-2,-3.1700000000000001E-4,3000]
["$","2022-02-24","02:59:26.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.63, 10.5785, 33.6993  "]
["$","2022-02-24","02:59:31.100","DeAnchor","Pump motor not faulted"]
["$","2022-02-24","02:59:32.100","DeAnchor","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","02:59:35","DeAnchor","Checking Global Issues."]
["$","2022-02-24","02:59:37.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.62, 10.5785, 33.6996  "]
["$","2022-02-24","02:59:41.500","DeAnchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","02:59:43","DeAnchor","Checking Global Issues."]
["$","2022-02-24","02:59:48","DeAnchor","Checking Global Issues."]
["$","2022-02-24","02:59:51.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.63, 10.5786, 33.6995  "]
["$","2022-02-24","02:59:52.300","DeAnchor","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","02:59:56.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.44, 10.5783, 33.6997  "]
["$","2022-02-24","02:59:59.300","DeAnchor","SBE41 Message",44.419998,61.088261000000003,32.15,155.5,null,null,null,null,null,null,null,null,"   44.42, 10.5784, 33.7002  ",44.419998,44.597019000000003,5.6899999999999995E-4,-1.6666E-2,-3.333E-3,6.38E-4,3000]
["$","2022-02-24","03:00:01.900","DeAnchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:00:04.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   44.40, 10.5780, 33.6998  "]
["$","2022-02-24","03:00:09.300","DeAnchor","SBE41 Message",44.119999,60.359456999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   44.12, 10.5819, 33.6985  ",44.119999,44.382106999999998,3.7069999999999998E-3,3.3340000000000002E-3,8.3330000000000001E-3,5.0309999999999999E-3,3000]
["$","2022-02-24","03:00:11.600","DeAnchor","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","03:00:11.600","DeAnchor","Twitter msg",null,null,null,null,null,null,"-3.99919;"]
["$","2022-02-24","03:00:13.100","DeAnchor","Checking Global Issues."]
["$","2022-02-24","03:00:20.300","DeAnchor","SBE41 Message",43.52,59.602936,32.15,155.5,null,null,null,null,null,null,null,null,"   43.52, 10.5884, 33.6979  ",43.52,43.799086000000003,1.6205000000000001E-2,0.02,1.8332999999999999E-2,1.7387E-2,3000]
["$","2022-02-24","03:00:21.200","DeAnchor","Twitter msg",null,null,null,null,null,null,"-146884;"]
["$","2022-02-24","03:00:22.400","DeAnchor","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:00:26.300","DeAnchor","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   42.91, 10.6052, 33.6942  "]
["$","2022-02-24","03:00:31.100","DeAnchor","System Data (dBar %full Volts mAmps): ",42.619999,58.806688000000001,32.049999999999997,725,419.75029599999999,66124.935549999995,null,32.049999999999997,184.5,1346.7877410000001,6612.3726749999996,null,null,null,null,null,null,null,null,null,1235.589966,12.12,38.282001000000001,12.12]
["$","2022-02-24","03:00:32","DeAnchor","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:00:35.400","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:35.400","Ascend","Twitter msg",null,null,null,null,null,null,"ST;"]
["$","2022-02-24","03:00:35.800","Ascend","[MSC] Resetting Sequencers"]
["$","2022-02-24","03:00:37.300","Ascend","SBE41 Message",41.720001000000003,58.38823,32.15,155.5,null,null,null,null,null,null,null,null,"   41.72, 10.6506, 33.6831  ",41.720001000000003,42.376551999999997,3.0995999999999999E-2,3.6666999999999998E-2,4.1667000000000003E-2,5.5944000000000001E-2,3000]
["$","2022-02-24","03:00:38.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:40.300","Ascend","BE::sendJV: -83284"]
["$","2022-02-24","03:00:41.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:42.800","Ascend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:00:43.200","Ascend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:00:44","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:45.300","Ascend","BE::sendJV: -69682"]
["$","2022-02-24","03:00:46.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-65948;"]
["$","2022-02-24","03:00:47.800","Ascend","Checking Global Issues."]
["$","2022-02-24","03:00:48.800","Ascend","Checking Global Issues."]
["$","2022-02-24","03:00:50.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:51.600","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:00:54.400","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:00:54.800","Ascend","FLBB Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"/99/99,99:99:99,695,91,700,771,546  "]
["$","2022-02-24","03:00:53.900","Ascend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","03:00:54.500","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:00:55.200","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   39.44, 10.6708, 33.6850  "]
["$","2022-02-24","03:00:56.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:00:57.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:00:58.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:00.200","Ascend","SBE41 Message",38.75,57.617007999999998,32.15,155.5,null,null,null,null,null,null,null,null,"   38.75, 10.6958, 33.6779  ",38.75,39.432664000000003,4.2882999999999998E-2,3.3333000000000002E-2,3.8332999999999999E-2,0.11249199999999999,3000]
["$","2022-02-24","03:01:01.200","Ascend","SBE41 Message",38.630001,57.598629000000003,32.15,155.5,null,null,null,null,null,null,null,null,"   38.63, 10.7009, 33.6739  ",38.630001,39.271684,4.3625999999999998E-2,0.04,3.6665999999999997E-2,0.114582,3000]
["$","2022-02-24","03:01:02.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:01:03.300","Ascend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:01:04.800","Ascend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","03:01:05.200","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   37.97, 10.7079, 33.6716  "]
["$","2022-02-24","03:01:06.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:01:07.400","Ascend","Vel PID Values",37.689999,57.352257999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,4.3333999999999998E-2,4.7995999999999997E-2,4.7399999999999997E-4,5.6429999999999996E-3,7.7865869999999999,7.7865869999999999,63787,1]
["$","2022-02-24","03:01:07.200","Ascend","SBE41 Message",37.689999,57.352257999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   37.69, 10.7089, 33.6716  ",37.689999,38.475914000000003,4.6066000000000003E-2,4.3333999999999998E-2,4.6667E-2,0.124191,3000]
["$","2022-02-24","03:01:09.200","Ascend","SBE41 Message",37.409999999999997,57.305956000000002,32.15,155.5,null,null,null,null,null,null,null,null,"   37.41, 10.7097, 33.6718  ",37.409999999999997,38.152149000000001,4.6156000000000003E-2,5.0000999999999997E-2,4.6665999999999999E-2,0.12694800000000001,3000]
["$","2022-02-24","03:01:09.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:11.400","Ascend","Vel PID Values",37.090000000000003,57.241768,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.3333E-2,4.9097000000000002E-2,3.59E-4,6.2919999999999998E-3,7.7910750000000002,7.7910750000000002,63824,1]
["$","2022-02-24","03:01:12.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-63556;"]
["$","2022-02-24","03:01:13.800","Ascend","[MSC] Data: 0x41E6,pH,02/24/2022 03:01:20,1645671654,39.88,10.6689,33.6802,58,6,0,12.76,38.14,11.672,4.620e-02,7.1234,3.549,-0.964876,0.000015,-0.919728,0.000011,+1.790e-09,+8.138e-11  "]
["$","2022-02-24","03:01:14.200","Ascend","SBE41 Message",36.529998999999997,57.112580000000001,32.15,155.5,null,null,null,null,null,null,null,null,"   36.53, 10.7258, 33.6689  ",36.529998999999997,37.407798999999997,4.9806999999999997E-2,6.3334000000000001E-2,6.6667000000000004E-2,0.133631,3000]
["$","2022-02-24","03:01:15.400","Ascend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","03:01:16.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:17.300","Ascend","BE::sendJV: -62890"]
["$","2022-02-24","03:01:18.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-64860;"]
["$","2022-02-24","03:01:19.900","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:21.300","Ascend","SBE41 Message",35.529998999999997,56.894159999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   35.53, 10.7337, 33.6662  ",35.529998999999997,36.230051000000003,5.4488000000000002E-2,6.6667000000000004E-2,5.6667000000000002E-2,0.142183,3000]
["$","2022-02-24","03:01:22.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:01:23.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:24.600","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:01:26.600","Ascend","Setting MSC time and CTD Values: 1645671686,33.67,10.745,34.72"]
["$","2022-02-24","03:01:25.500","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,160.294,10.661,40.234,39.542,48.467,8.925,930.6,669.2,439.4  "]
["$","2022-02-24","03:01:26.400","Ascend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","03:01:27.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:28.200","Ascend","SBE41 Message",34.259998000000003,56.641359999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   34.26, 10.7949, 33.6588  ",34.259998000000003,35.105649999999997,5.2393000000000002E-2,5.3332999999999998E-2,4.8333000000000001E-2,0.148262,3000]
["$","2022-02-24","03:01:29.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:01:31","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:32.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:01:33.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:01:34.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:35.200","Ascend","SBE41 Message",33.040000999999997,56.441867000000002,32.15,155.5,null,null,null,null,null,null,null,null,"   33.04, 10.9028, 33.6287  ",33.040000999999997,33.951425999999998,5.6085999999999997E-2,6.6667000000000004E-2,6.6666000000000003E-2,0.15606300000000001,3000]
["$","2022-02-24","03:01:36.300","Ascend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:01:37.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:38.200","Ascend","BE::sendJV: -57373"]
["$","2022-02-24","03:01:39.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:40.900","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:41.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:43.200","Ascend","BE::sendJV: -60802"]
["$","2022-02-24","03:01:44.200","Ascend","SBE41 Message",31.5,56.162190000000002,32.15,155.5,null,null,null,null,null,null,null,null,"   31.50, 11.0821, 33.5896  ",31.5,32.317307,6.0595000000000003E-2,5.6667000000000002E-2,5.5E-2,0.164961,3000]
["$","2022-02-24","03:01:45.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:46.600","Ascend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","03:01:47.400","Ascend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","03:01:48.500","Ascend","Vel PID Values",30.700001,56.033450999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.3333E-2,5.8867000000000003E-2,4.0400000000000001E-4,1.1924000000000001E-2,6.9791679999999996,6.9791679999999996,57173,1]
["$","2022-02-24","03:01:48.200","Ascend","SBE41 Message",30.700001,56.033450999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   30.70, 11.1350, 33.5754  ",30.700001,31.662185000000001,5.7044999999999998E-2,6.3333E-2,7.0000000000000007E-2,0.16770299999999999,3000]
["$","2022-02-24","03:01:49.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:01:51.200","Ascend","BE::sendJV: -55807"]
["$","2022-02-24","03:01:52.200","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:01:53.700","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:54.700","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   29.69, 11.1676, 33.5729  "]
["$","2022-02-24","03:01:55.500","Ascend","[MSC] RX: ACK  "]
["$","2022-02-24","03:01:55.700","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:01:56.400","Ascend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","03:01:57.500","Ascend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","03:01:58.200","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   28.90, 11.1933, 33.5604  "]
["$","2022-02-24","03:01:59.200","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:02:00.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:02.300","Ascend","Vel PID Values",28.129999000000002,55.700105000000001,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,5.3333999999999999E-2,6.1305999999999999E-2,2.0699999999999999E-4,1.3936E-2,6.9439339999999996,6.9439339999999996,56884,1]
["$","2022-02-24","03:02:03.200","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-58355;"]
["$","2022-02-24","03:02:04.200","Ascend","SBE41 Message",27.82,55.639701000000002,32.15,155.5,null,null,null,null,null,null,null,null,"   27.82, 11.2655, 33.5554  ",27.82,28.691898999999999,5.9587000000000001E-2,5.3332999999999998E-2,5.1666999999999998E-2,0.177012,3000]
["$","2022-02-24","03:02:05.200","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-58542;"]
["$","2022-02-24","03:02:06.800","Ascend","Checking Global Issues."]
["$","2022-02-24","03:02:07.500","Ascend","Twitter msg",null,null,null,null,null,null,"46187280;"]
["$","2022-02-24","03:02:08.500","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:02:09.200","Ascend","SBE41 Message",26.790001,55.490949000000001,32.15,155.5,null,null,null,null,null,null,null,null,"   26.79, 11.3601, 33.5313  ",26.790001,27.799472000000002,6.2579999999999997E-2,7.0000000000000007E-2,7.1665999999999994E-2,0.17939099999999999,3000]
["$","2022-02-24","03:02:10.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:11.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:12.700","Ascend","Checking Global Issues."]
["$","2022-02-24","03:02:14.200","Ascend","SBE41 Message",25.959999,55.339058999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   25.96, 11.4226, 33.5118  ",25.959999,26.811354000000001,6.1683000000000002E-2,6.3334000000000001E-2,5.6667000000000002E-2,0.18230199999999999,3000]
["$","2022-02-24","03:02:15.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:17.200","Ascend","BE::sendJV: -57091"]
["$","2022-02-24","03:02:17.800","Ascend","Twitter msg",null,null,null,null,null,null,"-55573;"]
["$","2022-02-24","03:02:18.600","Ascend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:02:19.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:20.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:22.500","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:02:22.400","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,171.175,11.109,39.180,38.488,47.415,8.927,900.7,667.6,425.0  "]
["$","2022-02-24","03:02:22.900","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:24.200","Ascend","BE::sendJV: -57094"]
["$","2022-02-24","03:02:25.200","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:02:26.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:29.200","Ascend","getting Elmo acceleration limit"]
["$","2022-02-24","03:02:28.600","Ascend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:02:28.800","Ascend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","03:02:29.400","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:30.100","Ascend","SBE41 Message",22.92,54.860487999999997,32.15,155.5,null,null,null,null,null,null,null,null,"   22.92, 11.4698, 33.5083  ",22.92,23.843316999999999,6.1962000000000003E-2,6.6667000000000004E-2,6.1667E-2,0.18675600000000001,3000]
["$","2022-02-24","03:02:31.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:32.200","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-58779;"]
["$","2022-02-24","03:02:34.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   22.17, 11.4723, 33.5072  "]
["$","2022-02-24","03:02:35.200","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:02:36.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:37.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:38.700","Ascend","System Data (dBar %full Volts mAmps): ",21.360001,54.598908000000002,32.1,245,459.44032900000002,67171.623359999998,null,32.125,195,1373.9373760000001,6717.0280249999996,null,null,null,null,null,null,null,null,null,1230.420044,12.12,37.994999,12.12]
["$","2022-02-24","03:02:39.400","Ascend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","03:02:40.400","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:02:41.100","Ascend","SBE41 Message",20.77,54.538406999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   20.77, 11.4730, 33.5086  ",20.77,21.780604,6.2459000000000001E-2,6.6666000000000003E-2,6.5000000000000002E-2,0.18701100000000001,3000]
["$","2022-02-24","03:02:42.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:44.200","Ascend","BE::sendJV: -55787"]
["$","2022-02-24","03:02:45.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:46.500","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:02:48.500","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:02:49.100","Ascend","Optode post: 4330,2707,194.736,11.398,37.415,36.723,45.653,8.930,849.5,665.7,415.8  "]
["$","2022-02-24","03:02:48.900","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:02:51.200","Ascend","getting Elmo acceleration limit"]
["$","2022-02-24","03:02:50.600","Ascend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:02:51.400","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-55456;"]
["$","2022-02-24","03:02:52.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-54753;"]
["$","2022-02-24","03:02:53.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:55.300","Ascend","Vel PID Values",18.059999000000001,54.139116000000001,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,0.06,6.5106999999999998E-2,2.3E-5,2.1332E-2,6.7940500000000004,6.7940500000000004,55656,1]
["$","2022-02-24","03:02:56.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:02:57.500","Ascend","[MSC] Data: 0x8ADF,A,02/24/2022 03:03:02,1645671768,19.64,11.4907,33.5051,62,6,0,0,12.93,37.94,11.500,5.650e-01,17481.00,899.00,1017.16,4.77,33.51,19.89,7.231e-04,36,77,2AA82F663318359D37063798378237163681360335B635B2360D36C6380539C43BE13E9141BA454949344D6F51DB56355A795E2C6154639764CD64E063D161A05EB55AF856F552D64EBB4AD547534424414C3EEC,1112.4  "]
["$","2022-02-24","03:02:58.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:00.100","Ascend","SBE41 Message",17.09,54.029670000000003,32.15,155.5,null,null,null,null,null,null,null,null,"   17.09, 11.4985, 33.5074  ",17.09,18.05396,6.5172999999999995E-2,7.0000000000000007E-2,6.3333E-2,0.19245999999999999,3000]
["$","2022-02-24","03:03:00.700","Ascend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:03:01.900","Ascend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:03:02.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:03.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:04.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:06.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   15.88, 11.5034, 33.5056  "]
["$","2022-02-24","03:03:06.300","Ascend","Vel PID Values",15.88,53.842283999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,6.5766000000000005E-2,5.3999999999999998E-5,2.2821999999999999E-2,6.7181059999999997,6.7181059999999997,55034,1]
["$","2022-02-24","03:03:08.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:10.100","Ascend","BE::sendJV: -55793"]
["$","2022-02-24","03:03:10.200","Ascend","Vel PID Values",15.11,53.760922000000001,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.3334000000000001E-2,6.5676999999999999E-2,-5.1999999999999997E-5,2.3361E-2,6.810746,6.810746,55793,1]
["$","2022-02-24","03:03:11.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-55644;"]
["$","2022-02-24","03:03:13","Ascend","getting Elmo acceleration limit"]
["$","2022-02-24","03:03:13.300"]
["$","2022-02-24","03:03:12.400","Ascend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","03:03:13.400","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:14.400","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:15.200","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:17.100","Ascend","BE::sendJV: -55403"]
["$","2022-02-24","03:03:18.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:20.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   13.12, 11.5312, 33.5006  "]
["$","2022-02-24","03:03:21","Ascend","[MSC] Post NO3: 18.80"]
["$","2022-02-24","03:03:21.400","Ascend","[MSC] TX: T2,1645671793,11.5346,33.5002,14.7100"]
["$","2022-02-24","03:03:22.400","Ascend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","03:03:23.200","Ascend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","03:03:24.300","Ascend","Vel PID Values",12.34,53.331170999999998,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.3333E-2,6.5616999999999995E-2,4.3000000000000002E-5,2.5250999999999999E-2,6.7409410000000003,6.7409410000000003,55221,1]
["$","2022-02-24","03:03:25.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:27.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:27.700","Ascend","Wrote to msg file: AscendPt:,2022-Feb-24T03:03:11Z,14.71,11.5346,33.500,11.477,35.143,8.933,-0.953072,18.80,347,551,546,0.0268,0.0239,0.0084,0.2246  "]
["$","2022-02-24","03:03:29.200","Ascend","Vel PID Values",11.28,53.180154999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,6.6792000000000004E-2,2.4600000000000002E-4,2.5919999999999999E-2,6.4853579999999997,6.4853579999999997,53128,1]
["$","2022-02-24","03:03:30.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-52514;"]
["$","2022-02-24","03:03:32.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   10.66, 11.5616, 33.4983  "]
["$","2022-02-24","03:03:32.600","Ascend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:03:33.800","Ascend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","03:03:34.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:35.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51167;"]
["$","2022-02-24","03:03:37.400","Ascend","Radiometer post: SATFI40545",2.2200000000000001E-2,2.3900000000000001E-2,1.03E-2,0.21529999999999999]
["$","2022-02-24","03:03:37.800","Ascend","Vel PID Values",9.58,52.970896000000003,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,6.9060999999999997E-2,2.3800000000000001E-4,2.6969E-2,6.3115370000000004,6.3115370000000004,51704,1]
["$","2022-02-24","03:03:37.800","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:38.600","Ascend","[MSC] TX: T1,1645671817,11.5682,33.4946,9.7800"]
["$","2022-02-24","03:03:39.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:41.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51716;"]
["$","2022-02-24","03:03:42.600","Ascend","System Data (dBar %full Volts mAmps): ",8.5,52.824891000000001,32.075000000000003,220,477.58809200000002,67695.705979999999,null,32.075000000000003,421,1387.89906,6769.4497179999998,null,null,null,null,null,null,null,null,null,1228.3000489999999,12.15,37.807999000000002,12.15]
["$","2022-02-24","03:03:43.300","Ascend","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","03:03:44.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:45.300","Ascend","BE::sendJV: -51081"]
["$","2022-02-24","03:03:46.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    7.65, 11.5678, 33.4950  "]
["$","2022-02-24","03:03:46.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:48.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:50.100","Ascend","BE::sendJV: -49568"]
["$","2022-02-24","03:03:50.200","Ascend","Vel PID Values",6.74,52.646537000000002,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.3332999999999995E-2,7.1785000000000002E-2,2.9399999999999999E-4,2.8622999999999999E-2,6.0508480000000002,6.0508480000000002,49568,1]
["$","2022-02-24","03:03:51.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-49575;"]
["$","2022-02-24","03:03:52.200","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-48415;"]
["$","2022-02-24","03:03:55.100","Ascend","getting Elmo deacceleration limit"]
["$","2022-02-24","03:03:54","Ascend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","03:03:55.100","Ascend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","03:03:56.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    5.37, 11.5683, 33.4957  "]
["$","2022-02-24","03:03:57.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:58.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:00.300","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:04:00.500","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:00.700","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:02","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    4.02, 11.5678, 33.4970  "]
["$","2022-02-24","03:04:03.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:04.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:05.200","Ascend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","03:04:06.200","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:04:07","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    2.92, 11.5666, 33.4967  "]
["$","2022-02-24","03:04:08","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    2.72, 11.5673, 33.4965  "]
["$","2022-02-24","03:04:09.200","Ascend","Vel PID Values",2.5099999999999998,52.202494000000002,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.0000000000000007E-2,7.4422000000000002E-2,-1.84E-4,3.0931E-2,6.2243899999999996,6.2243899999999996,50990,1]
["$","2022-02-24","03:04:10.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-50607;"]
["$","2022-02-24","03:04:12.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    1.84, 11.5700, 33.4951  "]
["$","2022-02-24","03:04:13.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:04:14.200","Ascend","Vel PID Values",1.51,52.049824999999998,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,5.3332999999999998E-2,7.3058999999999999E-2,-6.3000000000000003E-4,3.1539999999999999E-2,6.6906230000000004,6.6906230000000004,54809,1]
["$","2022-02-24","03:04:15.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-52402;"]
["$","2022-02-24","03:04:15.500","Set Bellows","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","03:04:15.600","Set Bellows","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","03:04:16.100","Set Bellows","SBE41 Message",1.02,51.933847,32.15,155.5,null,null,null,null,null,null,null,null,"    1.02, 11.5706, 33.4951  ",1.02,2.0717690000000002,7.4800000000000005E-2,7.3332999999999995E-2,8.1667000000000003E-2,0.221723,3000]
["$","2022-02-24","03:04:17.500","Set Bellows","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","03:04:26","Set Bellows","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:04:26.200","Set Bellows","Pump motor not faulted"]
["$","2022-02-24","03:04:30.300","Set Bellows","Checking Global Issues."]
["$","2022-02-24","03:04:36.300","Set Bellows","System Data (dBar %full Volts mAmps): ",1.02,50.997993999999998,31.975000000000001,1055,498.21090700000002,68136.515599999999,null,32.024999999999999,184,1399.117463,6813.5172490000004,null,null,null,null,null,null,null,null,null,1225.579956,12.18,38.097999999999999,12.18]
["$","2022-02-24","03:04:37.400","Set Bellows","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","03:04:46.200","Set Bellows","BE::sendJV: -200000"]
["$","2022-02-24","03:04:46.700","Set Bellows","Twitter msg",null,null,null,null,null,null,"0.68175;"]
["$","2022-02-24","03:04:47.700","Set Bellows","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:04:56.300","Set Bellows","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:04:58.100","Set Bellows","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","03:04:58.100","Set Bellows","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:05:05.100","Set Bellows","Checking Global Issues."]
["$","2022-02-24","03:05:08.200","Set Bellows","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:05:09.600","Set Bellows","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","03:05:19.100","Set Bellows","Pump motor not faulted"]
["$","2022-02-24","03:05:19.500","Set Bellows","Twitter msg",null,null,null,null,null,null,"0.40324;"]
["$","2022-02-24","03:05:22.800","Set Bellows","Checking Global Issues."]
["$","2022-02-24","03:05:29.900","Set Bellows","Checking Global Issues."]
["$","2022-02-24","03:05:31","Set Bellows","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","03:05:36.800","Set Bellows","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:05:40","Dump CPData","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:05:40","Dump CPData","Twitter msg",null,null,null,null,null,null,"MO=0;"]
["$","2022-02-24","03:05:41.200","Dump CPData","Set new CTD WFR timeout to: 00:00:05"]
["$","2022-02-24","03:05:42.200","Dump CPData","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","03:05:43.200","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:43.400","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:43.900","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:44.200","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:44.300","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:44.400","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:44.600","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:44.800","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:44.900","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:45.100","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:45.300","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:45.500","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:45.700","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:45.800","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:46","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:46.200","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:46.300","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:46.500","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:46.700","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:46.900","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:47.100","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:47.200","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:47.400","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:47.500","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:47.700","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:47.700","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:47.900","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:48.100","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:48.300","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:48.400","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:48.600","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:48.800","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:49","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:49.100","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:49.300","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:49.500","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:49.600","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:49.800","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:50","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:50.200","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:50.400","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:50.500","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:50.700","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:50.900","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:51.100","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:51.200","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:51.400","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:51.600","Dump CPData","Trying again for binaverage response"]
["$","2022-02-24","03:05:51.800","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:52","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:52.100","Dump CPData","Sending binaverage wait command"]
["$","2022-02-24","03:05:53.800","Dump CPData","getting Elmo deacceleration limit"]
["$","2022-02-24","03:05:53.200","Dump CPData","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","03:05:54.300","Dump CPData","Appending CP Data:  nbins = 23"]
["$","2022-02-24","03:05:54.500","Dump CPData","Trying again for da response"]
["$","2022-02-24","03:05:54.700","Dump CPData","Sending da wait command"]
["$","2022-02-24","03:05:54.900","Dump CPData","Sending da wait command"]
["$","2022-02-24","03:05:55.200","Dump CPData","Sending da wait command"]
["$","2022-02-24","03:05:55.400","Dump CPData","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   36.03,  10.7294,  33.6674, 12  "]
["$","2022-02-24","03:05:55.700","Dump CPData","Sending da wait command"]
["$","2022-02-24","03:05:55.900","Dump CPData","Appending CP Data: 00142D3182D80A  "]
["$","2022-02-24","03:05:56.200","Dump CPData","Appending CP Data: 00782D1482DD0A  "]
["$","2022-02-24","03:05:56.100","Dump CPData","CP Message",null,null,null,null,null,null,null,null,null,null,null,null,"00DD2CD182E30A  "]
["$","2022-02-24","03:05:56.200","Dump CPData","CP Message",null,null,null,null,null,null,null,null,null,null,null,null,"012C2B9783220B  "]
["$","2022-02-24","03:05:56.300","Dump CPData","CP Message",null,null,null,null,null,null,null,null,null,null,null,null,"01402B0983480B  "]
["$","2022-02-24","03:05:56.400","Dump CPData","CP Message",null,null,null,null,null,null,null,null,null,null,null,null,"01A5298B839812  "]
["$","2022-02-24","03:05:58.200","Dump CPData","Checking Global Issues."]
["$","2022-02-24","03:05:58.300","Surface Ops","Twitter msg",null,null,null,null,null,null,"JV=0;"]
["$","2022-02-24","03:06:19.300","Surface Ops","Attempting GPS time synch, try number: 0;  Set system time to: 02/24/2022 03:06:18"]
["$","2022-02-24","03:06:04.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:06:05.700","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:06:19.700","Surface Ops","SBE41 Message",-0.18,44.875093999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.18,-0.18,0.71076700000000004,7.2878999999999999E-2,-3.333E-3,0,4.3914000000000002E-2,3000]
["$","2022-02-24","03:06:24.900","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","03:06:25.900","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System Control,4330,2707,0,0,0  "]
["$","2022-02-24","03:06:26.400","Surface Ops","Sending Optode Get ConfigXML"]
["$","2022-02-24","03:06:30.300","Surface Ops","Sci Logger sending FastPressure to CTD"]
["$","2022-02-24","03:06:27.500","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CalDataAPress[hPa],4330,2707,993.137  "]
["$","2022-02-24","03:06:28","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog1 Coef,4330,2707,0.000000E+00,1.000000E+00  "]
["$","2022-02-24","03:06:28.700","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"<NodeConfig ID=\"4330-2707\" SerialNo=\"2707\" ProdNo=\"4330\" ProdName=\"Optode Sensor\" Descr=\"Optode Sensor #2707\" Adr=\"3234560\" IsSensor=\"true\" ProtocolVer=\"6\" ConfigVer=\"12\" NodeTypeID=\"2040\">  "]
["$","2022-02-24","03:06:29.800","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"5\" Descr=\"HW Version 3\" Type=\"VT_BSTR\" Access=\"R3W4\">Rev4</Property>  "]
["$","2022-02-24","03:06:33.900","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:06:32.400","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"3\" Descr=\"Flow Control\" Type=\"VT_I4\" Access=\"R3W3\" StandAlone=\"true\" Enum=\"None=0;Xon/Xoff=2\">2</Property>  "]
["$","2022-02-24","03:06:32.500","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"3\" Descr=\"PhaseCoef\" Type=\"VT_ARRAY|VT_R4\" Access=\"R1W3\">6.919999E-01;1.000000E+00;0.000000E+00;0.000000E+00</Property>  "]
["$","2022-02-24","03:06:34.400","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"13\" Descr=\"CalDataZero\" Type=\"VT_ARRAY|VT_R4\" Unit=\"Deg\" Format=\"%0.3f\" Access=\"R1W3\">6.158697E+01;2.215172E+01</Property>  "]
["$","2022-02-24","03:06:35.500","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,,<Property ID=\"0\" Descr=\"Enable Text\" Type=\"VT_BOOL\" Access=\"R1W2\" StandAlone=\"true\">false</Property>  "]
["$","2022-02-24","03:06:37","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",,<PropertyCategory ID=\"5\" Descr=\"Output Settings\">  "]
["$","2022-02-24","03:06:37.800","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,",</ConfigCategory>  "]
["$","2022-02-24","03:06:38.600","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:06:39.600","Surface Ops","SBE41 Message",-0.02,44.874322999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.02,-0.02,-0.17777799999999999,0.123889,-5.3332999999999998E-2,-2.8333000000000001E-2,3.7759000000000001E-2,3000]
["$","2022-02-24","03:06:42.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:06:45.600","Surface Ops","SBE41 Message",-0.12,44.876963000000003,32.15,155.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.173565,7.6988000000000001E-2,-1.6667000000000001E-2,1.6667000000000001E-2,3.5309E-2,3000]
["$","2022-02-24","03:06:51.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:06:55.300"]
["$","2022-02-24","03:06:57","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:00.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:04.600","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.12,44.845080000000003,0.47499999999999998,0,570.31009400000005,69289.577950000006,null,32.15,119.5,1422.67309,6928.8234830000001,null,null,null,null,null,null,null,null,null,1217.3199460000001,12.26,38.139000000000003,12.26]
["$","2022-02-24","03:07:09.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:13.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:18.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:21.600","Surface Ops","SBE41 Message",-0.05,44.851087999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-0.110623,1.544E-3,-4.3333000000000003E-2,-2.5000000000000001E-2,2.3911999999999999E-2,3000]
["$","2022-02-24","03:07:24.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","03:07:25.900","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","03:07:30.800","Surface Ops","SBE41 Message",7.0000000000000007E-2,44.842841,32.15,155.5,null,null,null,null,null,null,null,null,7.0000000000000007E-2,7.0000000000000007E-2,-0.139458,-4.4559999999999999E-3,-0.05,-3.5000000000000003E-2,2.1239999999999998E-2,3000]
["$","2022-02-24","03:07:31.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:32.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:32.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:32.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:33.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:33.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:33.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:33.700","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.19]
["$","2022-02-24","03:07:33.700"]
["$","2022-02-24","03:07:33.700","Surface Ops","SBE41 Message",-0.19,44.850333999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.19,-0.19,-0.13746800000000001,-2.751E-3,8.6666999999999994E-2,1.8332999999999999E-2,2.0392E-2,3000]
["$","2022-02-24","03:07:34.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:35.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:36.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:36.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:36.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:36.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:36.600","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.19,44.838317000000004,0.3,0,570.31140600000003,69551.753570000001,null,32.15,124,1426.6281899999999,6955.0410449999999,null,null,null,null,null,null,null,null,null,1217.369995,12.29,37.897998999999999,12.29]
["$","2022-02-24","03:07:36.700","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:07:38.100","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:07:38.100","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:07:36.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","03:07:38.100"]
["$","2022-02-24","03:07:36.800","Surface Ops","SBE41 Message",-0.05,44.838317000000004,32.15,155.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-0.11693099999999999,1.3999999999999999E-4,-4.6667E-2,0.02,1.9546999999999998E-2,3000]
["$","2022-02-24","03:07:38.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:39.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:39.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:39.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:39.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>f  "]
["$","2022-02-24","03:07:40.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:40.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:40.800","Surface Ops","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","03:07:41.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:42.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:42.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:42.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:42.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.18]
["$","2022-02-24","03:07:42.700"]
["$","2022-02-24","03:07:42.600","Surface Ops","SBE41 Message",-0.18,44.839756000000001,32.15,155.5,null,null,null,null,null,null,null,null,-0.18,-0.18,-9.1131000000000004E-2,1.897E-3,4.3333000000000003E-2,-1.6670000000000001E-3,1.8678E-2,3000]
["$","2022-02-24","03:07:43.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:44.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:45.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:45.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:45.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:45.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:45.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","03:07:45.800"]
["$","2022-02-24","03:07:45.800","Surface Ops","SBE41 Message",-0.15,44.843766000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-6.9980000000000001E-2,8.8900000000000003E-4,-0.01,1.6667000000000001E-2,1.7817E-2,3000]
["$","2022-02-24","03:07:46.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:47.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:47.200","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.15,44.843577000000003,0.27500000000000002,0,570.31140600000003,69638.921589999998,null,32.15,125,1427.9298550000001,6963.7578469999999,null,null,null,null,null,null,null,null,null,1217.369995,12.29,37.887999999999998,12.29]
["$","2022-02-24","03:07:47.300","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:07:48.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:48.700","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:07:48.700","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:07:47.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:47.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:48.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:48.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0.01]
["$","2022-02-24","03:07:48.800"]
["$","2022-02-24","03:07:48.600","Surface Ops","SBE41 Message",0.01,44.843577000000003,32.15,155.5,null,null,null,null,null,null,null,null,0.01,0.01,-6.6231999999999999E-2,-2.496E-3,-5.3332999999999998E-2,-3.1667000000000001E-2,1.6969000000000001E-2,3000]
["$","2022-02-24","03:07:48.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:49.700","Surface Ops","Starting Surface Optode and OCR Samples number 4 of 5"]
["$","2022-02-24","03:07:50.700","Surface Ops","SciLogger is writing previous sample before starting new one"]
["$","2022-02-24","03:07:50.800","Surface Ops","Wrote to msg file: AirCal:,2022-Feb-24T03:07:24Z,NaN,NaN,NaN,11.518,31.297,8.937,,,604,509,545,0.0221,0.0240,0.0089,0.1885  "]
["$","2022-02-24","03:07:50.800","Surface Ops","[ERROR] Missed CTD message 13"]
["$","2022-02-24","03:07:50.800","Surface Ops","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:07:51.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:51.800","Surface Ops","Sci Logger sending FastPressure to CTD"]
["$","2022-02-24","03:07:51.800","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:51.800","Surface Ops","Sci Logger sending sample Optode"]
["$","2022-02-24","03:07:51.800","Surface Ops","Sending Optode Do Sample"]
["$","2022-02-24","03:07:51.800","Surface Ops","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:07:51.800","Surface Ops","Sending radiometer pollSample"]
["$","2022-02-24","03:07:50.500","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:50.500","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:50.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:51.900","Surface Ops","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","03:07:51.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:51.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","03:07:52"]
["$","2022-02-24","03:07:51.600","Surface Ops","SBE41 Message",-0.17,44.830075000000001,32.15,155.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-8.4474999999999995E-2,-5.6829999999999997E-3,0.06,3.333E-3,1.6140999999999999E-2,3000]
["$","2022-02-24","03:07:52","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:53","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:53.700","Surface Ops","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",3.0300000000000001E-2,2.0199999999999999E-2,6.7999999999999996E-3,0.21440000000000001]
["$","2022-02-24","03:07:53.700","Surface Ops","Radiometer post: SATFI40545",3.0300000000000001E-2,2.0199999999999999E-2,6.7999999999999996E-3,0.21440000000000001]
["$","2022-02-24","03:07:53.700","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,305.004,11.070,32.096,31.404,40.342,8.938,692.8,663.2,426.3  "]
["$","2022-02-24","03:07:53.800","Surface Ops","Optode post: 4330,2707,305.004,11.070,32.096,31.404,40.342,8.938,692.8,663.2,426.3  "]
["$","2022-02-24","03:07:53.700","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","03:07:53.700","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:53.700","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:07:54","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:54.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:54.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:54.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","03:07:54.700"]
["$","2022-02-24","03:07:54.600","Surface Ops","SBE41 Message",-0.08,44.826033000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-0.108695,-5.8690000000000001E-3,-0.03,1.4999999999999999E-2,1.5332E-2,3000]
["$","2022-02-24","03:07:55","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:56","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:57","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:57.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:07:57.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:57.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:07:57.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","03:07:57.800"]
["$","2022-02-24","03:07:57.800","Surface Ops","SBE41 Message",-0.09,44.843089999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.118794,-2.7330000000000002E-3,3.333E-3,-1.3332999999999999E-2,1.4529E-2,3000]
["$","2022-02-24","03:07:58","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:58","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.09,44.837879999999998,0.25,0,570.31140600000003,69727.835659999997,null,32.15,123.5,1429.2641799999999,6972.6492539999999,null,null,null,null,null,null,null,null,null,1217.3900149999999,12.3,38.584000000000003,12.3]
["$","2022-02-24","03:07:58.100","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:07:59.500","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:07:59.600","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:07:59.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:07:59.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:07:59.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:00.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:00.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:00.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:00.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","03:08:00.700"]
["$","2022-02-24","03:08:00.600","Surface Ops","SBE41 Message",-0.09,44.840736999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.111139,1.3960000000000001E-3,0,1.6670000000000001E-3,1.3724999999999999E-2,3000]
["$","2022-02-24","03:08:01.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:02.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:03.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:03.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:03.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:03.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:03.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.08]
["$","2022-02-24","03:08:03.800"]
["$","2022-02-24","03:08:03.800","Surface Ops","SBE41 Message",-0.08,44.841365000000003,32.15,155.5,null,null,null,null,null,null,null,null,-0.08,-0.08,-9.9902000000000005E-2,3.8670000000000002E-3,-3.333E-3,-1.6670000000000001E-3,1.2909E-2,3000]
["$","2022-02-24","03:08:04.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:05.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:05.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:05.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:06.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:06.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:06.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:06.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","03:08:06.700"]
["$","2022-02-24","03:08:06.600","Surface Ops","SBE41 Message",-0.12,44.836950999999999,32.15,155.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-9.6648999999999999E-2,3.6519999999999999E-3,1.3332999999999999E-2,5.0000000000000001E-3,1.2081E-2,3000]
["$","2022-02-24","03:08:07.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:08.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:08.600","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.12,44.836323999999998,0.25,0,570.31140600000003,69814.197809999998,null,32.15,121.5,1430.551811,6981.2854699999998,null,null,null,null,null,null,null,null,null,1217.4499510000001,12.31,38.563000000000002,12.31]
["$","2022-02-24","03:08:08.700","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:08:09.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:10.100","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:08:10.100","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:08:09.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:09.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:09.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.16]
["$","2022-02-24","03:08:10.200"]
["$","2022-02-24","03:08:09.800","Surface Ops","SBE41 Message",-0.16,44.836323999999998,32.15,155.5,null,null,null,null,null,null,null,null,-0.16,-0.16,-9.6406000000000006E-2,1.542E-3,1.3332999999999999E-2,1.3332999999999999E-2,1.1224E-2,3000]
["$","2022-02-24","03:08:10.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:11.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:11.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:11.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:12.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:12.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:12.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:12.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","03:08:12.700"]
["$","2022-02-24","03:08:12.600","Surface Ops","SBE41 Message",-0.1,44.832689000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-9.3483999999999998E-2,-7.5799999999999999E-4,-0.02,-3.333E-3,1.031E-2,3000]
["$","2022-02-24","03:08:13.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:14.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:15.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:15.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:15.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:15.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:15.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","03:08:15.800"]
["$","2022-02-24","03:08:15.800","Surface Ops","SBE41 Message",-0.14000000000000001,44.833925999999998,32.15,155.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-9.3195E-2,-1.903E-3,1.3332999999999999E-2,-3.333E-3,9.273E-3,3000]
["$","2022-02-24","03:08:16.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:16.900","Surface Ops","Starting Surface Optode and OCR Samples number 5 of 5"]
["$","2022-02-24","03:08:17.900","Surface Ops","SciLogger is writing previous sample before starting new one"]
["$","2022-02-24","03:08:17.900","Surface Ops","Wrote to msg file: AirCal:,2022-Feb-24T03:07:51Z,NaN,NaN,NaN,11.070,31.404,8.938,,,604,509,545,0.0303,0.0202,0.0068,0.2144  "]
["$","2022-02-24","03:08:17.900","Surface Ops","[ERROR] Missed CTD message 14"]
["$","2022-02-24","03:08:17.900","Surface Ops","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:08:18.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:18.900","Surface Ops","Sci Logger sending FastPressure to CTD"]
["$","2022-02-24","03:08:18.900","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:19","Surface Ops","Sci Logger sending sample Optode"]
["$","2022-02-24","03:08:19","Surface Ops","Sending Optode Do Sample"]
["$","2022-02-24","03:08:19","Surface Ops","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:08:19","Surface Ops","Sending radiometer pollSample"]
["$","2022-02-24","03:08:17.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:17.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:18","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:19.100","Surface Ops","[ERROR]: stuck pressure count = 1   power cycle count = 0"]
["$","2022-02-24","03:08:18.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:18.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.01]
["$","2022-02-24","03:08:19.200"]
["$","2022-02-24","03:08:18.600","Surface Ops","SBE41 Message",-0.01,44.836128000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.01,-0.01,-0.101286,-1.681E-3,-4.3333000000000003E-2,-1.4999999999999999E-2,7.9369999999999996E-3,3000]
["$","2022-02-24","03:08:19.200","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:19.200","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.01,44.851562999999999,0.22500000000000001,0,570.31140600000003,69901.500140000004,null,32.15,136.5,1431.8452130000001,6990.015703,null,null,null,null,null,null,null,null,null,1217.469971,12.31,38.487000000000002,12.31]
["$","2022-02-24","03:08:19.300","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:08:20.700","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:08:20.700","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:08:20.800","Surface Ops","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",2.8500000000000001E-2,2.47E-2,6.4999999999999997E-3,0.22459999999999999]
["$","2022-02-24","03:08:20.800","Surface Ops","Radiometer post: SATFI40545",2.8500000000000001E-2,2.47E-2,6.4999999999999997E-3,0.22459999999999999]
["$","2022-02-24","03:08:19.900","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,307.327,10.893,32.091,31.399,40.336,8.937,692.2,662.9,431.9  "]
["$","2022-02-24","03:08:20.900","Surface Ops","Optode post: 4330,2707,307.327,10.893,32.091,31.399,40.336,8.937,692.2,662.9,431.9  "]
["$","2022-02-24","03:08:19.900","Surface Ops","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","03:08:20.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:20.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:20.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:21.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:21.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:21.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","03:08:21.700"]
["$","2022-02-24","03:08:21.600","Surface Ops","SBE41 Message",-0.14000000000000001,44.832262,32.15,155.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.11433699999999999,-6.7000000000000002E-4,4.3333000000000003E-2,0,6.1190000000000003E-3,3000]
["$","2022-02-24","03:08:21.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:22.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:23.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:24.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:24.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:24.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:24.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","03:08:24.800"]
["$","2022-02-24","03:08:24.800","Surface Ops","SBE41 Message",-0.17,44.838577999999998,32.15,155.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-0.121716,5.4699999999999996E-4,0.01,2.6667E-2,4.3420000000000004E-3,3000]
["$","2022-02-24","03:08:24.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:25.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:26.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:26.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:26.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:27.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:27.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:27.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","03:08:27.700"]
["$","2022-02-24","03:08:27.600","Surface Ops","SBE41 Message",-0.14000000000000001,44.835521,32.15,155.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.11605699999999999,1.6739999999999999E-3,-0.01,0,2.6340000000000001E-3,3000]
["$","2022-02-24","03:08:27.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:28.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:29.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:30","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.14000000000000001,44.830483999999998,0.22500000000000001,0,570.31140600000003,69989.474029999998,null,32.15,127,1433.1702250000001,6998.8130920000003,null,null,null,null,null,null,null,null,null,1217.4499510000001,12.32,37.867001000000002,12.32]
["$","2022-02-24","03:08:30","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:08:30.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:31.400","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:08:31.500","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:08:30.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:30.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:30.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.06]
["$","2022-02-24","03:08:31.600"]
["$","2022-02-24","03:08:30.800","Surface Ops","SBE41 Message",-0.06,44.830483999999998,32.15,155.5,null,null,null,null,null,null,null,null,-0.06,-0.06,-0.103739,2.2759999999999998E-3,-2.6667E-2,-1.8332999999999999E-2,1.1199999999999999E-3,3000]
["$","2022-02-24","03:08:31.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:32.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:33.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:33.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:33.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:33.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:33.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.19]
["$","2022-02-24","03:08:33.700"]
["$","2022-02-24","03:08:33.600","Surface Ops","SBE41 Message",-0.19,44.832946999999997,32.15,155.5,null,null,null,null,null,null,null,null,-0.19,-0.19,-0.10134799999999999,1.707E-3,4.3333000000000003E-2,8.3330000000000001E-3,1.2400000000000001E-4,3000]
["$","2022-02-24","03:08:34.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:35.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:36.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:36.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:36.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:36.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:36.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","03:08:36.800"]
["$","2022-02-24","03:08:36.800","Surface Ops","SBE41 Message",-0.1,44.845024000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.11466800000000001,2.1100000000000001E-4,-0.03,6.6670000000000002E-3,-3.88E-4,3000]
["$","2022-02-24","03:08:37.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:38.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:38.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:38.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:39.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:39.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:39.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:39.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.05]
["$","2022-02-24","03:08:39.700"]
["$","2022-02-24","03:08:39.600","Surface Ops","SBE41 Message",-0.05,44.841509000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.05,-0.05,-0.128332,-8.0400000000000003E-4,-1.6667000000000001E-2,-2.3333E-2,-5.1599999999999997E-4,3000]
["$","2022-02-24","03:08:40.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:40.600","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.05,44.840778999999998,0.22500000000000001,0,570.31140600000003,70076.776360000003,null,32.15,121.5,1434.475563,7007.5433249999996,null,null,null,null,null,null,null,null,null,1217.5200199999999,12.32,38.167000000000002,12.32]
["$","2022-02-24","03:08:40.700","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:08:42.100","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:08:42.100","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:08:42.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:42.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:42.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:42.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:42.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","03:08:42.800"]
["$","2022-02-24","03:08:42.800","Surface Ops","SBE41 Message",-0.14000000000000001,44.843020000000003,32.15,155.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.12953400000000001,-3.9800000000000002E-4,0.03,6.6670000000000002E-3,-4.8000000000000001E-4,3000]
["$","2022-02-24","03:08:43.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:44","Surface Ops","Surface sampling finished"]
["$","2022-02-24","03:08:44","Surface Ops","[MSC] Starting config data collection."]
["$","2022-02-24","03:08:44.100","Surface Ops","[MSC] TX: W"]
["$","2022-02-24","03:08:44.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:44.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:44.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:45.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:45.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:45.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:45.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","03:08:45.700"]
["$","2022-02-24","03:08:45.600","Surface Ops","SBE41 Message",-7.0000000000000007E-2,44.839143999999997,32.15,155.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.124518,9.2000000000000003E-4,-2.3333E-2,3.333E-3,-4.1100000000000002E-4,3000]
["$","2022-02-24","03:08:46.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:47","Surface Ops","[MSC] Timeout for CommandWake"]
["$","2022-02-24","03:08:47.100","Surface Ops","[MSC] TX: W"]
["$","2022-02-24","03:08:47.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:47.200","Surface Ops","[MSC] RX: "]
["$","2022-02-24","03:08:48.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:48.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:48.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:48.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:48.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.17]
["$","2022-02-24","03:08:48.800"]
["$","2022-02-24","03:08:48.800","Surface Ops","SBE41 Message",-0.17,44.836244000000001,32.15,155.5,null,null,null,null,null,null,null,null,-0.17,-0.17,-0.11884,2E-3,3.3333000000000002E-2,5.0000000000000001E-3,-3.4299999999999999E-4,3000]
["$","2022-02-24","03:08:49.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:50.100","Surface Ops","[MSC] Timeout for CommandWake"]
["$","2022-02-24","03:08:50.100","Surface Ops","[MSC] TX: W"]
["$","2022-02-24","03:08:50.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:50.200","Surface Ops","[MSC] RX: ACK  "]
["$","2022-02-24","03:08:50.300","Surface Ops","[MSC] TX: MODE,1"]
["$","2022-02-24","03:08:50.500","Surface Ops","[MSC] RX: ACK,MODE,1  "]
["$","2022-02-24","03:08:50.600","Surface Ops","[MSC] TX: ACK "]
["$","2022-02-24","03:08:50.600","Surface Ops","[MSC] TX: C"]
["$","2022-02-24","03:08:50.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:50.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:50.800","Surface Ops","[MSC] RX: H, Datalogger Serial Num , SN:0003  "]
["$","2022-02-24","03:08:50.900","Surface Ops","[MSC] RX: H, Application      Name , CPF_MAIN.C  "]
["$","2022-02-24","03:08:50.900","Surface Ops","[MSC] RX: H, App Build        Date , Nov 20 2020, 13:19:41  "]
["$","2022-02-24","03:08:51","Surface Ops","[MSC] RX: H, Power Up Time   (GMT) , 02/24/2022 00:57:06  "]
["$","2022-02-24","03:08:51","Surface Ops","[MSC] RX: H, Current  Time   (GMT) , 02/24/2022 03:08:50  "]
["$","2022-02-24","03:08:51.100","Surface Ops","[MSC] RX: H, Alarm    Time   (GMT) , 02/24/2022 10:57:11  "]
["$","2022-02-24","03:08:51.100","Surface Ops","[MSC] RX: H, Power Active  Timeout , 10  "]
["$","2022-02-24","03:08:51.100","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:51.100","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.17,44.841253000000002,0.2,0,570.31140600000003,70163.272830000002,null,32.15,130.5,1435.831005,7016.1929710000004,null,null,null,null,null,null,null,null,null,1217.5,12.33,38.354999999999997,12.33]
["$","2022-02-24","03:08:51.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:51.200","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:08:52.700","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:08:52.700","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:08:52.700","Surface Ops","[MSC] RX: H, Persistor CF2-1M Info , S/N:15079 - BIOS:4.03 - PicoDOS:4.03  "]
["$","2022-02-24","03:08:52.700","Surface Ops","[MSC] RX: H, Compact FLASH    Size , 256614400  "]
["$","2022-02-24","03:08:52.700","Surface Ops","[MSC] RX: H, Compact FLASH    Left , 90.92%  "]
["$","2022-02-24","03:08:51.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:52.800","Surface Ops","[MSC] RX: H, Power Cycle   Counter , 6  "]
["$","2022-02-24","03:08:52.800","Surface Ops","[MSC] RX: H, System Reset  Counter , 6  "]
["$","2022-02-24","03:08:52.800","Surface Ops","[MSC] RX: H, System Error  Counter , 0  "]
["$","2022-02-24","03:08:52.800","Surface Ops","[MSC] RX: H, Last System     Error , 0  "]
["$","2022-02-24","03:08:52.800","Surface Ops","[MSC] RX: H, Last System ErrorTime , 01/01/1970 00:00:00  "]
["$","2022-02-24","03:08:52.900","Surface Ops","[MSC] RX: H, ISUS  Error   Counter , 0  "]
["$","2022-02-24","03:08:52.900","Surface Ops","[MSC] RX: H, Last ISUS       Error , 0  "]
["$","2022-02-24","03:08:52.900","Surface Ops","[MSC] RX: H, Last ISUS Error  Time , 01/01/1970 00:00:00  "]
["$","2022-02-24","03:08:52.900","Surface Ops","[MSC] RX: H, ISUS Sample   Counter , 66  "]
["$","2022-02-24","03:08:52.900","Surface Ops","[MSC] RX: H, Last Sample Rec. Time , 02/24/2022 03:04:12  "]
["$","2022-02-24","03:08:51.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.14000000000000001]
["$","2022-02-24","03:08:53"]
["$","2022-02-24","03:08:51.600","Surface Ops","SBE41 Message",-0.14000000000000001,44.841253000000002,32.15,155.5,null,null,null,null,null,null,null,null,-0.14000000000000001,-0.14000000000000001,-0.10957600000000001,1.91E-3,-0.01,1.1667E-2,-2.8699999999999998E-4,3000]
["$","2022-02-24","03:08:53","Surface Ops","[MSC] RX: H, Fiberlite    Odometer , 05:24:28  "]
["$","2022-02-24","03:08:53","Surface Ops","[MSC] RX: H, Fiberlite      Cycles , 7430  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Spec Intensity LampON , 5000  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Spec Integration Time , 375  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Spec Pre  scans taken , 2  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Spec Lite scans taken , 3  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Spec Dark scans taken , 1  "]
["$","2022-02-24","03:08:53.100","Surface Ops","[MSC] RX: H, Calibration      Date , 11/24/2020  "]
["$","2022-02-24","03:08:53.200","Surface Ops","[MSC] RX: H, Sw Calibration   Temp , 19.94  "]
["$","2022-02-24","03:08:53.200","Surface Ops","[MSC] RX: H, Wavelength Fit  Range , 217.295 <-> 239.828  "]
["$","2022-02-24","03:08:53.200","Surface Ops","[MSC] RX: H, Pixel Fit       Range , 36 <-> 64  "]
["$","2022-02-24","03:08:53.200","Surface Ops","[MSC] RX: H, Fitted Concentrations , 2  "]
["$","2022-02-24","03:08:53.200","Surface Ops","[MSC] RX: H, Baseline        Model , (ax + b)  "]
["$","2022-02-24","03:08:53.300","Surface Ops","[MSC] RX: H, Br Temp  Compensation , ENABLED  "]
["$","2022-02-24","03:08:53.300","Surface Ops","[MSC] RX: H, Bromide Term in Model , will be FIXED (to external CTD value)  "]
["$","2022-02-24","03:08:53.300","Surface Ops","[MSC] RX: H, Zeiss Coefficient Vals, 1.885090e+02,7.959960e-01,1.113850e-04,-3.090260e-07,0.000000e+00  "]
["$","2022-02-24","03:08:53.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:54.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:54.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:54.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:54.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:54.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.1]
["$","2022-02-24","03:08:54.800"]
["$","2022-02-24","03:08:54.800","Surface Ops","SBE41 Message",-0.1,44.833660999999999,32.15,155.5,null,null,null,null,null,null,null,null,-0.1,-0.1,-0.10148,4.1599999999999997E-4,-1.3332999999999999E-2,-1.1667E-2,-2.5099999999999998E-4,3000]
["$","2022-02-24","03:08:55.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:56.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:56.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:08:56.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:08:57.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:08:57.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:08:57.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:57.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.12]
["$","2022-02-24","03:08:57.700"]
["$","2022-02-24","03:08:57.600","Surface Ops","SBE41 Message",-0.12,44.842804999999998,32.15,155.5,null,null,null,null,null,null,null,null,-0.12,-0.12,-0.10377,-1.518E-3,6.6670000000000002E-3,-3.333E-3,-2.33E-4,3000]
["$","2022-02-24","03:08:58.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:08:59.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:00.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:00.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:00.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:00.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:00.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.15]
["$","2022-02-24","03:09:00.800"]
["$","2022-02-24","03:09:00.800","Surface Ops","SBE41 Message",-0.15,44.837401,32.15,155.5,null,null,null,null,null,null,null,null,-0.15,-0.15,-0.11532299999999999,-2.4039999999999999E-3,0.01,8.3330000000000001E-3,-2.2100000000000001E-4,3000]
["$","2022-02-24","03:09:00.900","Surface Ops","[MSC] TX: SE,?"]
["$","2022-02-24","03:09:01.100","Surface Ops","[MSC] RX: ACK,SE?,0  "]
["$","2022-02-24","03:09:01.100","Surface Ops","[MSC] ERRORS AVAILABLE: 0"]
["$","2022-02-24","03:09:01.100","Surface Ops","[MSC] TX: W"]
["$","2022-02-24","03:09:01.200","Surface Ops","[MSC] RX: ACK  "]
["$","2022-02-24","03:09:01.300","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:01.300","Surface Ops","System Data (dBar %full Volts mAmps): ",-0.15,44.838766999999997,0.2,0,570.31140600000003,70246.545819999999,null,32.15,133.5,1437.1638869999999,7024.5202710000003,null,null,null,null,null,null,null,null,null,1217.469971,12.33,38.577998999999998,12.33]
["$","2022-02-24","03:09:01.400","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:09:02.800","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:09:02.800","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:09:02.800","Surface Ops","[MSC] TX: MODE,2"]
["$","2022-02-24","03:09:02.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:02.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:09:02.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:03.100","Surface Ops","[MSC] RX: ACK,MODE,2  "]
["$","2022-02-24","03:09:03.100","Surface Ops","[MSC] TX: ACK "]
["$","2022-02-24","03:09:03.100","Surface Ops","[MSC] TX: C"]
["$","2022-02-24","03:09:03.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:03.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:03.400","Surface Ops","[MSC] RX: H, Datalogger Serial Num , SN:0003  "]
["$","2022-02-24","03:09:03.400","Surface Ops","[MSC] RX: H, Application      Name , CPF_MAIN.C  "]
["$","2022-02-24","03:09:03.500","Surface Ops","[MSC] RX: H, App Build        Date , Nov 20 2020, 13:19:41  "]
["$","2022-02-24","03:09:03.500","Surface Ops","[MSC] RX: H, Power Up Time   (GMT) , 02/24/2022 00:57:06  "]
["$","2022-02-24","03:09:03.500","Surface Ops","[MSC] RX: H, Current  Time   (GMT) , 02/24/2022 03:09:03  "]
["$","2022-02-24","03:09:03.600","Surface Ops","[MSC] RX: H, Alarm    Time   (GMT) , 02/24/2022 10:57:11  "]
["$","2022-02-24","03:09:03.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","03:09:03.700"]
["$","2022-02-24","03:09:03.600","Surface Ops","SBE41 Message",-7.0000000000000007E-2,44.826835000000003,32.15,155.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.126138,-1.745E-3,-2.6667E-2,-8.3330000000000001E-3,-1.93E-4,3000]
["$","2022-02-24","03:09:03.700","Surface Ops","[MSC] RX: H, Power Active  Timeout , 10  "]
["$","2022-02-24","03:09:03.800","Surface Ops","[MSC] RX: H, Persistor CF2-1M Info , S/N:15079 - BIOS:4.03 - PicoDOS:4.03  "]
["$","2022-02-24","03:09:03.800","Surface Ops","[MSC] RX: H, Compact FLASH    Size , 256614400  "]
["$","2022-02-24","03:09:03.800","Surface Ops","[MSC] RX: H, Compact FLASH    Left , 90.92%  "]
["$","2022-02-24","03:09:03.800","Surface Ops","[MSC] RX: H, Power Cycle   Counter , 6  "]
["$","2022-02-24","03:09:03.800","Surface Ops","[MSC] RX: H, System Reset  Counter , 6  "]
["$","2022-02-24","03:09:03.900","Surface Ops","[MSC] RX: H, System Error  Counter , 0  "]
["$","2022-02-24","03:09:03.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:03.900","Surface Ops","[MSC] RX: H, Last System     Error , 0  "]
["$","2022-02-24","03:09:04","Surface Ops","[MSC] RX: H, Last System ErrorTime , 01/01/1970 00:00:00  "]
["$","2022-02-24","03:09:04","Surface Ops","[MSC] RX: H, DURA  Error   Counter , 0  "]
["$","2022-02-24","03:09:04","Surface Ops","[MSC] RX: H, Last DURA       Error , 0  "]
["$","2022-02-24","03:09:04.100","Surface Ops","[MSC] RX: H, Last DURA Error  Time , 01/01/1970 00:00:00  "]
["$","2022-02-24","03:09:04.100","Surface Ops","[MSC] RX: H, DURA Sample   Counter , 66  "]
["$","2022-02-24","03:09:04.200","Surface Ops","[MSC] RX: H, Last Sample Rec. Time , 02/24/2022 03:04:21  "]
["$","2022-02-24","03:09:04.200","Surface Ops","[MSC] RX: H, AtoD Reads per Sample , 10  "]
["$","2022-02-24","03:09:04.200","Surface Ops","[MSC] RX: H, AtoD Reading    Delay , 100  "]
["$","2022-02-24","03:09:04.300","Surface Ops","[MSC] RX: H, Samps per AtoD  Recal , 250  "]
["$","2022-02-24","03:09:04.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:05.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:06.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:06.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:06.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:06.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.13]
["$","2022-02-24","03:09:06.800"]
["$","2022-02-24","03:09:06.800","Surface Ops","SBE41 Message",-0.13,44.833951999999996,32.15,155.5,null,null,null,null,null,null,null,null,-0.13,-0.13,-0.12845000000000001,-1.9699999999999999E-4,0.02,-3.333E-3,-1.4799999999999999E-4,3000]
["$","2022-02-24","03:09:06.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:07.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:08.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:08.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>  "]
["$","2022-02-24","03:09:08.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:09.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:09.300","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:09.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","03:09:09.700"]
["$","2022-02-24","03:09:09.600","Surface Ops","SBE41 Message",0,44.836542000000001,32.15,155.5,null,null,null,null,null,null,null,null,0,0,-0.124519,1.343E-3,-4.3333000000000003E-2,-1.1667E-2,-9.5000000000000005E-5,3000]
["$","2022-02-24","03:09:09.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:10.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:11.900","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:11.900","Surface Ops","System Data (dBar %full Volts mAmps): ",0,44.847689000000003,0.2,0,570.31140600000003,70333.579530000003,null,32.15,135,1438.5552680000001,7033.2236419999999,null,null,null,null,null,null,null,null,null,1217.4499510000001,12.34,37.681998999999998,12.34]
["$","2022-02-24","03:09:12","Surface Ops","Pump motor not faulted"]
["$","2022-02-24","03:09:12.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:13.400","Surface Ops","getting Elmo acceleration limit"]
["$","2022-02-24","03:09:13.400","Surface Ops","getting Elmo deacceleration limit"]
["$","2022-02-24","03:09:12.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:12.400","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:12.800","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-0.09]
["$","2022-02-24","03:09:13.500"]
["$","2022-02-24","03:09:12.800","Surface Ops","SBE41 Message",-0.09,44.847689000000003,32.15,155.5,null,null,null,null,null,null,null,null,-0.09,-0.09,-0.120277,2.137E-3,0.03,-6.6670000000000002E-3,-3.6999999999999998E-5,3000]
["$","2022-02-24","03:09:13.600","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:13.600","Surface Ops","[MSC] TX: SE,?"]
["$","2022-02-24","03:09:13.800","Surface Ops","[MSC] RX: ACK,SE?,0  "]
["$","2022-02-24","03:09:13.800","Surface Ops","[MSC] ERRORS AVAILABLE: 0"]
["$","2022-02-24","03:09:13.800","Surface Ops","IModem Sending SBDD2 cmd"]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->  <--  "]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->0  <--  "]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:09:14","Surface Ops","IModem invalid response: IModem Looking for IModem-->OK<--  IModem Got-->  <--  "]
["$","2022-02-24","03:09:13.900","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OK  "]
["$","2022-02-24","03:09:14","Surface Ops","IModem correct response: IModem Looking for IModem-->OK<--  IModem Got-->OK  <--  "]
["$","2022-02-24","03:09:14","Surface Ops","IModem Sending CREG cmd"]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem invalid response: IModem Looking for IModem-->+CREG:<--  IModem Got-->  <--  "]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+CREG:000,001  "]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem correct response: IModem Looking for IModem-->+CREG:<--  IModem Got-->+CREG:000,001  <--  "]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
["$","2022-02-24","03:09:14.100","Surface Ops","IModem Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OK  "]
["$","2022-02-24","03:09:15.200","Surface Ops","CTD Sending fast pressure"]
["$","2022-02-24","03:09:17.200","Surface Ops","Trying GPS get position try num: 0 of 2",-0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UBX,00,030917.00,3652.73138,N,12156.35823,W,-34.383,G3,4.7,5.8,1.771,83.14,-0.222,,1.26,2.07,1.52,7,0,0*70  "]
["$","2022-02-24","03:09:17.300","Surface Ops","Got Position: lat = 3652.73138","N  lon = 12156.35823","W   num sats = 7"]
["$","2022-02-24","03:09:17.300","Surface Ops","Succesful GPS getPosition"]
["$","2022-02-24","03:09:15.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"SBE 41CP V 7.2.5  "]
["$","2022-02-24","03:09:15.200","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"S>fp  "]
["$","2022-02-24","03:09:15.600","Surface Ops","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,-7.0000000000000007E-2]
["$","2022-02-24","03:09:17.400"]
["$","2022-02-24","03:09:15.600","Surface Ops","SBE41 Message",-7.0000000000000007E-2,44.834071999999999,32.15,155.5,null,null,null,null,null,null,null,null,-7.0000000000000007E-2,-7.0000000000000007E-2,-0.114066,1.7960000000000001E-3,-6.6670000000000002E-3,1.1667E-2,2.4000000000000001E-5,3000]
["$","2022-02-24","03:09:17.400","Surface Ops","Checking Global Issues."]
["$","2022-02-24","03:09:17.400","Surface Ops","Ending SciLogger Sample Cycle"]
["$","2022-02-24","03:09:17.400","Surface Ops","SciLogger endSampleCycle is writing samples"]
["$","2022-02-24","03:09:17.500","Surface Ops","Wrote to msg file: AirCal:,2022-Feb-24T03:08:19Z,NaN,NaN,NaN,10.893,31.399,8.937,,,604,509,545,0.0285,0.0247,0.0065,0.2246  "]
["$","2022-02-24","03:09:17.500","Surface Ops","[ERROR] Missed CTD message 15"]

{"sheet":"Ascend Science Samples","index":2,"n_rows":271,"n_cols":52,"rows_kept":271,"cut":false,"hidden":false,"merged":[]}
["$","Date","Time","State","Comment","Pressure","BelPos","PumpVolts","PumpMilliamps","PumpoCoulombs","PumpJoules","PumpMotor","HotelVolts","HotelMilliamps","HotelCoulombs","HotelJoules","CTDTemp","CTDSal","RawPress","LPFPress","LPFVel","DiffVel","Diff2 Vel","SlopeLPFPress.","CTDSamplePeriod","LPS331Press","LPS331Temp","SHT21Humid","SHT21Temp","pidSP","pidPV","pidY1","pidY2","pidI","pid_v","pid_u","pid_uCPS","pid_h","FLBB","Topt","Tphase","Rphase","NO3","pHVrs","OCRtext","OCRCh1","OCRCh2","OCRCh3","OCRCH4","GPS","IridModem","MSC"]
["$","2022-02-24","03:00:51.600","Ascend","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:00:51.600","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:00:51.600","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:00:51.600","Ascend","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","03:00:51.600","Ascend","Sci Logger sending sample FLBB"]
["$","2022-02-24","03:00:51.600","Ascend","Sending FLBB run command"]
["$","2022-02-24","03:00:51.600","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:00:51.700","Ascend","Sending radiometer pollSample"]
["$","2022-02-24","03:00:51.800","Ascend","Checking Global Issues."]
["$","2022-02-24","03:00:52.800","Ascend","Checking Global Issues."]
["$","2022-02-24","03:00:52.800","Ascend","System Data (dBar %full Volts mAmps): ",39.990001999999997,57.890839999999997,32.1,305,428.77302400000002,66303.032309999995,null,32.1,187,1350.7609419999999,6630.1823510000004,null,null,null,null,null,null,null,null,null,1234.5200199999999,12.12,37.950001,12.12]
["$","2022-02-24","03:00:52.900","Ascend","Pump motor not faulted"]
["$","2022-02-24","03:00:54.300","Ascend","getting Elmo acceleration limit"]
["$","2022-02-24","03:00:54.300","Ascend","getting Elmo deacceleration limit"]
["$","2022-02-24","03:00:54.300","Ascend","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",2.7300000000000001E-2,2.6499999999999999E-2,9.1000000000000004E-3,0.22120000000000001]
["$","2022-02-24","03:00:54.400","Ascend","Radiometer post: SATFI40545",2.7300000000000001E-2,2.6499999999999999E-2,9.1000000000000004E-3,0.22120000000000001]
["$","2022-02-24","03:00:52.900","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   39.88, 10.6689, 33.6802  "]
["$","2022-02-24","03:00:54.400","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:00:54.400","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:00:54.400","Ascend","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","03:00:54.400","Ascend","Setting MSC time and CTD Values: 1645671654,33.68,10.669,39.88"]
["$","2022-02-24","03:00:54.500","Ascend","SciLogger: Starting PHandNO3 sequence"]
["$","2022-02-24","03:00:54.500","Ascend","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","03:00:54.500","Ascend","[MSC] Starting ISUS Sample"]
["$","2022-02-24","03:00:54.500","Ascend","[MSC] TX: W"]
["$","2022-02-24","03:00:54.500"]
["$","2022-02-24","03:00:54.500","Ascend","BE::sendJV: -65744"]
["$","2022-02-24","03:00:54.600","Ascend","Vel PID Values",39.880001,57.856572,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,3.6666999999999998E-2,3.4167999999999997E-2,1.555E-3,3.0760000000000002E-3,8.0254200000000004,8.0254200000000004,65744,1]
["$","2022-02-24","03:00:52.900","Ascend","SBE41 Message",39.880001,57.856572,32.15,155.5,null,null,null,null,null,null,null,null,"   39.88, 10.6689, 33.6802  ",39.880001,40.472825,4.4127E-2,3.6666999999999998E-2,3.5000000000000003E-2,9.4470999999999999E-2,3000]
["$","2022-02-24","03:00:52.900","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,159.039,10.579,40.374,39.682,48.608,8.926,934.3,669.4,442.0  "]
["$","2022-02-24","03:00:54.700","Ascend","Optode post: 4330,2707,159.039,10.579,40.374,39.682,48.608,8.926,934.3,669.4,442.0  "]
[]
["$","2022-02-24","03:01:24.500","Ascend","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:01:24.500","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:01:24.500","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:01:24.600","Ascend","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","03:01:24.600","Ascend","Sci Logger sending sample FLBB"]
["$","2022-02-24","03:01:24.600","Ascend","Sending FLBB run command"]
["$","2022-02-24","03:01:24.600","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:01:24.600","Ascend","Sending radiometer pollSample"]
["$","2022-02-24","03:01:24.900","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:24.900","Ascend","System Data (dBar %full Volts mAmps): ",34.869999,56.769151000000001,32.1,285,438.39385600000003,66566.551040000006,null,32.125,213.5,1357.634033,6656.5207929999997,null,null,null,null,null,null,null,null,null,1233.119995,12.12,37.419998,12.12]
["$","2022-02-24","03:01:25","Ascend","Pump motor not faulted"]
["$","2022-02-24","03:01:26.400","Ascend","getting Elmo acceleration limit"]
["$","2022-02-24","03:01:26.400","Ascend","getting Elmo deacceleration limit"]
["$","2022-02-24","03:01:26.500","Ascend","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",3.8699999999999998E-2,2.0799999999999999E-2,8.6E-3,0.22950000000000001]
["$","2022-02-24","03:01:26.500","Ascend","Radiometer post: SATFI40545",3.8699999999999998E-2,2.0799999999999999E-2,8.6E-3,0.22950000000000001]
["$","2022-02-24","03:01:25","Ascend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:01:25","Ascend","Twitter msg",null,null,null,null,null,null,"-57480;"]
["$","2022-02-24","03:01:25.200","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   34.72, 10.7452, 33.6748  "]
["$","2022-02-24","03:01:26.600","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:01:26.600","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:01:26.600","Ascend","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","03:01:26.600","Ascend","Setting MSC time and CTD Values: 1645671686,33.67,10.745,34.72"]
["$","2022-02-24","03:01:26.600","Ascend","SciLogger: Starting PHandNO3 sequence"]
["$","2022-02-24","03:01:26.600","Ascend","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","03:01:26.600","Ascend","[MSC] Starting ISUS Sample"]
["$","2022-02-24","03:01:26.600","Ascend","[MSC] TX: W"]
["$","2022-02-24","03:01:26.700"]
["$","2022-02-24","03:01:26.700","Ascend","BE::sendJV: -58630"]
["$","2022-02-24","03:01:26.800","Ascend","Vel PID Values",34.720001000000003,56.775036999999998,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,4.9999000000000002E-2,5.4011999999999998E-2,6.6299999999999996E-4,8.4910000000000003E-3,7.1570819999999999,7.1570819999999999,58630,1]
["$","2022-02-24","03:01:25.200","Ascend","SBE41 Message",34.720001000000003,56.775036999999998,32.15,155.5,null,null,null,null,null,null,null,null,"   34.72, 10.7452, 33.6748  ",34.720001000000003,35.692162000000003,5.0227000000000001E-2,4.9999000000000002E-2,6.3333E-2,0.14613699999999999,3000]
["$","2022-02-24","03:01:25.200","Ascend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","03:01:25.200","Ascend","Twitter msg",null,null,null,null,null,null,"0.26595;"]
["$","2022-02-24","03:01:25.400","Ascend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","03:01:25.400","Ascend","Twitter msg",null,null,null,null,null,null,"-1.05570;"]
["$","2022-02-24","03:01:26.900","Ascend","FLBB Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"/99/99,99:99:99,695,79,700,710,546  "]
["$","2022-02-24","03:01:27","Ascend","FLBB post: /99/99,99:99:99,695,79,700,710,546  "]
["$","2022-02-24","03:01:25.500","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,160.294,10.661,40.234,39.542,48.467,8.925,930.6,669.2,439.4  "]
["$","2022-02-24","03:01:27","Ascend","Optode post: 4330,2707,160.294,10.661,40.234,39.542,48.467,8.925,930.6,669.2,439.4  "]
[]
["$","2022-02-24","03:01:52.500","Ascend","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:01:52.500","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:01:52.500","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:01:52.500","Ascend","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","03:01:52.600","Ascend","Sci Logger sending sample FLBB"]
["$","2022-02-24","03:01:52.600","Ascend","Sending FLBB run command"]
["$","2022-02-24","03:01:52.600","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:01:52.600","Ascend","Sending radiometer pollSample"]
["$","2022-02-24","03:01:52.700","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:53.700","Ascend","Checking Global Issues."]
["$","2022-02-24","03:01:54.700","Ascend","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",2.5000000000000001E-2,2.5100000000000001E-2,1.0500000000000001E-2,0.21679999999999999]
["$","2022-02-24","03:01:54.700","Ascend","Radiometer post: SATFI40545",2.5000000000000001E-2,2.5100000000000001E-2,1.0500000000000001E-2,0.21679999999999999]
["$","2022-02-24","03:01:54.700","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   29.82, 11.1636, 33.5652  "]
["$","2022-02-24","03:01:54.700","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:01:54.700","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:01:54.700","Ascend","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","03:01:54.800","Ascend","Setting MSC time and CTD Values: 1645671714,33.57,11.164,29.82"]
["$","2022-02-24","03:01:54.800","Ascend","SciLogger: Starting PHandNO3 sequence"]
["$","2022-02-24","03:01:54.800","Ascend","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","03:01:54.800","Ascend","[MSC] Starting ISUS Sample"]
["$","2022-02-24","03:01:54.800","Ascend","[MSC] TX: W"]
["$","2022-02-24","03:01:54.800"]
["$","2022-02-24","03:01:54.800","Ascend","BE::sendJV: -59100"]
["$","2022-02-24","03:01:55","Ascend","Vel PID Values",29.82,55.863588999999997,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,4.6665999999999999E-2,6.0421000000000002E-2,-4.3999999999999999E-5,1.2643E-2,7.2144269999999997,7.2144269999999997,59100,1]
["$","2022-02-24","03:01:54.700","Ascend","SBE41 Message",29.82,55.863588999999997,32.15,155.5,null,null,null,null,null,null,null,null,"   29.82, 11.1636, 33.5652  ",29.82,30.701733000000001,5.9854999999999998E-2,4.6665999999999999E-2,4.8333000000000001E-2,0.17024900000000001,3000]
["$","2022-02-24","03:01:54.700","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   29.69, 11.1676, 33.5729  "]
["$","2022-02-24","03:01:55.100","Ascend","BE::sendJV: -61092"]
["$","2022-02-24","03:01:55.200","Ascend","Vel PID Values",29.690000999999999,55.842177999999997,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,4.3333000000000003E-2,6.0103999999999998E-2,-3.1700000000000001E-4,1.2787E-2,7.4575820000000004,7.4575820000000004,61092,1]
["$","2022-02-24","03:01:54.700","Ascend","SBE41 Message",29.690000999999999,55.842177999999997,32.15,155.5,null,null,null,null,null,null,null,null,"   29.69, 11.1676, 33.5729  ",29.690000999999999,30.504859,6.1336000000000002E-2,4.3333000000000003E-2,4.4999999999999998E-2,0.170739,3000]
["$","2022-02-24","03:01:54.700","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,163.191,10.729,39.976,39.284,48.210,8.927,923.4,668.7,437.2  "]
["$","2022-02-24","03:01:55.300","Ascend","Optode post: 4330,2707,163.191,10.729,39.976,39.284,48.210,8.927,923.4,668.7,437.2  "]
[]
["$","2022-02-24","03:02:20.500","Ascend","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:02:20.500","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:02:20.600","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:02:20.600","Ascend","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","03:02:20.600","Ascend","Sci Logger sending sample FLBB"]
["$","2022-02-24","03:02:20.600","Ascend","Sending FLBB run command"]
["$","2022-02-24","03:02:20.600","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:02:20.600","Ascend","Sending radiometer pollSample"]
["$","2022-02-24","03:02:21.500","Ascend","Checking Global Issues."]
["$","2022-02-24","03:02:22.400","Ascend","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",3.1300000000000001E-2,2.47E-2,9.5999999999999992E-3,0.22850000000000001]
["$","2022-02-24","03:02:22.500","Ascend","Radiometer post: SATFI40545",3.1300000000000001E-2,2.47E-2,9.5999999999999992E-3,0.22850000000000001]
["$","2022-02-24","03:02:22.400","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   24.57, 11.4384, 33.5121  "]
["$","2022-02-24","03:02:22.500","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:02:22.500","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:02:22.500","Ascend","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","03:02:22.600","Ascend","Setting MSC time and CTD Values: 1645671742,33.51,11.438,24.57"]
["$","2022-02-24","03:02:22.600","Ascend","SciLogger: Starting PHandNO3 sequence"]
["$","2022-02-24","03:02:22.600","Ascend","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","03:02:22.600","Ascend","[MSC] Starting ISUS Sample"]
["$","2022-02-24","03:02:22.600","Ascend","[MSC] TX: W"]
["$","2022-02-24","03:02:22.600"]
["$","2022-02-24","03:02:22.600","Ascend","BE::sendJV: -56334"]
["$","2022-02-24","03:02:22.800","Ascend","Vel PID Values",24.57,55.104717999999998,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.3334000000000001E-2,6.2728999999999993E-2,1.5200000000000001E-4,1.6615999999999999E-2,6.8768070000000003,6.8768070000000003,56334,1]
["$","2022-02-24","03:02:22.400","Ascend","SBE41 Message",24.57,55.104717999999998,32.15,155.5,null,null,null,null,null,null,null,null,"   24.57, 11.4384, 33.5121  ",24.57,25.550951999999999,6.0149000000000001E-2,6.3334000000000001E-2,0.06,0.183337,3000]
["$","2022-02-24","03:02:22.400","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   24.39, 11.4380, 33.5078  "]
["$","2022-02-24","03:02:22.900","Ascend","BE::sendJV: -56756"]
["$","2022-02-24","03:02:23","Ascend","Vel PID Values",24.389999,55.061636,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,0.06,6.2808000000000003E-2,8.0000000000000007E-5,1.6754999999999999E-2,6.9282490000000001,6.9282490000000001,56756,1]
["$","2022-02-24","03:02:22.400","Ascend","SBE41 Message",24.389999,55.061636,32.15,155.5,null,null,null,null,null,null,null,null,"   24.39, 11.4380, 33.5078  ",24.389999,25.346187,6.0407000000000002E-2,0.06,6.1667E-2,0.18365300000000001,3000]
["$","2022-02-24","03:02:22.400","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,171.175,11.109,39.180,38.488,47.415,8.927,900.7,667.6,425.0  "]
["$","2022-02-24","03:02:23.100","Ascend","Optode post: 4330,2707,171.175,11.109,39.180,38.488,47.415,8.927,900.7,667.6,425.0  "]
[]
["$","2022-02-24","03:02:46.500","Ascend","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:02:46.500","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:02:46.500","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:02:46.500","Ascend","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","03:02:46.500","Ascend","Sci Logger sending sample FLBB"]
["$","2022-02-24","03:02:46.500","Ascend","Sending FLBB run command"]
["$","2022-02-24","03:02:46.500","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:02:46.500","Ascend","Sending radiometer pollSample"]
["$","2022-02-24","03:02:46.600","Ascend","Checking Global Issues."]
["$","2022-02-24","03:02:47.600","Ascend","Checking Global Issues."]
["$","2022-02-24","03:02:48.400","Ascend","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",3.4599999999999999E-2,2.29E-2,7.7000000000000002E-3,0.21779999999999999]
["$","2022-02-24","03:02:48.500","Ascend","Radiometer post: SATFI40545",3.4599999999999999E-2,2.29E-2,7.7000000000000002E-3,0.21779999999999999]
["$","2022-02-24","03:02:48.400","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   19.64, 11.4907, 33.5051  "]
["$","2022-02-24","03:02:48.500","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:02:48.500","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:02:48.500","Ascend","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","03:02:48.500","Ascend","Setting MSC time and CTD Values: 1645671768,33.51,11.491,19.64"]
["$","2022-02-24","03:02:48.500","Ascend","SciLogger: Starting PHandNO3 sequence"]
["$","2022-02-24","03:02:48.600","Ascend","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","03:02:48.600","Ascend","[MSC] Starting ISUS Sample"]
["$","2022-02-24","03:02:48.600","Ascend","[MSC] TX: W"]
["$","2022-02-24","03:02:48.600"]
["$","2022-02-24","03:02:48.600","Ascend","BE::sendJV: -56286"]
["$","2022-02-24","03:02:48.700","Ascend","Vel PID Values",19.639999,54.356279000000001,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,0.06,6.4207E-2,1.5999999999999999E-5,2.0239E-2,6.8709319999999998,6.8709319999999998,56286,1]
["$","2022-02-24","03:02:48.400","Ascend","SBE41 Message",19.639999,54.356279000000001,32.15,155.5,null,null,null,null,null,null,null,null,"   19.64, 11.4907, 33.5051  ",19.639999,20.589718999999999,6.5453999999999998E-2,0.06,6.1667E-2,0.18787799999999999,3000]
["$","2022-02-24","03:02:48.400","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   19.45, 11.4901, 33.5062  "]
["$","2022-02-24","03:02:48.800","Ascend","BE::sendJV: -56401"]
["$","2022-02-24","03:02:49","Ascend","Vel PID Values",19.450001,54.323748999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.3333E-2,6.4205999999999999E-2,-9.9999999999999995E-7,2.0376999999999999E-2,6.8849229999999997,6.8849229999999997,56401,1]
["$","2022-02-24","03:02:48.400","Ascend","SBE41 Message",19.450001,54.323748999999999,32.15,155.5,null,null,null,null,null,null,null,null,"   19.45, 11.4901, 33.5062  ",19.450001,20.400379999999998,6.5153000000000003E-2,6.3333E-2,6.1665999999999999E-2,0.188,3000]
["$","2022-02-24","03:02:48.400","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,194.736,11.398,37.415,36.723,45.653,8.930,849.5,665.7,415.8  "]
["$","2022-02-24","03:02:49.100","Ascend","Optode post: 4330,2707,194.736,11.398,37.415,36.723,45.653,8.930,849.5,665.7,415.8  "]
[]
["$","2022-02-24","03:03:11.400","Ascend","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:03:11.400","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:03:11.400","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:03:11.400","Ascend","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","03:03:11.500","Ascend","Sci Logger sending sample FLBB"]
["$","2022-02-24","03:03:11.500","Ascend","Sending FLBB run command"]
["$","2022-02-24","03:03:11.500","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:03:11.500","Ascend","Sending radiometer pollSample"]
["$","2022-02-24","03:03:11.500","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:11.500","Ascend","System Data (dBar %full Volts mAmps): ",14.91,53.730220000000003,32.1,260,468.98508700000002,67440.917480000004,null,32.125,197.5,1380.912644,6743.9708680000003,null,null,null,null,null,null,null,null,null,1229.3199460000001,12.14,38.050998999999997,12.14]
["$","2022-02-24","03:03:11.600","Ascend","Pump motor not faulted"]
["$","2022-02-24","03:03:13","Ascend","getting Elmo acceleration limit"]
["$","2022-02-24","03:03:13","Ascend","getting Elmo deacceleration limit"]
["$","2022-02-24","03:03:11.600","Ascend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:03:11.600","Ascend","Twitter msg",null,null,null,null,null,null,"-54887;"]
["$","2022-02-24","03:03:13.100","Ascend","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",2.6800000000000001E-2,2.3900000000000001E-2,8.3999999999999995E-3,0.22459999999999999]
["$","2022-02-24","03:03:13.100","Ascend","Radiometer post: SATFI40545",2.6800000000000001E-2,2.3900000000000001E-2,8.3999999999999995E-3,0.22459999999999999]
["$","2022-02-24","03:03:11.800","Ascend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","03:03:11.800","Ascend","Twitter msg",null,null,null,null,null,null,"0.18683;"]
["$","2022-02-24","03:03:12","Ascend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","03:03:12","Ascend","Twitter msg",null,null,null,null,null,null,"-2.36833;"]
["$","2022-02-24","03:03:12.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"   14.71, 11.5346, 33.5002  "]
["$","2022-02-24","03:03:13.300","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:03:13.300","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:03:13.300","Ascend","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","03:03:13.300","Ascend","Setting MSC time and CTD Values: 1645671793,33.50,11.535,14.71"]
["$","2022-02-24","03:03:13.300","Ascend","SciLogger: Starting PHandNO3 sequence"]
["$","2022-02-24","03:03:13.300","Ascend","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","03:03:13.300","Ascend","[MSC] Starting ISUS Sample"]
["$","2022-02-24","03:03:13.300","Ascend","[MSC] TX: W"]
["$","2022-02-24","03:03:13.300"]
["$","2022-02-24","03:03:13.400","Ascend","BE::sendJV: -55508"]
["$","2022-02-24","03:03:13.500","Ascend","Vel PID Values",14.71,53.727451000000002,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,6.5645999999999996E-2,-5.0000000000000004E-6,2.3630999999999999E-2,6.7758989999999999,6.7758989999999999,55508,1]
["$","2022-02-24","03:03:12.100","Ascend","SBE41 Message",14.71,53.727451000000002,32.15,155.5,null,null,null,null,null,null,null,null,"   14.71, 11.5346, 33.5002  ",14.71,15.690272,6.5723000000000004E-2,6.6667000000000004E-2,6.6667000000000004E-2,0.196129,3000]
["$","2022-02-24","03:03:12.200","Ascend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","03:03:12.200","Ascend","Twitter msg",null,null,null,null,null,null,"62964496;"]
["$","2022-02-24","03:03:13.600","Ascend","FLBB Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"/99/99,99:99:99,695,347,700,551,546  "]
["$","2022-02-24","03:03:13.600","Ascend","FLBB post: /99/99,99:99:99,695,347,700,551,546  "]
["$","2022-02-24","03:03:12.400","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,220.361,11.477,35.835,35.143,44.077,8.933,802.5,663.8,413.3  "]
["$","2022-02-24","03:03:13.700","Ascend","Optode post: 4330,2707,220.361,11.477,35.835,35.143,44.077,8.933,802.5,663.8,413.3  "]
[]
["$","2022-02-24","03:03:35.400","Ascend","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:03:35.400","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:03:35.400","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:03:35.400","Ascend","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","03:03:35.400","Ascend","Sci Logger sending sample FLBB"]
["$","2022-02-24","03:03:35.500","Ascend","Sending FLBB run command"]
["$","2022-02-24","03:03:35.500","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:03:35.500","Ascend","Sending radiometer pollSample"]
["$","2022-02-24","03:03:36","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:37","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:37.300","Ascend","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",2.2200000000000001E-2,2.3900000000000001E-2,1.03E-2,0.21529999999999999]
["$","2022-02-24","03:03:37.400","Ascend","Radiometer post: SATFI40545",2.2200000000000001E-2,2.3900000000000001E-2,1.03E-2,0.21529999999999999]
["$","2022-02-24","03:03:37.300","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    9.78, 11.5682, 33.4946  "]
["$","2022-02-24","03:03:37.400","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:03:37.400","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:03:37.400","Ascend","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","03:03:37.400","Ascend","Setting MSC time and CTD Values: 1645671817,33.49,11.568,9.78"]
["$","2022-02-24","03:03:37.400","Ascend","SciLogger: Starting PHandNO3 sequence"]
["$","2022-02-24","03:03:37.500","Ascend","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","03:03:37.500","Ascend","[MSC] Starting ISUS Sample"]
["$","2022-02-24","03:03:37.500","Ascend","[MSC] TX: W"]
["$","2022-02-24","03:03:37.500"]
["$","2022-02-24","03:03:37.500","Ascend","BE::sendJV: -51233"]
["$","2022-02-24","03:03:37.600","Ascend","Vel PID Values",9.7799999999999994,52.981067000000003,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.0000000000000007E-2,6.8822999999999995E-2,3.3399999999999999E-4,2.6839999999999999E-2,6.2540570000000004,6.2540570000000004,51233,1]
["$","2022-02-24","03:03:37.300","Ascend","SBE41 Message",9.7799999999999994,52.981067000000003,32.15,155.5,null,null,null,null,null,null,null,null,"    9.78, 11.5682, 33.4946  ",9.7799999999999994,10.856546,6.9323999999999997E-2,7.0000000000000007E-2,7.3332999999999995E-2,0.19777,3000]
["$","2022-02-24","03:03:37.300","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    9.58, 11.5677, 33.4944  "]
["$","2022-02-24","03:03:37.700","Ascend","BE::sendJV: -51704"]
["$","2022-02-24","03:03:37.800","Ascend","Vel PID Values",9.58,52.970896000000003,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,6.9060999999999997E-2,2.3800000000000001E-4,2.6969E-2,6.3115370000000004,6.3115370000000004,51704,1]
["$","2022-02-24","03:03:37.300","Ascend","SBE41 Message",9.58,52.970896000000003,32.15,155.5,null,null,null,null,null,null,null,null,"    9.58, 11.5677, 33.4944  ",9.58,10.64748,6.9327E-2,6.6667000000000004E-2,6.8333000000000005E-2,0.19803100000000001,3000]
["$","2022-02-24","03:03:37.300","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,238.796,11.525,34.821,34.129,43.064,8.935,772.3,662.9,411.7  "]
["$","2022-02-24","03:03:38","Ascend","Optode post: 4330,2707,238.796,11.525,34.821,34.129,43.064,8.935,772.3,662.9,411.7  "]
[]
["$","2022-02-24","03:03:58.400","Ascend","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:03:58.400","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:03:58.400","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:03:58.400","Ascend","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","03:03:58.400","Ascend","Sci Logger sending sample FLBB"]
["$","2022-02-24","03:03:58.400","Ascend","Sending FLBB run command"]
["$","2022-02-24","03:03:58.500","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:03:58.500","Ascend","Sending radiometer pollSample"]
["$","2022-02-24","03:03:59.100","Ascend","Checking Global Issues."]
["$","2022-02-24","03:04:00.100","Ascend","Checking Global Issues."]
["$","2022-02-24","03:04:00.300","Ascend","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",2.7E-2,2.52E-2,8.0999999999999996E-3,0.21679999999999999]
["$","2022-02-24","03:04:00.300","Ascend","Radiometer post: SATFI40545",2.7E-2,2.52E-2,8.0999999999999996E-3,0.21679999999999999]
["$","2022-02-24","03:04:00.300","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    4.70, 11.5688, 33.4956  "]
["$","2022-02-24","03:04:00.300","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:04:00.300","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:04:00.300","Ascend","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","03:04:00.400","Ascend","Setting MSC time and CTD Values: 1645671840,33.50,11.569,4.70"]
["$","2022-02-24","03:04:00.400","Ascend","SciLogger: Starting PHandNO3 sequence"]
["$","2022-02-24","03:04:00.400","Ascend","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","03:04:00.400","Ascend","[MSC] Starting ISUS Sample"]
["$","2022-02-24","03:04:00.400","Ascend","[MSC] TX: W"]
["$","2022-02-24","03:04:00.400"]
["$","2022-02-24","03:04:00.400","Ascend","BE::sendJV: -48691"]
["$","2022-02-24","03:04:00.500","Ascend","Vel PID Values",4.7,52.373660000000001,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.3332999999999995E-2,7.4373999999999996E-2,1.7000000000000001E-4,2.9725999999999999E-2,5.94374,5.94374,48691,1]
["$","2022-02-24","03:04:00.300","Ascend","SBE41 Message",4.7,52.373660000000001,32.15,155.5,null,null,null,null,null,null,null,null,"    4.70, 11.5688, 33.4956  ",4.7,5.8189679999999999,7.5305999999999998E-2,7.3332999999999995E-2,7.6666999999999999E-2,0.21213000000000001,3000]
["$","2022-02-24","03:04:00.300","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    4.47, 11.5689, 33.4935  "]
["$","2022-02-24","03:04:00.700","Ascend","BE::sendJV: -48530"]
["$","2022-02-24","03:04:00.800","Ascend","Vel PID Values",4.47,52.368822999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.6666999999999999E-2,7.4551000000000006E-2,1.7699999999999999E-4,2.9846999999999999E-2,5.9241570000000001,5.9241570000000001,48530,1]
["$","2022-02-24","03:04:00.300","Ascend","SBE41 Message",4.47,52.368822999999999,32.15,155.5,null,null,null,null,null,null,null,null,"    4.47, 11.5689, 33.4935  ",4.47,5.5912940000000004,7.5513999999999998E-2,7.6666999999999999E-2,7.4999999999999997E-2,0.21293799999999999,3000]
["$","2022-02-24","03:04:00.300","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,253.293,11.562,34.084,33.392,42.331,8.939,750.2,662.2,410.5  "]
["$","2022-02-24","03:04:00.900","Ascend","Optode post: 4330,2707,253.293,11.562,34.084,33.392,42.331,8.939,750.2,662.2,410.5  "]

{"sheet":"Single Ascend Science Sample","index":3,"n_rows":235,"n_cols":52,"rows_kept":235,"cut":false,"hidden":false,"merged":[]}
["$","Date","Time","State","Comment","Pressure","BelPos","PumpVolts","PumpMilliamps","PumpoCoulombs","PumpJoules","PumpMotor","HotelVolts","HotelMilliamps","HotelCoulombs","HotelJoules","CTDTemp","CTDSal","RawPress","LPFPress","LPFVel","DiffVel","Diff2 Vel","SlopeLPFPress.","CTDSamplePeriod","LPS331Press","LPS331Temp","SHT21Humid","SHT21Temp","pidSP","pidPV","pidY1","pidY2","pidI","pid_v","pid_u","pid_uCPS","pid_h","FLBB","Topt","Tphase","Rphase","NO3","pHVrs","OCRtext","OCRCh1","OCRCh2","OCRCh3","OCRCH4","GPS","IridModem","MSC"]
["$","2022-02-24","03:03:35.400","Ascend","Starting New SciLogger Sample Cycle"]
["$","2022-02-24","03:03:35.400","Ascend","Sci Logger sending sample Optode"]
["$","2022-02-24","03:03:35.400","Ascend","Sending Optode Do Sample"]
["$","2022-02-24","03:03:35.400","Ascend","Sci Logger set wait for CTD then sample pH and NO3 true"]
["$","2022-02-24","03:03:35.400","Ascend","Sci Logger sending sample FLBB"]
["$","2022-02-24","03:03:35.500","Ascend","Sending FLBB run command"]
["$","2022-02-24","03:03:35.500","Ascend","Sci Logger sending sample Radiometer"]
["$","2022-02-24","03:03:35.500","Ascend","Sending radiometer pollSample"]
["$","2022-02-24","03:03:36","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:37","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:37.300","Ascend","Radiometer Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATFI40545",2.2200000000000001E-2,2.3900000000000001E-2,1.03E-2,0.21529999999999999]
["$","2022-02-24","03:03:37.400","Ascend","Radiometer post: SATFI40545",2.2200000000000001E-2,2.3900000000000001E-2,1.03E-2,0.21529999999999999]
["$","2022-02-24","03:03:37.300","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    9.78, 11.5682, 33.4946  "]
["$","2022-02-24","03:03:37.400","Ascend","SciLogger: Setting get NO3 true"]
["$","2022-02-24","03:03:37.400","Ascend","SciLogger: Setting get PH true"]
["$","2022-02-24","03:03:37.400","Ascend","SciLogger: Setting MSC CTD values"]
["$","2022-02-24","03:03:37.400","Ascend","Setting MSC time and CTD Values: 1645671817,33.49,11.568,9.78"]
["$","2022-02-24","03:03:37.400","Ascend","SciLogger: Starting PHandNO3 sequence"]
["$","2022-02-24","03:03:37.500","Ascend","[MSC] Starting PH and NO3 Sample Sequence, using T1/T2"]
["$","2022-02-24","03:03:37.500","Ascend","[MSC] Starting ISUS Sample"]
["$","2022-02-24","03:03:37.500","Ascend","[MSC] TX: W"]
["$","2022-02-24","03:03:37.500"]
["$","2022-02-24","03:03:37.500","Ascend","BE::sendJV: -51233"]
["$","2022-02-24","03:03:37.600","Ascend","Vel PID Values",9.7799999999999994,52.981067000000003,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.0000000000000007E-2,6.8822999999999995E-2,3.3399999999999999E-4,2.6839999999999999E-2,6.2540570000000004,6.2540570000000004,51233,1]
["$","2022-02-24","03:03:37.300","Ascend","SBE41 Message",9.7799999999999994,52.981067000000003,32.15,155.5,null,null,null,null,null,null,null,null,"    9.78, 11.5682, 33.4946  ",9.7799999999999994,10.856546,6.9323999999999997E-2,7.0000000000000007E-2,7.3332999999999995E-2,0.19777,3000]
["$","2022-02-24","03:03:37.300","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    9.58, 11.5677, 33.4944  "]
["$","2022-02-24","03:03:37.700","Ascend","BE::sendJV: -51704"]
["$","2022-02-24","03:03:37.800","Ascend","Vel PID Values",9.58,52.970896000000003,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,6.9060999999999997E-2,2.3800000000000001E-4,2.6969E-2,6.3115370000000004,6.3115370000000004,51704,1]
["$","2022-02-24","03:03:37.300","Ascend","SBE41 Message",9.58,52.970896000000003,32.15,155.5,null,null,null,null,null,null,null,null,"    9.58, 11.5677, 33.4944  ",9.58,10.64748,6.9327E-2,6.6667000000000004E-2,6.8333000000000005E-2,0.19803100000000001,3000]
["$","2022-02-24","03:03:37.300","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4330,2707,238.796,11.525,34.821,34.129,43.064,8.935,772.3,662.9,411.7  "]
["$","2022-02-24","03:03:38","Ascend","Optode post: 4330,2707,238.796,11.525,34.821,34.129,43.064,8.935,772.3,662.9,411.7  "]
["$","2022-02-24","03:03:37.300","Ascend","Optode Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"#  "]
["$","2022-02-24","03:03:38","Ascend","FLBB Message",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"/99/99,99:99:99,695,521,700,957,545  "]
["$","2022-02-24","03:03:38","Ascend","FLBB post: /99/99,99:99:99,695,521,700,957,545  "]
["$","2022-02-24","03:03:37.600","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:37.600","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:37.600","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51233;"]
["$","2022-02-24","03:03:37.600","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:37.600","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:37.600","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:38.200","Ascend","[MSC] RX: ACK  "]
["$","2022-02-24","03:03:37.800","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:37.800","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:37.800","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51704;"]
["$","2022-02-24","03:03:37.800","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:37.800","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:37.800","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:38.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    9.35, 11.5671, 33.4951  "]
["$","2022-02-24","03:03:38.300","Ascend","BE::sendJV: -50959"]
["$","2022-02-24","03:03:38.400","Ascend","Vel PID Values",9.35,52.966500000000003,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.6666999999999999E-2,6.9379999999999997E-2,3.2000000000000003E-4,2.7098000000000001E-2,6.2206760000000001,6.2206760000000001,50959,1]
["$","2022-02-24","03:03:38.100","Ascend","SBE41 Message",9.35,52.966500000000003,32.15,155.5,null,null,null,null,null,null,null,null,"    9.35, 11.5671, 33.4951  ",9.35,10.434533999999999,6.9420999999999997E-2,7.6666999999999999E-2,7.1666999999999995E-2,0.19850899999999999,3000]
["$","2022-02-24","03:03:38.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:38.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:38.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-50959;"]
["$","2022-02-24","03:03:38.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:38.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:38.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:38.600","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:38.600","Ascend","[MSC] TX: T1,1645671817,11.5682,33.4946,9.7800"]
["$","2022-02-24","03:03:39.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    9.14, 11.5677, 33.4981  "]
["$","2022-02-24","03:03:39.100","Ascend","BE::sendJV: -51093"]
["$","2022-02-24","03:03:39.200","Ascend","Vel PID Values",9.14,52.915267,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.0000000000000007E-2,6.9653000000000007E-2,2.72E-4,2.7227000000000001E-2,6.2370330000000003,6.2370330000000003,51093,1]
["$","2022-02-24","03:03:39.100","Ascend","SBE41 Message",9.14,52.915267,32.15,155.5,null,null,null,null,null,null,null,null,"    9.14, 11.5677, 33.4981  ",9.14,10.217411,6.9681000000000007E-2,7.0000000000000007E-2,7.3332999999999995E-2,0.19902900000000001,3000]
["$","2022-02-24","03:03:39.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:39.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:39.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51093;"]
["$","2022-02-24","03:03:39.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:39.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:39.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:39.600","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:40.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    8.94, 11.5677, 33.4953  "]
["$","2022-02-24","03:03:40.100","Ascend","BE::sendJV: -51623"]
["$","2022-02-24","03:03:40.200","Ascend","Vel PID Values",8.94,52.907505999999998,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,6.9827E-2,1.74E-4,2.7355000000000001E-2,6.3016639999999997,6.3016639999999997,51623,1]
["$","2022-02-24","03:03:40.100","Ascend","SBE41 Message",8.94,52.907505999999998,32.15,155.5,null,null,null,null,null,null,null,null,"    8.94, 11.5677, 33.4953  ",8.94,9.9995899999999995,6.9969000000000003E-2,6.6667000000000004E-2,6.8333000000000005E-2,0.19955400000000001,3000]
["$","2022-02-24","03:03:40.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:40.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:40.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51623;"]
["$","2022-02-24","03:03:40.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:40.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:40.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:40.600","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:41.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    8.73, 11.5681, 33.4931  "]
["$","2022-02-24","03:03:41.100","Ascend","BE::sendJV: -51716"]
["$","2022-02-24","03:03:41.200","Ascend","Vel PID Values",8.73,52.870530000000002,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.0000000000000007E-2,6.9972999999999994E-2,1.46E-4,2.7483E-2,6.313008,6.313008,51716,1]
["$","2022-02-24","03:03:41.100","Ascend","SBE41 Message",8.73,52.870530000000002,32.15,155.5,null,null,null,null,null,null,null,null,"    8.73, 11.5681, 33.4931  ",8.73,9.7839700000000001,7.0157999999999998E-2,7.0000000000000007E-2,6.8333000000000005E-2,0.20011699999999999,3000]
["$","2022-02-24","03:03:41.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:41.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:41.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51716;"]
["$","2022-02-24","03:03:41.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:41.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:41.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:41.600","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:42.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    8.50, 11.5665, 33.4959  "]
["$","2022-02-24","03:03:42.100","Ascend","BE::sendJV: -51020"]
["$","2022-02-24","03:03:42.200","Ascend","Vel PID Values",8.5,52.846943000000003,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.6666999999999999E-2,7.0202000000000001E-2,2.2900000000000001E-4,2.7611E-2,6.2280319999999998,6.2280319999999998,51020,1]
["$","2022-02-24","03:03:42.100","Ascend","SBE41 Message",8.5,52.846943000000003,32.15,155.5,null,null,null,null,null,null,null,null,"    8.50, 11.5665, 33.4959  ",8.5,9.5701660000000004,7.0278999999999994E-2,7.6666999999999999E-2,7.3332999999999995E-2,0.200682,3000]
["$","2022-02-24","03:03:42.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:42.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:42.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51020;"]
["$","2022-02-24","03:03:42.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:42.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:42.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:42.600","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:42.600","Ascend","System Data (dBar %full Volts mAmps): ",8.5,52.824891000000001,32.075000000000003,220,477.58809200000002,67695.705979999999,null,32.075000000000003,421,1387.89906,6769.4497179999998,null,null,null,null,null,null,null,null,null,1228.3000489999999,12.15,37.807999000000002,12.15]
["$","2022-02-24","03:03:42.700","Ascend","Pump motor not faulted"]
["$","2022-02-24","03:03:44.100","Ascend","getting Elmo acceleration limit"]
["$","2022-02-24","03:03:44.100","Ascend","getting Elmo deacceleration limit"]
["$","2022-02-24","03:03:42.700","Ascend","Twitter msg",null,null,null,null,null,null,"VX;"]
["$","2022-02-24","03:03:42.700","Ascend","Twitter msg",null,null,null,null,null,null,"-52994;"]
["$","2022-02-24","03:03:42.900","Ascend","Twitter msg",null,null,null,null,null,null,"ID;"]
["$","2022-02-24","03:03:42.900","Ascend","Twitter msg",null,null,null,null,null,null,"0.03581;"]
["$","2022-02-24","03:03:43.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    8.30, 11.5670, 33.4956  "]
["$","2022-02-24","03:03:44.300","Ascend","BE::sendJV: -51586"]
["$","2022-02-24","03:03:44.400","Ascend","Vel PID Values",8.3000000000000007,52.831870000000002,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,6.6667000000000004E-2,7.0332000000000006E-2,1.2999999999999999E-4,2.7737999999999999E-2,6.2971890000000004,6.2971890000000004,51586,1]
["$","2022-02-24","03:03:43.100","Ascend","SBE41 Message",8.3000000000000007,52.831870000000002,32.15,155.5,null,null,null,null,null,null,null,null,"    8.30, 11.5670, 33.4956  ",8.3000000000000007,9.3571989999999996,7.041E-2,6.6667000000000004E-2,7.1666999999999995E-2,0.20124600000000001,3000]
["$","2022-02-24","03:03:43.100","Ascend","Twitter msg",null,null,null,null,null,null,"IQ;"]
["$","2022-02-24","03:03:43.100","Ascend","Twitter msg",null,null,null,null,null,null,"-3.27291;"]
["$","2022-02-24","03:03:43.300","Ascend","Twitter msg",null,null,null,null,null,null,"SR;"]
["$","2022-02-24","03:03:43.300","Ascend","Twitter msg",null,null,null,null,null,null,"113296144;"]
["$","2022-02-24","03:03:43.500","Ascend","Twitter msg",null,null,null,null,null,null,"CL[1];"]
["$","2022-02-24","03:03:43.500","Ascend","Twitter msg",null,null,null,null,null,null,"4.76000;"]
["$","2022-02-24","03:03:43.700","Ascend","Twitter msg",null,null,null,null,null,null,"PL[1];"]
["$","2022-02-24","03:03:43.700","Ascend","Twitter msg",null,null,null,null,null,null,"13.50000;"]
["$","2022-02-24","03:03:43.900","Ascend","Twitter msg",null,null,null,null,null,null,"PL[2];"]
["$","2022-02-24","03:03:43.900","Ascend","Twitter msg",null,null,null,null,null,null,"3.00000;"]
["$","2022-02-24","03:03:44.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    8.08, 11.5665, 33.4954  "]
["$","2022-02-24","03:03:44.700","Ascend","BE::sendJV: -51316"]
["$","2022-02-24","03:03:44.800","Ascend","Vel PID Values",8.08,52.782916,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.3332999999999995E-2,7.0486999999999994E-2,1.56E-4,2.7865999999999998E-2,6.2642319999999998,6.2642319999999998,51316,1]
["$","2022-02-24","03:03:44.100","Ascend","SBE41 Message",8.08,52.782916,32.15,155.5,null,null,null,null,null,null,null,null,"    8.08, 11.5665, 33.4954  ",8.08,9.1454570000000004,7.0548E-2,7.3332999999999995E-2,7.0000000000000007E-2,0.20180899999999999,3000]
["$","2022-02-24","03:03:44.100","Ascend","Twitter msg",null,null,null,null,null,null,"AC;"]
["$","2022-02-24","03:03:44.100","Ascend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","03:03:44.100","Ascend","Twitter msg",null,null,null,null,null,null,"DC;"]
["$","2022-02-24","03:03:44.100","Ascend","Twitter msg",null,null,null,null,null,null,"1000000000;"]
["$","2022-02-24","03:03:44.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:44.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:44.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51586;"]
["$","2022-02-24","03:03:44.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:44.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:44.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:44.700","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:44.700","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:44.700","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51316;"]
["$","2022-02-24","03:03:44.700","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:44.700","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:44.700","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:45.100","Ascend","[MSC] RX: 0x608D,A,02/24/2022 03:03:49,1645671817,9.78,11.5682,33.4946,64,6,0,0,13.03,37.80,11.500,5.638e-01,17668.00,1049.00,1020.27,5.09,33.49,18.04,8.189e-04,36,77,2AA22F78332735B9371437933789370F367235E13584356F35CF367E37B5395D3B853E3C415644F348EB4D2F518F55F25A315DE8611B635B649164AB638261685E6D5AB2569A52794E604A6746ED43B140E23E73,928.6  "]
["$","2022-02-24","03:03:45.200","Ascend","[MSC] Data: 0x608D,A,02/24/2022 03:03:49,1645671817,9.78,11.5682,33.4946,64,6,0,0,13.03,37.80,11.500,5.638e-01,17668.00,1049.00,1020.27,5.09,33.49,18.04,8.189e-04,36,77,2AA22F78332735B9371437933789370F367235E13584356F35CF367E37B5395D3B853E3C415644F348EB4D2F518F55F25A315DE8611B635B649164AB638261685E6D5AB2569A52794E604A6746ED43B140E23E73,928.6  "]
["$","2022-02-24","03:03:45.200","Ascend","[MSC] Post NO3: 18.04"]
["$","2022-02-24","03:03:45.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    7.86, 11.5666, 33.4968  "]
["$","2022-02-24","03:03:45.300","Ascend","BE::sendJV: -51081"]
["$","2022-02-24","03:03:45.400","Ascend","Vel PID Values",7.86,52.76585,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.3332999999999995E-2,7.0662000000000003E-2,1.74E-4,2.7993000000000001E-2,6.2355510000000001,6.2355510000000001,51081,1]
["$","2022-02-24","03:03:45.100","Ascend","SBE41 Message",7.86,52.76585,32.15,155.5,null,null,null,null,null,null,null,null,"    7.86, 11.5666, 33.4968  ",7.86,8.9345130000000008,7.0624999999999993E-2,7.3332999999999995E-2,7.3332999999999995E-2,0.202372,3000]
["$","2022-02-24","03:03:45.300","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:45.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:45.300","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51081;"]
["$","2022-02-24","03:03:45.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:45.300","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:45.300","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:45.500","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:45.600","Ascend","[MSC] Done Sampling."]
["$","2022-02-24","03:03:45.600","Ascend","[MSC] Starting pH sample"]
["$","2022-02-24","03:03:45.600","Ascend","[MSC] TX: W"]
["$","2022-02-24","03:03:45.800","Ascend","[MSC] RX: ACK  "]
["$","2022-02-24","03:03:45.800","Ascend","[MSC] TX: T2,1645671817,11.5682,33.4946,9.7800"]
["$","2022-02-24","03:03:46.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    7.65, 11.5678, 33.4950  "]
["$","2022-02-24","03:03:46.100","Ascend","BE::sendJV: -51273"]
["$","2022-02-24","03:03:46.200","Ascend","Vel PID Values",7.65,52.738669999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.0000000000000007E-2,7.0793999999999996E-2,1.3200000000000001E-4,2.8119000000000002E-2,6.2589319999999997,6.2589319999999997,51273,1]
["$","2022-02-24","03:03:46.100","Ascend","SBE41 Message",7.65,52.738669999999999,32.15,155.5,null,null,null,null,null,null,null,null,"    7.65, 11.5678, 33.4950  ",7.65,8.7225190000000001,7.0584999999999995E-2,7.0000000000000007E-2,7.1666999999999995E-2,0.20296400000000001,3000]
["$","2022-02-24","03:03:46.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:46.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:46.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51273;"]
["$","2022-02-24","03:03:46.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:46.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:46.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:46.500","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:47.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    7.44, 11.5674, 33.4957  "]
["$","2022-02-24","03:03:47.100","Ascend","BE::sendJV: -51453"]
["$","2022-02-24","03:03:47.200","Ascend","Vel PID Values",7.44,52.722003000000001,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.0000000000000007E-2,7.0888999999999994E-2,9.5000000000000005E-5,2.8246E-2,6.2808909999999996,6.2808909999999996,51453,1]
["$","2022-02-24","03:03:47.100","Ascend","SBE41 Message",7.44,52.722003000000001,32.15,155.5,null,null,null,null,null,null,null,null,"    7.44, 11.5674, 33.4957  ",7.44,8.508794,7.0444999999999994E-2,7.0000000000000007E-2,7.0000000000000007E-2,0.20363400000000001,3000]
["$","2022-02-24","03:03:47.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:47.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:47.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-51453;"]
["$","2022-02-24","03:03:47.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:47.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:47.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:47.500","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:48","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    7.19, 11.5668, 33.4951  "]
["$","2022-02-24","03:03:48.100","Ascend","BE::sendJV: -50044"]
["$","2022-02-24","03:03:48.200","Ascend","Vel PID Values",7.19,52.701217,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,8.3333000000000004E-2,7.1170999999999998E-2,2.8200000000000002E-4,2.8372000000000001E-2,6.1089770000000003,6.1089770000000003,50044,1]
["$","2022-02-24","03:03:48","Ascend","SBE41 Message",7.19,52.701217,32.15,155.5,null,null,null,null,null,null,null,null,"    7.19, 11.5668, 33.4951  ",7.19,8.2941520000000004,7.0314000000000002E-2,8.3333000000000004E-2,7.6666999999999999E-2,0.20433999999999999,3000]
["$","2022-02-24","03:03:48.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:48.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:48.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-50044;"]
["$","2022-02-24","03:03:48.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:48.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:48.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:48.500","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:49","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    6.96, 11.5670, 33.4961  "]
["$","2022-02-24","03:03:49.100","Ascend","BE::sendJV: -49578"]
["$","2022-02-24","03:03:49.200","Ascend","Vel PID Values",6.96,52.660350999999999,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.6666999999999999E-2,7.1492E-2,3.21E-4,2.8497999999999999E-2,6.052009,6.052009,49578,1]
["$","2022-02-24","03:03:49","Ascend","SBE41 Message",6.96,52.660350999999999,32.15,155.5,null,null,null,null,null,null,null,null,"    6.96, 11.5670, 33.4961  ",6.96,8.0791229999999992,7.0290000000000005E-2,7.6666999999999999E-2,0.08,0.205071,3000]
["$","2022-02-24","03:03:49.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:49.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:49.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-49578;"]
["$","2022-02-24","03:03:49.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:49.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:49.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:49.500","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:50.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    6.74, 11.5676, 33.4953  "]
["$","2022-02-24","03:03:50.100","Ascend","BE::sendJV: -49568"]
["$","2022-02-24","03:03:50.200","Ascend","Vel PID Values",6.74,52.646537000000002,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.3332999999999995E-2,7.1785000000000002E-2,2.9399999999999999E-4,2.8622999999999999E-2,6.0508480000000002,6.0508480000000002,49568,1]
["$","2022-02-24","03:03:50.100","Ascend","SBE41 Message",6.74,52.646537000000002,32.15,155.5,null,null,null,null,null,null,null,null,"    6.74, 11.5676, 33.4953  ",6.74,7.8634230000000001,7.0368E-2,7.3332999999999995E-2,7.4999999999999997E-2,0.20579700000000001,3000]
["$","2022-02-24","03:03:50.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:50.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:50.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-49568;"]
["$","2022-02-24","03:03:50.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:50.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:50.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:50.500","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:51.100","Ascend","Unparsed SBE41 Message",null,null,null,null,null,null,null,null,null,null,null,null,"    6.52, 11.5673, 33.4954  "]
["$","2022-02-24","03:03:51.100","Ascend","BE::sendJV: -49575"]
["$","2022-02-24","03:03:51.200","Ascend","Vel PID Values",6.52,52.622165000000003,32.15,155.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,7.3332999999999995E-2,7.2051000000000004E-2,2.6600000000000001E-4,2.8747000000000002E-2,6.0517409999999998,6.0517409999999998,49575,1]
["$","2022-02-24","03:03:51.100","Ascend","SBE41 Message",6.52,52.622165000000003,32.15,155.5,null,null,null,null,null,null,null,null,"    6.52, 11.5673, 33.4954  ",6.52,7.645486,7.0572999999999997E-2,7.3332999999999995E-2,7.3332999999999995E-2,0.206515,3000]
["$","2022-02-24","03:03:51.100","Ascend","Twitter msg",null,null,null,null,null,null,"MO=1;"]
["$","2022-02-24","03:03:51.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:51.100","Ascend","Twitter msg",null,null,null,null,null,null,"JV=-49575;"]
["$","2022-02-24","03:03:51.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:51.100","Ascend","Twitter msg",null,null,null,null,null,null,"BG;"]
["$","2022-02-24","03:03:51.100","Ascend","Twitter msg",null,null,null,null,null,null,";"]
["$","2022-02-24","03:03:51.500","Ascend","Checking Global Issues."]
["$","2022-02-24","03:03:52","Ascend","[MSC] RX: 0x565A,pH,02/24/2022 03:03:58,1645671817,9.78,11.5682,33.4946,64,6,0,13.04,37.80,11.672,4.560e-02,7.1234,3.552,-0.952346,0.000019,-0.914515,0.000016,+4.484e-09,+3.760e-09  "]
["$","2022-02-24","03:03:52","Ascend","[MSC] Data: 0x565A,pH,02/24/2022 03:03:58,1645671817,9.78,11.5682,33.4946,64,6,0,13.04,37.80,11.672,4.560e-02,7.1234,3.552,-0.952346,0.000019,-0.914515,0.000016,+4.484e-09,+3.760e-09  "]
["$","2022-02-24","03:03:52.100","Ascend","Everything posted, writing sample"]
["$","2022-02-24","03:03:52.100","Ascend","Wrote to msg file: AscendPt:,2022-Feb-24T03:03:35Z,9.78,11.5682,33.495,11.525,34.129,8.935,-0.952346,18.04,521,957,545,0.0222,0.0239,0.0103,0.2153  "]