APR17 changes to BOG CPF 2

Motherboard:

Replace R20 and R21 with WSLG-.007CT-ND.


Daughter card SN2:

Remove U6, U10, U15, U2, U7, U12



Daughter card SN3:

Remove U6, U10, U15, U2, U7, U12
Replace Q1 with IRFR7440TRPBFCT-ND
Replace R21 with WSLG-.02CT-ND



Daughter card SN4:
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Remove U6, U10, U15
Replace Q2 with IRFR7440TRPBFCT-ND
Replace R43 with WSLG-.02CT-ND


