1. [bookmark: _GoBack]Goal 1: Make sure we can deploy he MR safely and can run the standard MR processing scripts
1.1. Oct 8: Deployment 1
1.1.1.  Depth 105 meters
1.1.2.  Anchor on the bottom
1.1.3.  5 profiles 
1.1.4. Microrider mounted with 2 probes
1.2. Science Analysis
1.2.1.  Verify the noise characteristics of the SBE41 pressure sensor
1.2.2.  More
2. Goal 2:  Determine the safe mission duration (2 deployments)
2.1. Week of Oct 11-15 and one more in the same week of the next week: 
2.2. Same as above with max profiles
3. Goal 3: Verify parking capability (1 deployment) 
3.1. Park at 90 meters in 105 meters of water
3.2. 5 profiles
4. Goal 4: Verify parking capability with max mission duration ( 1-2 deployments)
4.1. Park at 90 meters in 105 meters of water
4.2. Max profiles
5. Goal 5: Verify max depth capability
5.1. In parallel with 1-4 Gene will review calcs and potentially pressure test a spare housing
5.2. No MR.  1 profile parking at 150 meters in 175 – 250 meters of water
5.3. Check internal humidity and pressure and whatever else makes sense.  Maybe recover an inspect
5.4. Repeat 5.1-5.3 at 200 and 250 meter parking depths.
6. 1 day of  profiles at M1
7. Max number of profiles at M1 parking at 250 meters 2-3 deployments



