CPF Deployment plan
1. Define deployment date, location and duration (Jacki/Joseph)
a. Coordinate pre-cruise with Jared
2. Engineering verification ready for deployment (Gene/Eric)
a. Engineering makes sure that CPF has the right software loaded and it works.
3. Science verification ready for deployment (Jacki/Joseph)
a. Make sure the charge cycle is complete.
4. Stage for Jared (Jacki/Joseph)
a. Put the CPF on the deployment cart and roll it to wherever we agree the transfer point is (high bay, dock house, ???).
b. Verify the CPF passes its pre-deployment check.
c. Power down the CPF
5. Load on the Paragon (Jared and crew)
a. Repeat pre-deployment check
6. Deploy (Jared and crew)
a. When the CPF is submerged, send CPF deployment e-mail alias time and lat/lon.
7. Monitor deployment (Jacki/Joseph) 
a. Need to designate specific responsible individual (and team if necessary)
b. Note: Matlab scripts exist to process the SBD e-mails and create data summaries and KML files for Google Earth.  And we’re working on a web page to do the same thing.
8. Recover (Jared and crew)
a. [bookmark: _GoBack]Unload and let Jacki/Joseph know
9. Get the CPF (Joseph/Jacki)
a. Put it on the charger
10. Download the data (Joseph/Jacki)
a. Notify the data consumption team (Joseph/Jacki)
11. Review the data and agree on code changes if any (All)
