CPF-P2 Deployment check list				Date:

1.0  Software checks
___________Clear breakpoints				______Comment out compiler directives

2.0  Mission configuration
_____________Bellows upper/lower limit		________________Park hours/minutes  
_____________Surface ops bellows position	________________Recovery mode BP
_____________parkdepth 				________________maxPressure
_____________maxProfiles				________________maxDays/Hours
_____________Pre mission delay TO			________________Surface ops TO
_____________Descend TO				________________Park TO
_____________Anchor TO				________________Ascend TO
_____________Number of SBD retries		________________ Homer ID

3.0  Pre-Deployment Mechanical
_____Receive SBD message				_____Receive  GPS tracker message
_____Double check lifting bridle			_____Remove Optode  cover
_____Remove CTD caps					_____Remove FLBB cover
_____Connector dummy plugs installed		_____Remove GPS tracker off magnet
___________________Number of ballast bars	_________________Battery bus voltage
___________________Humidity/Temp.		_________________Int. pressure/Temp.
_____Remove Telonics magnet/Frequency (160.12210 MHz)
[bookmark: _GoBack]_____Remove ISUS cover
 
4.0  Deployment
__________________Mission start time		__________________Over the side time
__________________Deployment lat.		__________________Deployment long.
__________________AB retract fast start time	__________________ Descend time
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