CPF-P2 Deployment check list				Date:
User: 
Mission Statement:

1.0  Software Engineering Cchecks [footnoteRef:1] [1:  Gene or Eric] 

_____ Clear breakpoints					_____	Comment out compiler directives

2.0  Mission Cconfiguration (i.e., Creating Mission)
3.0 GM print out___Bellows upper/lower limit				Anchor/Park hours:minutes  
4.0 GM print out___Surface ops bellows position	GM print out____Recovery mode BP
_____________ Mission TimeOut (HH:MM)		_____________ Park Sample Period (HH:MM) 

_____________park depth 				________________max Pressure
_____________maxProfiles				________________max Days:Hours_____________ Max Profiles				_____________ Max Pressure (m)
_____________ Park Depth (Ascend Table)		_____________ Ascend Glide Depth*	
_____________ Platform Velocity Descend		_____________ Platform Velocity Ascend
_____________ Park/Anchor Time (HH:MM, Descend Table) 
_____________ Estimated Surfacing Time (HH:MM) 
_____________ GM print out__Pre- mission Mission Ddelay TimeOut*			_____________ GM print out_____Surface ops Ops TO*
_____________ GM print out__Descend TimeOut* 			_____________ GM print out_____Park TO*
_____________ GM print out__Anchor TimeOut*O				_____________ GM print out_____Ascend TO*
________________ Homer ID
________________ Park/Anchor Sample Period

_____________ Can Humidity (% RH)			_____________ Can Pressure (mbar)
_____________ Battery Bus Voltage (V)		_____________ Battery Bus Current (mA)
_____________ Bellows Position Limits*[endnoteRef:1]		_____________ Number of Ballast Bars*	  [1:  To Be Printed Out] 

_____________ SurfaceOps Bellows Position	_____________ RecoveryMode Bellows Position

5.0  Pre-Deployment
_____Receive SBD message				if mounted______Receive  GPS Ttracker  mMessage (if mounted)
_____Double check lifting bridle			_____Remove Optode  cover
_____Remove CTD caps					_____Remove FLBB cover
_____Remove ISUS cover				_____Connector dummy plugs installed

_____Connector dummy plugs installed		_____Remove GPS tracker off magnet
Gene to count__Number of ballast bars	           _________________Battery bus voltage
___________________Humidity/Temp.		_________________Int. pressure/Temp.
_____Remove Telonics Mmagnet /Frequency (Freq 160.154000MHz) 

_____Homer Beacon (ID 13 (07-1))


 
6.0  Deployment
__________________ __________________Water Depth (m)  		__________________ Over the side Ttime (LT)
__________________ __________________Mission Sstart Ttime (On)		__________________ Under Surface Ttime (LT)      
__________________ ___________Profile Sstart Ttime ($GO)	__________________ Descend Time (LT)
__________________ __________________Deployment lat.Lat (underUnder)		__________________________________ Deployment longLon . (underUnder)
)	__________________ Descend time

FORM ON BACK FOR SUBSEQUENT DIVES FROM STARTING PROFILE:

	Profile #
	Under Time
	Lat/Lon Under
	Surface Time
	Lat/Lon Surface
	Surfac
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