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	TO:
	Gene Massion
	COMPANY:
	MBARI


	FROM:
	Steven S. Thumbeck
	FAX #:
	831-775-1646


	DATE:
	September 7, 2001
	REF. #:
	


	SUBJECT:
	Revised Connector Quote 


FAX MESSAGE:

Ocean Design, Inc. 

- Quotation #5412 Rev A -

Gene,  

Attached is the revised quotation you requested.

Notes:

· This revised proposal includes changes and clarifications as identified in the SB cable specification and cable block diagram sent.

· We may install the electro-optical termination at any location.  We would need a clean dry working space for assembly.  We could estimate that it will take two technicians one day to install each termination.  We have included a copy of our field installation rates for your reference.  Basically, we charge at our cost +15% for travel expenses.  It is difficult to tell how long we may need to wait before we may install the equipment so when budgeting a few extra stand-by days should be included.

· For a cable termination we will qualify the termination to an actual sample of cable at our pressure test facility.  This qualification ensures that we will have no troubles on site during installation. 

· Orders in excess of $100,000.00 will follow a milestone payment schedule (included on page 2)

Thank you for the opportunity to provide this quotation.  Please call me if you have any additional questions or requirements.

Sincerely,

_________________

Steven S. Thumbeck

Inside Sales Manager

cc: Brock Rosenthal – 858-454-5775

ORIGINAL WILL:

	
	FOLLOW VIA MAIL

	
	FOLLOW VIA OVERNIGHT EXPRESS

	(
	NOT BE SENT


- Quotation #5412 Rev A -

Ocean Design is pleased to offer the following quotation:

	Date:
	September 7, 2001

	To:
	MBARI

	Attn:
	Gene Massion

	Re:
	Connector Quote


The following pricing includes Ocean Design’s standard Quality Acceptance testing.

	ITEM
	QTY
	DESCRIPTION
	PRICE

	1
	Lot
	Connectors and Assemblies per Attached Table
	See Table


	Delivery:
	Items: 3,4,5,6,7,8

Delivery 12 Weeks ARO.  A firm cable specification is required at order placement.  To perform production build, the free issue cable is required 6 weeks prior to delivery.

Items: 1&2

Delivery 12-14 Weeks ARO.  A firm cable specification is required at order placement.  To perform qualification build, A 2 meter sample of cable is required 8 weeks prior to delivery.


	Payment Milestone Schedule:
	Milestone 1 – 15% of Contract – Due upon Submission of Outline/Interface & General Assembly Drawings for Customer review.  Drawings will be provided 2-3 weeks from receipt of contract.

Milestone 2 – 35% of Contract – Placement of long lead-time material orders.  4 weeks from receipt of 

Customer approved outline/interface and general assembly drawings.

Balance of Contract -Due upon completion of Factory Acceptance Testing (FAT) on a line Item Basis.


This tender is Ocean Design Quotation #5412 Rev A which is subject to attached Terms and Conditions.

Sincerely,

Steven S. Thumbeck

Inside Sales Manager

 Ocean Design, Inc.

9 Aviator Way

Ormond Beach, FL  32174

TERMS  AND  CONDITION  OF  SALE

General Provisions

By accepting this quotation, Buyer agrees to comply fully with the following terms and conditions, and none of the Buyers Terms and Conditions shall apply.  Acceptance of  the Buyer’s purchase order by  Ocean Design, Inc. shall not constitute agreement to the Buyers terms and conditions.

1. Prices quoted are net prices, Ex-Works, ODI Ormond Beach(INCOTERMS 1990). Quotations are valid for 30 days from the date of quotation.

2. Ocean Design, Inc. is not responsible for typographical errors made in the quotation.

3. Deliveries quoted are ARO, and are based on current workload.  Firm deliveries will be provided to the Buyer within one (1)  week of order placement.

4. Shipping charges, where applicable, will be shown as a separate item on our invoice, and are payable in full with the invoice.

5. Terms are 2% discount if paid within 10 days of date of invoice, net 30 days.   Shipping charges, where applicable, are not subject to this prompt payment discount.

6. Invoices paid after 30 days will be subject to an interest payment of 1.5% per month.

7. The laws of the State of Florida, U.S.A. that are in force at the date of this quotation shall govern the validity, interpretation and performance of these conditions.

8. Except as otherwise stated, Buyer shall release, indemnify, defend and hold Ocean Design, Inc. harmless from all claims, causes of action, liability, expenses and costs (including attorneys fees) for property loss or damage, and personal injury or death arising directly from and in any connection with the performance of Ocean Design, Inc. products.

9. Warranty of Ocean Design, Inc. product is for a period of two (2) years from the date of shipment or one (1) year from the date the product in placed into service, whichever is sooner.  Ocean Design, Inc. shall replace or repair at no charge to the Buyer, any product found to be defective on return of said product to factory.  Determination to repair or replace is at the sole discretion of Ocean Design, Inc.  For field installable assemblies, warranty is valid only where Ocean Design personnel, or personnel suitably qualified and re-validated on an annual basis by Ocean Design, have installed the equipment.

10. Ocean Design, Inc. shall not be held responsible for any consequential loss or damage to Buyer or Buyer’s customer, as a result of defective products, or any costs associated with the recovery of defective product to factory.

11. Contracts which involve field service by Ocean Design, Inc. employees, shall be governed by the above terms and conditions.

12. Ocean Design offers to sell  hardware as described at a fixed price.  Ocean Design will retain all rights to all intellectual, proprietary information, and patented material now held or in the future developed by Ocean Design.  Ocean Design will offer to modify existing designs to suit particular needs of various programs and to prove-out the changes according to proposed test plans.  Ocean Design may provide at the Buyers request general assembly drawings of sufficient detail for the appropriate design to be evaluated.  Furnishing of such drawings does not grant or imply the granting of any rights to the Buyer or any third party in the information contained therein.  All such information remains the sole property of Ocean Design and may be used only for the express purpose for which it has been delivered.

13. Prices are for supply within the 2001 calendar year.  Pricing for supplies beyond this date will be subject to annual adjustment in accordance with an agreed formulae, an example of which is below for 2002:-

PY = PB x {0.25 x MY/MP + 0.75 x LY/LP}

Where:


PY = Price in Year Y


PB = Base Price (2000)

MY= Producer Price Index “Metal & Metal Products” (Commodity Code 10) for (Insert Month)                                                                                   

MP = Producer Price Index “Metal & Metal Products” (Commodity Code 10) for 2000


LY  = Average Hourly Labor Rate for S.I.C. Code 3721 Including Lump Sum for (Insert Month)


LP = Average Hourly Labor Rate for S.I.C. Code 3721 Including Lump Sum for (Insert Month) of 2000

- oOo -
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 Attachment 1 - Field Installation Rates

Effective From 01-Jan-2001 to 31-Dec-2001

ONSHORE

DAY RATE:
Electrical Technician

- $  600 per  (8 hour day or part of)



Senior Elec Technician 
- $  680 per  (8 hour day or part of)



Optical Technician

- $  675 per  (8 hour day or part of)



Senior Optical Technician
- $  750 per  (8 hour day or part of)



Engineer 


- $  850 per  (8 hour day or part of)



Senior Engineer 

- $  925 per  (8 hour day or part of)



Vice President/Director
- $1,100 per  (8 hour day or part of)

OFFSHORE

DAY RATE:
Electrical Technician

- $1,250 per (12 hour day or part of)



Senior Elec Technician 
- $1,325 per (12 hour day or part of)



Optical Technician

- $1,300 per (12 hour day or part of)



Senior Optical Technician
- $1,450 per (12 hour day or part of)



Engineer 


- $1,600 per (12 hour day or part of)



Senior Engineer 

- $1,750 per (12 hour day or part of)



Vice President/Director
- $2,100 per (12 hour day or part of)

TRAVEL:
ACTUAL COST OF:

Air Fare


Rental Car



Hotel




Per Diem







Plus 15%

EMERGENCY CALLOUT PREMIUM:

- $500
(LESS THAN 72 HOURS)
NOTES:
Hours in excess of 8 per day onshore (12 per day offshore) are charged on a pro-rata basis.

	
	
	
	
	Conn/Assy Qtys

	
	No. of MBARI Line
	Unit
	ODI Connector
	Qty Per Line
	TOTAL
	Line Item Unit
	Line Item Extended

	Item
	Items
	
	Part No.
	Item
	QTY
	Price
	Price

	
	
	MBARI Quote 5412 Rev A
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	HYBRID CONNECTORS
	
	
	
	
	

	1
	5
	In-Line Rolling Seal Hybrid ROV Connector Consisting of (Parts Only):
	1
	5
	$15,277 
	$76,385 

	1.1
	5
	4-Optic 2-Electric Flying ROV Connector With Hose Termination; Material Titanium
	1
	5
	
	

	1.2
	5
	4-0ptic / 2-Electric - 10 FT Oil Filled Hose Assembly
	 
	1
	5
	
	

	1.3
	5
	Cable Termination and Splice Chamber for; 6-Way Cable Assembly - Electro-Optical Cable Type (Spec SB-43701 - Kevlar Armor, 316SS K Tube) Material; Titanium (Termination Load Rating 500LB Working Load)
	Customer Supplied Cable
	1
	5
	
	

	
	
	
	
	
	
	
	

	2
	5
	In-Line Rolling Seal Hybrid ROV Connector and Penetrator Consisting of:
	1
	5
	$12,689 
	$63,445 

	2.1
	5
	4-Optic 2-Electric Flanged ROV With Hose Termination; Material Titanium
	1
	5
	
	

	2.2
	5
	4-0ptic / 2-Electric - 10 FT Oil Filled Hose Assembly
	 
	1
	5
	
	

	2.3
	5
	4-Optic 2-Electric Pressure Housing Penetrator With Hose Termination; Material Titanium
	 
	1
	5
	 
	

	
	
	
	
	
	
	
	

	
	
	ELECTRICAL CONNECTORS
	
	
	
	
	

	3
	2
	Nobska Current Meter and SeaBird CT Connections:
	1
	2
	$2,928 
	$5,856 

	3.1
	2
	8-Way Flying ROV Plug (Pins) With PU Molded Termination; Material Titanium
	1
	2
	
	

	3.2
	2
	Free Issue - 8-Way Cable Assembly, Cable (Spec TBD, with Qty 2 RMG-4-FS)
	Customer Supplied Cable
	1
	2
	
	

	
	
	
	
	
	
	
	

	4
	2
	Pressure Housing Mounted Assembly Consisting of:
	1
	2
	$4,992 
	$9,984 

	4.1
	2
	8-Way Flanged ROV Receptacle (Sockets) With Hose Termination; Material Titanium
	1
	2
	
	

	4.2
	2
	8-Electric - 10 FT Oil Filled Hose Assembly
	 
	1
	2
	
	

	4.3
	2
	8-Electric Pressure Housing Penetrator With Hose Termination; Material Titanium
	 
	1
	2
	 
	

	
	
	
	
	
	
	
	

	5
	2
	RDI ADCP Connections:
	
	1
	2
	$2,928 
	$5,856 

	5.1
	2
	8-Way Flying ROV Plug (Pins) With PU Molded Termination; Material Titanium
	1
	2
	
	

	5.2
	2
	Free Issue - 7-Way Cable Assembly, Cable (Spec TBD, with Qty 1 LPMIL-7-FS)
	Customer Supplied Cable
	1
	2
	
	

	
	
	
	
	
	
	
	

	6
	2
	Pressure Housing Mounted Assembly Consisting of:
	1
	2
	$4,992 
	$9,984 

	6.1
	2
	8-Way Flanged ROV Receptacle (Sockets) With Hose Termination; Material Titanium
	1
	2
	
	

	6.2
	2
	7-Electric - 10 FT Oil Filled Hose Assembly
	 
	1
	2
	
	

	6.3
	2
	8-Electric Pressure Housing Penetrator With Hose Termination; Material Titanium
	 
	1
	2
	 
	


	
	
	MBARI Quote 5412 Rev A
	
	
	
	
	

	7
	4
	Mast Mounted Nobska and Battery Housing Connections:
	1
	4
	$2,936 
	$11,744 

	7.1
	4
	4-Way Flying ROV Plug (Pins) With PU Molded Termination; Material Titanium
	1
	4
	
	

	7.2
	4
	Free Issue - 4-Way Cable Assembly, Cable (Spec TBD, with Qty 1 RMG-4-FS)
	Customer Supplied Cable
	1
	4
	
	

	
	
	
	
	
	
	
	

	8
	4
	Pressure Housing Mounted Assembly Consisting of:
	1
	4
	$4,077 
	$16,308 

	8.1
	4
	4-Way Flanged ROV Receptacle (Sockets) With Hose Termination; Material Titanium
	1
	4
	
	

	8.2
	4
	4-Electric - 10 FT Oil Filled Hose Assembly
	 
	1
	4
	
	

	8.3
	4
	4-Electric Pressure Housing Penetrator With Hose Termination; Material Titanium
	 
	1
	4
	 
	

	
	
	
	
	
	
	
	

	
	1
	Production Set - Totals
	
	
	28
	
	$199,562 
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Electrical Only Subsea Connectors – General

The connector(s) supplied shall be specifically designed and qualified for subsea use. Each deliverable connector(s) shall be factory acceptance tested (FAT) as specified in Table 1.  Batch testing is not acceptable.  Each connector shall include a documentation package including all material certifications, material origins and test results.  A Certificate of Conformance (C of C) shall be supplied for each connector.  One copy of the documentation package shall be provided to the buyer at no charge.  The supplier shall retain a documentation package for a minimum period of 20 Years.  At a minimum, the supplier shall meet or exceed all ratings as listed in Table 2. The supplier shall be ISO 9001 registered. 

Quality Conformance - Requirements

Table 1 - Supplier Testing Standards

Hydrostatic Test:

Insulation Resistance: Bench Tests:

Insulation Resistance: Mate/Demate Function:

7,500psi

Pin-Pin & Pin-Gnd 10G( Min @ 1,000Vdc

Pin-Pin & Pin-Gnd 10G( Min @ 1,000Vdc 
1 Cycle Minimum

Table 2 - Standard Specifications 

Physical Characteristics:

Type:



ROV & Stab-Plate Operable





Number of Circuits:

8

Material:


Titanium CP Gr 2

ROV Handle Type:

Flexible Paddle Type

Key Way:


Major - Single

Operational Characteristics: 

Amperage Rating:

30 Amps per circuit

Voltage Rating: 

3.3 KVDC / 2.3 KVAC RMS

Mate/Demate Cycles: 

>1000

Operational Temperature: 
-2°C - +50°C
Storage Temperature: 

-25°C - +60°C
Mating Force:


<5 lbs. Force per circuit

Design Characteristics: 

Contact Resistance:

<0.01 Ohms per circuit 

Design Life:


25 years
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PROJECT/ACCOUNT CHARGE NUMBER:

200126-5330

199,562.00

      

 

SALE/USE TAX

7.0%

13,969.34

        

 

REMARKS:

100.00

             

 

213,631.34

$    

 

APPROVAL:

DATE:

Form Revised  04/13/01





Net 30





Steven Thumbeck

Gene Massion





831 7751922

SHIPPING

TOTAL

SUBTOTAL









MBARI is an Affirmative Action/Equal Employment Opportunity employer. MBARI does not discriminate against any employee or applicant for employment 

becauseof race, color, religion, sex or national origin. MBARI takes affirmative action to ensure that applicants are employed, and that employees are treated 

during employment, without regard to their race, color, religion, sex or national origin. MBARI will comply with the provisions of Executive Order 11246 of 

9/24/65, and relevant rules and regulations as required by law. Please be advised that all contractors and subcontractors having 50 or more employees and a 

federal government contract or subcontract of $50,000 or more must develop a written affirmative action plan under the federal guidelines.



























Items 3.1, 5.1, 7.1, 1.1 to have 45 degree, extended length

UNIT PRICE

$199,562.00







Connector/cable assemblies per

ODI Quotation #5412 Rev A and

MBARI drawing  #101324SCD





1.1, 1.2, 1.3 may have extended delivery time, please advise best estimate.

strain relief.  Design to be approved by MBARI before fabrication

Item 1.3 molded strain relief design to be approved by MBARI before fab.

All items except 1.1, 1.2, 1.3 are required by the end of November 2001.  Items



PO-0102893

10/5/2001



9 Aviator Way

Ocean Design, Inc



Ormond Beah, FL 32174

904 6753575

DESCRIPTION


Table 2 - Standard Specifications Physical Characteristics:
Type:
ROV Operable

Number of Circuits:
8

Material:
Titanium CP Gr2
ROV Handle Type:
Flexible Paddle Type

Key Way:
Major – Single

Electric/Optic (Hybrid) Connectors – General

The connector(s) supplied shall be specifically designed and qualified for subsea use.  Each deliverable connector(s) shall be factory acceptance tested (FAT) as specified in Table 1.  Batch testing is not acceptable.  Each connector shall include a documentation package including all material certifications, material origins and test results.  A Certificate of Conformance (C of C) shall be supplied for each connector.  One copy of the documentation package shall be provided to the buyer at no charge. The supplier shall retain a documentation package for a minimum period of 20 Years.  At a minimum, the supplier shall meet or exceed all ratings as listed in Table 2. The supplier shall be ISO 9001 registered. 

Quality Conformance - Requirements

Table 1 - Supplier Testing Standards

Hydrostatic Test:

Insulation Resistance: Insertion Loss: 

Bench Tests:

Insulation Resistance: Insertion Loss: Mate/Demate Function:

7,500psi

Pin-Pin & Pin-Gnd 10G( Min @ 1,000Vdc 

<0.50 dB / per circuit

Pin-Pin & Pin-Gnd 10G( Min @ 1,000Vdc <0.50 dB / per circuit

1 Cycle Minimum

Operational Characteristics:

Amperage Rating: 

Voltage Rating: 

Insertion Loss: 

Mated Back Reflection: Mate/Demate Cycles: Operational Temperature: Storage Temperature: Mating Force

Design Characteristics:

<0.50 dB Matched, <0.75 dB Unmatched / per circuit 

5 Amps / per circuit 1,000VDC / 600VAC RMS 

> -30dB

>100

0°C - +50°C --- --23°C - +60°C <80 lbs. Force
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Flying ROV Connector

Fixed Mount ROV Connector
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Contact Resistance:
<0.01 ( / per circuit

Design Life:
25 Years

Ancillary Equipment Oil-Filled Hose Series

Subsea Jumpers Cable Assemblies - General
The Jumper(s) supplied shall be specifically designed and qualified for subsea use.  Each deliverable jumper shall be factory acceptance tested (FAT) as specified in Table 1.  Batch testing is not acceptable. Each jumper shall include a documentation package including all material certifications, material origins and test results.  A Certificate of Conformance (C of C) shall be supplied for each jumper assembly.  One copy of the documentation package shall be provided to the buyer at no charge. The supplier shall retain a documentation package for a minimum period of 20 Years.
At a minimum, the supplier shall meet or exceed all ratings as listed in Table 2. The supplier shall be ISO 9001 registered. 

Quality Conformance - Requirements

Table 1 - Supplier Testing Standards

Hydrostatic Test:


7,500 psi

Continuity Resistance: 
End to End 1 @ 500 Vdc


Insulation Resistance: 
Pin-Pin, Pin-Gnd 10G Min @ 1000 Vdc 

Insertion Loss: 

<0.5 dB per circuit

Bench Tests:

Gas Leak:


30 Minutes @ 30 psi (Minimum)

Insulation Resistance: 
Pin-Pin, Pin-Gnd 10G Min @ 1000 Vdc


Insertion Loss: 

<0.5 dB per circuit

Table 2 - Standard Specifications

Typical Jumper Assembly

	ODHOSE-12HBD
	01.150
	00.625
	ITEM
	DESCRIPTION
	MATERIAL/LAY-UP FROM OUTSIDE INWARD

	
	
	
	1.
	OUTER
	COLOR TO

	ODHOSE-BHBD
	00.850
	00.410
	
	JACKET/COVER
	NBR/PVC BLEND, BE SPECIFIED

ON P0.

	ODHOSE-6HBD
	00.700
	00.310
	2.
	RADIAL REINFORCEMENT
	POLYESTER

	REF NUMBER
	p "q^
	,.B„
	3.

4.
	INSULATION

AXIAL REINFORCEMENT
	HYPALON

KEVLAR

	TABLE 1
	5.
	INNER LINER/TUBE
	NON-CONDUCTNE NITRILE
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	FEATURE
	-6 RATING
	-8 RATING
	-12 RATING

	MIMIMUM BEND RADIUS:
	3" (76mm)
	4° (102mm)
	5' (125mm)

	AXIAL LOAD;
	
	
	

	MAX WORKING:
	300 Ibs
	400 Ibs
	600 Ibs

	MIN FAILURE:
	450 Ibs
	600 Ibs
	900 Ibs

	MAX AXIAL STRETCH:
	27. ® 300 Ibs
	3% ® 400 Ibs
	3% ® 600 Ibs

	PRESSURE RATING;
	
	
	

	MAX WORKING:
	225psi
	225psi
	225psi

	PROOF TEST:
	450psi
	450psi
	400psi

	MIN BURST:
	900psi
	900psi
	900psi

	MIN RADIAL EXPANSION:
	157, 0 150 psi
	15% ® 150 psi
	15% ® 150 psi

	LENGTH CHANGE UNDER
	
	
	

	PRESSURE:
	+0/-1% 0 150 psi
	+0/-1% ® 150 psi
	+0/-1% ® 150 psi

	FLUID COMPATABILITY:
	SEAWATER & SILICONE OIL
	SEAWATER & SILICONE OIL
	SEAWATER & SILICONE OIL

	TEMPERATURE RATING:
	
	
	

	LOWER LIMIT:
	-2'C
	-2'C
	-2'C

	UPPER LIMIT:
	+50'C
	+50'C
	+50'C


Product Specification -Ancillary Equipment

FITA Series

Cable Terminations

Field Installable Testable Assemblies (FITA) - General
The FITA(s) supplied shall be specifically designed and qualified for subsea use.  Each FITA shall be Qualified for the cable that it will be installed to as specified in Table 1.  Each FITA shall include a documentation package including all material certifications, material origins and test results.  A Certificate of Conformance (C of C) shall be supplied for each FITA assembly.  One copy of the documentation package shall be provided to the buyer at no charge. The supplier shall retain a documentation package for a minimum period of 20 Years. The supplier shall be ISO 9001 registered. 

Quality Conformance - Requirements

Table 1 - Supplier Qualification Testing Standards

Hydrostatic Test:


7,500 psi

Insulation Resistance:

Pin-Pin, Pin-Gnd 10G Min @ 1000 Vdc 

Insertion Loss: 

<0.5 dB per circuit

Bench Tests:

Water Flooded Termination:
Insulation Resistance (IR) 

Cable Load Test:

500 lbf

Gas Leak:


30 Minutes @ 20 psi (Minimum)

Continuity Resistance:
End to End 1 @ 500 Vdc 


Insulation Resistance:
Pin-Pin, Pin-Gnd 10G Min @ 1000 Vdc
Insertion Loss:

<0.5 dB per circuit
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MBARI is an Affirmative Action/Equal Employment Opportunity employer. MBARI does not discriminate against any employee or applicant for employment 

becauseof race, color, religion, sex or national origin. MBARI takes affirmative action to ensure that applicants are employed, and that employees are treated 

during employment, without regard to their race, color, religion, sex or national origin. MBARI will comply with the provisions of Executive Order 11246 of 

9/24/65, and relevant rules and regulations as required by law. Please be advised that all contractors and subcontractors having 50 or more employees and a 

federal government contract or subcontract of $50,000 or more must develop a written affirmative action plan under the federal guidelines.



























Items 3.1, 5.1, 7.1, 1.1 to have 45 degree, extended length
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$199,562.00







Connector/cable assemblies per

ODI Quotation #5412 Rev A and

MBARI drawing  #101324SCD





1.1, 1.2, 1.3 may have extended delivery time, please advise best estimate.

strain relief.  Design to be approved by MBARI before fabrication

Item 1.3 molded strain relief design to be approved by MBARI before fab.

All items except 1.1, 1.2, 1.3 are required by the end of November 2001.  Items
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																		PURCHASE  ORDER

																		Purchase Order Invalid Without PO#

																		PO#:		PO-0102893

																		DATE:		10/5/01

				VENDOR:				Ocean Design, Inc										SHIP TO:

				ADDRESS:				9 Aviator Way												7700 Sandholdt Road

								Ormond Beah, FL 32174												Moss Landing, CA 95039-9644

				Phone:				904 6753575				Fax:		904 6733671

				Contact:				Steven Thumbeck										SHIP VIA:

																				UPS		FedEX

				MBARI Contacts:

				Name:				Gene Massion										EXPECTED DELIVERY DATE:

				Phone:				831 7751922				Fax:		831 7751646				FOB:		Shipping Point				Destination

				Name:														PAYMENT TERMS:				Net 30

				Phone:								Fax:						Send Invoices to:

																		MBARI Accounts Payable

																		7700 Sandholdt Rd., Moss Landing, CA 95039-9644

				REQUISTIONER:														Phone: (831) 775-1700     Fax: (831) 775-1630

				ITEM		QTY.		U/M		PART NUMBER		DESCRIPTION								UNIT PRICE				EXTENDED

				1		1		lot				Connector/cable assemblies per								$199,562.00				199,562.00

												ODI Quotation #5412 Rev A and												- 0

												MBARI drawing  #101324SCD												- 0

																								- 0

										Items 3.1, 5.1, 7.1, 1.1 to have 45 degree, extended length														- 0

										strain relief.  Design to be approved by MBARI before fabrication														- 0

																								- 0

										Item 1.3 molded strain relief design to be approved by MBARI before fab.														- 0

																								- 0

										All items except 1.1, 1.2, 1.3 are required by the end of November 2001.  Items														- 0

										1.1, 1.2, 1.3 may have extended delivery time, please advise best estimate.														- 0

																								- 0

																								- 0

																								- 0

																								- 0

				PROJECT/ACCOUNT CHARGE NUMBER:										200126-5330						SUBTOTAL				199,562.00

																				SALE/USE TAX		7.0%		13,969.34

				REMARKS:																SHIPPING				100.00

																				TOTAL				$   213,631.34

				APPROVAL:

				DATE:

				MBARI is an Affirmative Action/Equal Employment Opportunity employer. MBARI does not discriminate against any employee or applicant for employment becauseof race, color, religion, sex or national origin. MBARI takes affirmative action to ensure that appli

				Form Revised  04/13/01



Use this area for purchases charged to multiple projects. Please include line items or % to be charged to each project / account number.

Default tax rate. 
Change the tax % if needed

Calculates using default tax rate. 
Change the tax % if needed

If using e-mail signatures, leave blank. Forwarding e-mail is equal to a signature.  If obtaining manual signatures, print PO then get signatures.
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