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DIP & MULTI PURPOSE CELLS

BODY MATERIAL: CENTRIFUGAL CAST EPOXY
TUBING. BLACK
PLATE MATERIAL: BASE NICKEL #200
Au. GOLD OVER NICKEL
4375

40 Pt PLATINUM BLACK OVER
W GOLD OVER NICKEL
@V_m 800 MULT! PURPOSE CELLS SPACER: HIGH DENSITY POLYETHYLENE
T T LARGE FLOW CELL
8 PIN DIN CONNECTOR BODY MATERIAL : mﬂﬂwcmmwﬁmzq EPOXY
PLATE MATERIAL: BASE STAINLESS STEEL #318
800 DIP CELLS SPACER: CENTRIFUGAL CAST EPOXY
m IW_ TJUBING. BLACK
6.00 RECOMMENDED MAX IMUNS
TEMPERATURE : 70 DEG. C
375 PRESSURE : 25 P.S. 1.
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