**********************************************************
GHI Electronics, LLC
Gadgeteer SDK for NETMF 
**********************************************************

SDK Version 2013 R3 (v4.2.101)
October 23, 2013
======================================

Built With

•	Microsoft .NET Micro Framework v4.3 (RTM)
•	GHI Electronics OSHW v4.2 NETMF SDK v1.0.7
•	GHI Electronics Premium v4.2 NETMF SDK v1.0.6
•	Microsoft Gadgeteer Core v2.42.800
____________________________________________________________

FEZ Hydra Mainboard

•	See GHI OSHW SDK Release Notes.
____________________________________________________________

FEZ Spider Mainboard

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Spider II Mainboard

•	FEZ Spider II uses G120 SoM, see GHI Premium SDK Release Notes.
•	Updated pin mappings.
____________________________________________________________

FEZ Cobra II Mainboard

•	FEZ Cobra II uses G120 SoM, see GHI Premium SDK Release Notes.
•	Fixed the Socket 8 COM port and pin sharing.
____________________________________________________________

FEZ Cerberus Mainboard

•	Serial Camera module may not work as expected.
•	See GHI OSHW Release Notes for firmware changes.
____________________________________________________________

FEZ Raptor Mainboard

•	FEZ Raptor uses G400S SoM, see GHI Premium SDK Release Notes.
•	Now properly imports the Premium libraries and has proper socket construction.
•	Distance US3 module now works properly with the Raptor.
____________________________________________________________

Gadgeteer Modules

•	All modules have updated internal documentation/commenting. 
•	All module interfaces have been reviewed, and some interfaces may have changed.
•	Display CP7 and N7 are no longer corrupted on G120.
•	The music module no longer crashes on construction.
•	HubAP5 no longer throws an exception when using glitch filter.
•	Improved Joystick read performance.
•	Added channel band and spacing to the FM Radio.
•	Added Button S7 driver.
•	Added DAQ 8B driver.

Miscellaneous 

Release Info

•	None.

SDK Version 1.6.14
April 30, 2013
======================================

Version Info

Built with:
•	Microsoft .NET Micro Framework v4.3 (RTM)
•	GHI Electronics OSHW v4.2 NETMF SDK v1.0.5
•	GHI Electronics Premium v4.2 NETMF SDK v1.0.4
•	Microsoft Gadgeteer Core v2.42.700
____________________________________________________________

FEZ Hydra Mainboard

•	See GHI OSHW SDK Release Notes.
____________________________________________________________

FEZ Spider Mainboard

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Spider II Mainboard

•	FEZ Spider II uses G120 SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Cobra II Mainboard

•	FEZ Cobra II now has an extended designer with 4 extra sockets to allow users to have access to the header while using Gadgeteer sockets.
•	Serial Camera module and WiFi may not work as expected if used at the same time.
•	FEZ Cobra II uses G120 SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Cerberus Mainboard

•	Sockets 5 and 6 were changed from having type Y to type X to avoid pin reservation errors relating to the shared SPI pins on sockets 5 and 6.
•	Serial Camera module may not work as expected.
•	See GHI OSHW Release Notes for firmware changes.
____________________________________________________________

Gadgeteer Modules

•	All modules have updated internal documentation/commenting. 
•	All module interfaces have been reviewed, and some interfaces may have changed.
•	An error with the Bluetooth module’s SetPinCode function was corrected.
•	Errors in the MaxO module’s WritePin and Clear functions were corrected.
•	Display CP7 minor change to event names to make interface more uniform.
•	LED7R has a minor change involving pin reservation.
•	Relay ISO16 module error with requiring socket type “S” instead of “Y” has been corrected.
•	Relay ISO16 module error with DisableAllRelays function has been corrected.
•	FEZCobra II mainboard has been extended with 4 extra sockets.
•	FEZSpider II mainboard has been added.
•	FEZCerbot mainboard has been added.
•	FEZCerbot Controller module has been added to provide access to the FEZCerbot’s on-board features.
•	Distance US3 module has been added.
•	Tunes module has been added.
•	Radio FM1 module has been added.
•	USB Serial SP module has been added.
•	WiFi RN171 module has been added, with a beta driver.
•	LED Strip module has been added.
•	Accel G248 module has been added.
•	Amp M35 module has been added.
•	Serial Camera module interface changed to be uniform with the USB Host Camera module driver.
•	Added delays to Character Display module to increase stability on some mainboards.
•	Display N18 module driver Initialize method made private, and interface to draw has been improved. 
•	All modules and mainboards now have power consumption estimates included, which can be viewed in the designer.
•	Properly marked SPI pins as shared for all S type sockets.
•	LED7C added off color. 

Miscellaneous 

Release Info

•	Removed updater applications.

SDK Version 1.6.12
February 14, 2013
======================================

Version Info

Built with:
•	Microsoft .NET Micro Framework v4.2 (QFE2)
•	GHI Electronics OSHW v4.2 NETMF SDK v1.0.3
•	GHI Electronics Premium v4.2 NETMF SDK v1.0.2
•	Microsoft Gadgeteer Core v2.42.600
____________________________________________________________

FEZ Hydra Mainboard

•	See GHI OSHW SDK Release Notes.
____________________________________________________________

FEZ Spider Mainboard

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Cobra II Mainboard

•	FEZ Cobra II uses G120 SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Cerberus Mainboard

•	See GHI OSHW Release Notes for firmware changes.
____________________________________________________________

Gadgeteer Modules

•	All modules have updated internal documentation/commenting. 
•	All module interfaces have been reviewed, and some interfaces may have changed.
•	Added Beta support for Gadgeteer Networking interface to Ethernet J11D.

SDK Version 1.6.11
February 1, 2013
======================================

Version Info

Built with:
•	Microsoft .NET Micro Framework v4.2 (QFE2)
•	GHI Electronics OSHW v4.2 NETMF SDK v1.0.2
•	GHI Electronics Premium v4.2 NETMF SDK v1.0.1
•	Microsoft Gadgeteer Core v2.42.600
____________________________________________________________

FEZ Hydra Mainboard

•	See GHI OSHW SDK Release Notes.
•	Added missing support for native software I2C, increasing performance of software I2C. 
____________________________________________________________

FEZ Spider Mainboard

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Cobra II Mainboard

•	FEZ Cobra II uses G120 SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Cerberus Mainboard

•	See GHI OSHW Release Notes for firmware changes.
•	Added missing support for native software I2C, increasing performance of software I2C.
•	Added Bitmap Converter support.
____________________________________________________________

Gadgeteer Modules

•	All modules have updated internal documentation/commenting. 
•	All module interfaces have been reviewed, and some interfaces may have changed.
•	Corrected Relay ISO16 module to use Y socket type instead of S socket type.
•	Altered T35, CP7, and TE35 to better reserve pins on certain sockets.
•	Added Display N18 module driver. 
•	Added Display T43 module driver.
•	Added FEZtive module driver.
•	Added LED7C module driver.
•	Fixed IO60P16 static member issue that stopped multiple modules from being used simultaneously.
•	Fixed IO60P16 PWM error.

SDK Version 1.6.10
November 29, 2012
======================================

Version Info

Built with:
•	Microsoft .NET Micro Framework v4.2 (QFE2)
•	GHI Electronics OSHW NETMF SDK v1.0.1
•	GHI Electronics Premium v4.2 NETMF SDK v1.0.0
•	Microsoft Gadgeteer Core v2.42.600
____________________________________________________________

FEZ Hydra Mainboard

•	See GHI OSHW SDK Release Notes.
____________________________________________________________

FEZ Spider Mainboard

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Cobra II Mainboard

•	FEZ Cobra II uses G120 SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Cerberus Mainboard

•	See GHI OSHW Release Notes for firmware changes.
____________________________________________________________

Gadgeteer Modules

•	All modules have updated internal documentation/commenting. 
•	All module interfaces have been reviewed, and some interfaces may have changed.
•	Added ColorSense Module.

SDK Version 1.6.9
November 21, 2012
======================================

Version Info

Built with:
•	Microsoft .NET Micro Framework v4.2 (QFE2)
•	GHI Electronics OSHW NETMF SDK v1.0.0
•	GHI Electronics Premium v4.2 NETMF SDK v0.0.7
•	Microsoft Gadgeteer Core v2.42.600
____________________________________________________________

FEZ Hydra Mainboard

•	See GHI OSHW SDK Release Notes.
____________________________________________________________

FEZ Spider Mainboard

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Cobra II Mainboard

•	Initial release.
•	FEZ Cobra II uses G120 SoM, see GHI Premium SDK Release Notes.
____________________________________________________________

FEZ Cerberus Mainboard

•	See GHI OSHW Release Notes for firmware changes.
____________________________________________________________

Gadgeteer Modules

•	All modules have updated internal documentation/commenting. 
•	All module interfaces have been reviewed, and some interfaces may have changed.
•	WifiRS21, Ethernet J11D and Ethernet ENC28 modules’ Gadgeteer networking class removed to avoid confusion with included premium library implementation.
•	Added Stepper L647x module.
•	Motor Controller frequency altered.
•	MaxO module inverted output corrected.
•	Added Thermocouple module.
•	Added Breakout module.
•	Added FEZ Cobra II mainboard driver.

SDK Version 1.6.8
October 24, 2012
======================================

Version Info

Built with:
•	Microsoft .NET Micro Framework v4.2 (QFE2)
•	GHI Electronics OSHW NETMF SDK v0.0.8
•	GHI Electronics Premium v4.2 NETMF SDK v0.0.6
•	Microsoft Gadgeteer Core v2.42.600

____________________________________________________________

FEZ Hydra Mainboard / Kit

Release Info

•	See GHI OSHW SDK Release Notes.
•	Socket 14 has been changed from socket type AY to AX.
•	4.1 support removed.

Known Issues

•	See GHI OSHW SDK Release Notes.

____________________________________________________________

FEZ Spider Mainboard / Kit

Release Info

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes.
•	4.1 support removed.

Known Issues

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes..

____________________________________________________________

FEZ Cerberus Mainboard / Kit

Release Info

•	See GHI OSHW Release Notes for firmware changes.

Known Issues

•	None
____________________________________________________________

Gadgeteer Modules

Release Info

•	All modules have updated internal documentation/commenting. 
•	All module interfaces have been reviewed, and some interfaces may have changed.
•	All 4.1 support has been removed.
•	Community contributed Bluetooth driver was added.
•	Checksum verification was added to the RFID module driver, so usage may change.
•	Added GasSense module.
•	Added Current ASC712 module.
•	Added Relay ISOx16 module.
•	Added Pulse InOut module.
•	Added UC Battery 4xAA module.
•	Added FLASH module.
•	Added SerCam module.
•	Added Ethernet ENC28 module.
•	Added Ethernet J11D driver.
•	Added USB Client SP module.
•	Added WiFi RS21 driver.
•	Removed EBlock Expansion module.

Known Issues

•	Motor Controller may not accept setting a low speed, causing the motor to be set to 100% speed.

SDK Version 1.6.7
August 23, 2012
======================================

Version Info

Built with:
•	Microsoft .NET Micro Framework v4.2 (QFE2)
•	GHI Electronics NETMF SDK v1.0.19
•	GHI Electronics OSH NETMF SDK v1.0.5
•	GHI Electronics OSHW NETMF SDK v0.0.7
•	GHI Electronics Premium v4.2 NETMF SDK v0.0.5
•	Microsoft Gadgeteer Core v2.42.600

____________________________________________________________

FEZ Hydra Mainboard / Kit

Release Info

•	See GHI OSHW SDK Release Notes.

Known Issues

•	See GHI OSHW SDK Release Notes.

____________________________________________________________

FEZ Spider Mainboard / Kit

Release Info

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes.

Known Issues

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes..

____________________________________________________________

FEZ Cerberus Mainboard / Kit

Release Info

•	See GHI OSHW Release Notes for firmware changes.

Known Issues

•	4.1 not supported.
____________________________________________________________

Gadgeteer Modules

Release Info

•	Fixed Music module to properly handle events.

Known Issues

•	OBDII not supported in 4.1.
•	No Ethernet J11D driver is included. Tested to work with FEZ Spider with no needed drivers.
•	WIFi support is only available in 4.1.
•	SerCam driver currently not available.
•	Bluetooth driver currently not available.
•	Motor Controller may not accept setting a low speed, causing the motor to be set to 100% speed.

SDK Version 1.6.6
August 13, 2012
======================================

Version Info

Built with:
•	Microsoft .NET Micro Framework v4.2
•	GHI Electronics NETMF SDK v1.0.19
•	GHI Electronics OSH NETMF SDK v1.0.5
•	GHI Electronics OSHW NETMF SDK v0.0.6
•	GHI Electronics Premium v4.2 NETMF SDK v0.0.4
•	Microsoft Gadgeteer Core v2.42.600

____________________________________________________________

FEZ Hydra Mainboard / Kit

Release Info

•	See GHI OSHW SDK Release Notes.
•	Added messages alerting the user when the mainboard will reboot when setting a display configuration.
•	Now properly shares display socket (R,G,B) pins again.

Known Issues

•	See GHI OSHW SDK Release Notes.

____________________________________________________________

FEZ Spider Mainboard / Kit

Release Info

•	FEZ Spider uses EMX SoM, see GHI Premium SDK Release Notes.
•	Added messages alerting the user when the mainboard will reboot when setting a display configuration.
•	Now properly shares display socket (R,G,B) pins again.
•	Added native Bitmap Converter driver.
•	Warning on socket #9 referring to missing analog out has been corrected.

Known Issues

•	FEZ Spider uses EMX SoM  see GHI Premium SDK Release Notes..

____________________________________________________________

FEZ Cerberus Mainboard / Kit

Release Info

•	See GHI OSHW Release Notes for firmware changes.

Known Issues

•	4.1 not supported.
____________________________________________________________

Gadgeteer Modules

Release Info

•	Added community contributed IO60P16 module driver.
•	Corrected MotorControllerL298 for 4.2 PWM. 
•	Added Display TE35 module.
•	Corrected LCD configuration properties for Display CP7.

Known Issues

•	OBDII not supported in 4.1.
•	No Ethernet J11D driver is included. Tested to work with FEZ Spider with no needed drivers.
•	WIFi support is only available in 4.1.