**********************************************************
GHI Electronics, LLC
Premium SDK for NETMF v4.2
**********************************************************

SDK Version 1.0.2
February 14, 2013
======================================

Version Info

Important Note: Requires .NET Micro Framework 4.2 QFE2 and Visual Studio 2010

•	EMX v4.2.9.0, TinyBooter v4.2.9.0
•	G120 v4.2.9.0, TinyBooter v4.2.9.0
•	GHI Premium NETMF Library v4.2.9.0

____________________________________________________________

EMX System-on-Module

Release Info

•	PWM has been fixed.
•	USB Mass Storage support fixed.
•	File creation/modification time error corrected.

Known Issues

•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.

G120 System-on-Module

Release Info

•	SSL is now supported.
•	USB Mass Storage fixed.
•	File creation/modification time error corrected.
•	Boot time significantly decreased.

Known Issues

•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.
•	Wi-Fi support using static IP and DCHP has stability issues.

Premium Libraries

Release Info

•	Added Startup logo.
•	Added .Wav playback support.

Known Issues

•	Low Power feature is not currently supported.
•	Number of networking sockets is limited to 32. Please see https://netmf.codeplex.com/workitem/1907 for more information.

SDK Version 1.0.1
February 1, 2013
======================================

Version Info

Important Note: Requires .NET Micro Framework 4.2 QFE2 and Visual Studio 2010

•	EMX v4.2.8.0, TinyBooter v4.2.8.0
•	G120 v4.2.8.0, TinyBooter v4.2.8.0
•	GHI Premium NETMF Library v4.2.8.0

____________________________________________________________

EMX System-on-Module

Release Info

•	Corrected UDP implementation. Now sends proper datagrams.
•	TimeService now works as expected.
•	Number of TCP and UDP Sockets increased to 128.
•	Defaulted IP and DNS values to 0.0.0.0.
•	OneWire now functions as expected.

Known Issues

•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.

G120 System-on-Module

Release Info

•	RLP now works as expected.
•	TimeService now works as expected.
•	Number of TCP and UDP Sockets increased to 128.
•	Defaulted IP and DNS values to 0.0.0.0.
•	Setting the same network interface multiple times no longer raises an exception.
•	The issue concerning a firmware lockup involving Garbage Collection was resolved.
•	OneWire now functions as expected.

Known Issues

•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.

Premium Libraries

Release Info

•	System Update feature was added.
•	USB Client Keyboard support now works with a PC BIOS.

Known Issues

•	User Application Protection is not currently supported.

SDK Version 1.0.0
November 29, 2012
======================================

Version Info

Important Note: Requires .NET Micro Framework 4.2 QFE2 and Visual Studio 2010

•	EMX v4.2.7.0, TinyBooter v4.2.7.0
•	G120 v4.2.7.0, TinyBooter v4.2.7.0
•	GHI Premium NETMF Library v4.2.7.0

____________________________________________________________

EMX System-on-Module

Release Info

•	Corrected One Wire.

Known Issues

•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.

G120 System-on-Module

Release Info

•	Resistive touch is now implemented.

Known Issues

•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.
•	Setting the same network interface more than once may raise an exception when trying to set it again.

Premium Libraries

Release Info

•	Ethernet ENC28 and WiFi RS21 now have the ability to set the SPI clock speed.

Known Issues

•	User Application Protection is not currently supported.
•	SystemUpdate is not currently supported.

SDK Version 0.0.7
November 21, 2012
======================================

Version Info

Important Note: Requires .NET Micro Framework 4.2 QFE2 and Visual Studio 2010

•	EMX v4.2.6.0, TinyBooter v4.2.6.0
•	G120 v4.2.6.0, TinyBooter v4.2.6.0
•	GHI Premium NETMF Library v4.2.6.0

____________________________________________________________

EMX System-on-Module

Release Info

•	Added SSL support.
•	USB camera support added.

Known Issues

•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.
•	One Wire is not functioning. 

G120 System-on-Module

Release Info

•	SD card support now works as expected.
•	See below changes to the GHI Premium Libraries.
•	COM5 is now supported.
•	GPIO Glitch Filter is now supported.
•	SPI3 now supported.
•	Fixed USB camera support.
•	Handshaking on COM2 is now supported.

Known Issues

•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.
•	Setting the same network interface more than once may raise an exception when trying to set it again.
•	Resistive touch is not yet implemented.

Premium Libraries

Release Info

•	Configuration:StartupLogo has been temporarily removed.
•	Miscellaneous spelling errors were corrected.

Known Issues

•	User Application Protection is not currently supported.
•	SystemUpdate is not currently supported.

SDK Version 0.0.6
October 24, 2012
======================================

Version Info

Important Note: Requires .NET Micro Framework 4.2 QFE2 and Visual Studio 2010

•	EMX v4.2.5.0, TinyBooter v4.2.5.0
•	G120 v4.2.5.0, TinyBooter v4.2.5.0
•	GHI Premium NETMF Library v4.2.5.0

____________________________________________________________

EMX System-on-Module

Release Info

•	Added LWIP TCP/IP stack.
•	Added built-in Ethernet driver.
•	Added Ethernet ENC28 driver.
•	Added WiFi RS21 driver.
•	See below for changes to the GHI Premium Libraries.

Known Issues

•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.
•	SSL is not currently supported.

G120 System-on-Module

Release Info

•	Initial public release. 
•	Added Alpha SD card support.
•	Added LWIP TCP/IP stack.
•	Added Ethernet ENC28 driver.
•	Added WiFi RS21 driver.
•	See below changes to the GHI Premium Libraries.

Known Issues

•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.
•	COM5 is not yet supported.
•	Handshaking on COM2 is not yet supported.
•	GPIO Glitch Filter is not currently supported.
•	SD driver is Alpha quality.
•	Setting the same network interface more than once may raise an exception when trying to set it again.

Premium Libraries

Release Info

•	GHI.Premium.Net has been added.
•	Parallel Port class is now available in GHI.Premium.Hardware.
•	Power class is now available in GHI.Premium.Hardware.
•	SignalCapture (was PinCapture) class is now available in GHI.Premium.Hardware.
•	Watchdog class is now available in GHI.Premium.Hardware.

Known Issues

•	User Application Protection is not currently supported.
•	SystemUpdate is not currently supported.

SDK Version 0.0.5
August 23, 2012
======================================

Version Info

Important Note: Requires .NET Micro Framework 4.2 QFE2 and Visual Studio 2010

•	EMX v4.2.4.0, TinyBooter v4.2.4.0
•	G120 v4.2.4.0, TinyBooter v4.2.4.0
•	GHI Premium NETMF Library v4.2.4.0

____________________________________________________________

EMX System on Module

Release Info

•	Added LWIP TCP/IP stack with Ethernet driver.
•	1-Wire is now functioning as expected.
•	1-Wire now uses Microsoft.SPOT.Hardware.OneWire.
•	Replaced RTIP TCP/IP stack with lwip TCP/IP stack.
•	DHCP can now be enabled from MFDeploy
•	Switched Analog Out support from GHI Premium libraries to Microsoft standard libraries.

Known Issues

•	Watchdog class is not available and is being evaluated.
•	Hibernate(WakeUpInterrupt WakeUpInterrupt) is not available and is being evaluated.
•	EthernetOscillatorEnable(bool state) is not available and is being evaluated.\
•	User Application Protection is not available and is being evaluated.
•	Setting PWM frequency will corrupt Duty Cycle. To fix, a user must then set Duty Cycle. See https://netmf.codeplex.com/workitem/1749 for more information.
•	SSL is not currently supported.
•	SystemUpdate is not currently supported.
•	WiFi is not currently supported.
•	PPP is not currently supported.

G120 System on Module

Release Info

•	Initial release, for select customer testing.

Known Issues

•	TBD.

SDK Version 0.0.4
August 13, 2012
======================================

Version Info

Important Note: Requires .NET Micro Framework 4.2 QFE1 and Visual Studio 2010

•	EMX v4.2.3.0, TinyBooter v4.2.3.0
•	GHI Premium NETMF Library v4.2.3.0

____________________________________________________________

EMX SoM

Release Info

•	Added SQlite.
•	Added USB Client.
•	Persistent Storage now works as expected.
•	Display configuration fixed to set the correct pixel clock rate to stop screen flicker.
•	Software I2C restart condition corrected.
•	Added LWIP TCP/IP stack with Ethernet driver (Alpha Support).

Known Issues

•	The following libraries are not yet supported: Net, SystemUpdate.
•	WiFi is not currently supported.
•	PPP is not currently supported.
•	1-Wire is not functioning as expected.
•	Watchdog class is not available,  and is being evaluated.
•	Hibernate(WakeUpInterrupt WakeUpInterrupt) is not available and is being evaluated.
•	EthernetOscillatorEnable(bool state) is not available and is being evaluated.

SDK Version 0.0.3 BETA
July 23, 2012
======================================

Version Info

Important Note: Requires .NET Micro Framework 4.2 and Visual Studio 2010

•	EMX v4.2.2.0, TinyBooter v4.2.2.0
•	GHI Premium NETMF Library v4.2.2.0

____________________________________________________________

EMX SoM

Release Info

•	Analog Out added to Hardware library.
•	Analog In altered to return a more accurate value.
•	Display Configuration Pixel Clock Divider member removed and replaced with Pixel Clock Rate.
•	The Watchdog and Power classes are being evaluated, and may be altered in an upcoming release.

Known Issues

•	The following libraries are not yet supported: Net, SQLite, SystemUpdate, USBClient.

SDK Version 0.0.2 BETA
June 22, 2012
======================================

Version Info

Important Note: Requires .NET Micro Framework 4.2 and Visual Studio 2010

•	EMX v4.2.1.0, TinyBooter v4.2.1.0
•	GHI Premium NETMF Library v4.2.1.0

____________________________________________________________

EMX SoM

Release Info

•	Addition of the following Premium 4.2 libraries: Hardware, Hardware.EMX, IO, Native, System, USBHost.
•	The Watchdog and Power classes are being evaluated, and may be altered in an upcoming release.

Known Issues

•	The following libraries are not yet supported: Net, SQLite, SystemUpdate, USBClient.

SDK Version 0.0.1 BETA
June 15, 2012
======================================

Version Info

Important Note: Requires .NET Micro Framework 4.2 and Visual Studio 2010

•	EMX v4.2.0.0, TinyBooter v4.2.0.0
•	No GHI Premium NETMF Library yet

____________________________________________________________

EMX SoM

Release Info

•	Initial release including all major peripherals, Display, SPI, I2C, UART, USB Client, Analog, PWM.

Known Issues

•	No Premium Library yet
•	Missing library-related peripherals, CAN, USN Host, Ethernet, WiFi, SD.
•	Display is locked to 320x240 and no native touch support yet.