%~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
% $Id: IridiumMsgSample.tex,v 1.2 2006/11/24 23:58:15 swift Exp $
%~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
% RCS Log:
%
% $Log: IridiumMsgSample.tex,v $
% Revision 1.2  2006/11/24 23:58:15  swift
% Updated format descriptions to account for changes in Sbe41cp firmware.
%
% Revision 1.1  2006/11/03 19:08:57  swift
% Added user manual to CVS control.
%
% Revision 1.2  2006/07/10 22:24:49  swift
% Modifications to bring the manual up to date with
% changes to the SeaBird CTD firmware (v1.1c).
%
% Revision 1.1  2006/04/11 15:32:40  swift
% Initial revision
%
%~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

\section{Sample: Iridium message file.}
\label{sec:IridiumMsgSample}
\renewcommand{\theequation}{\Alph{section}.\arabic{equation}}

The following is an example Iridium-message file (5135.009.msg) from
profile~9 of UW float~5135.  The blocks with park-phase PT data and high
resolution PTS data have been snipped to save space.  The actual message
file is included in the \emph{manual} directory your distribution.

{\small
\begin{verbatim}
ParkPt:    Oct 27 2006 09:12:21  1161940341   21614  991.13  5.0624
ParkPt:    Oct 27 2006 10:12:18  1161943938   25211  997.14  5.0385
ParkPt:    Oct 27 2006 11:12:18  1161947538   28811  994.93  5.0252
[snippage...]
ParkPt:    Nov 05 2006 12:12:18  1162728738  810011  999.88  5.0748
ParkPt:    Nov 05 2006 13:12:18  1162732338  813611  999.87  5.0815
ParkPt:    Nov 05 2006 14:12:18  1162735938  817211 1001.27  5.1691
$ Profile 5135.009 terminated: Sun Nov  5 23:33:42 2006
$ Discrete samples: 22
$       p        t        s
   999.76   5.1389  34.6385 (Park Sample)
  1995.95   2.4262  34.7183
  1947.22   2.5096  34.7160
  1898.18   2.5933  34.7124
  [snippage...]
  1098.41   4.7406  34.6413
  1047.72   4.9210  34.6328
   997.88   5.1765  34.6345
# Nov 05 2006 23:38:59 Sbe41cpSerNo[1520] NSample[11134] NBin[495]
00000000000000[2]
002B5CE0885115
003C5CE188511F
00505CE088511E
00645CE088511D
00785CDF88521C
008C5CDF88521B
00A05CDF88511A
00B45CDC88511A
[snippage...]
2670144B874714
2684144D874814
2698145C874D14
# GPS fix obtained in 65 seconds.
#         lon     lat mm/dd/yyyy hhmmss nsat
Fix:  106.738 -19.100 11/05/2006 234740    7
Apf9iFwRev=051906
ActiveBallastAdjustments=0
AirBladderPressure=124
AirPumpAmps=69
AirPumpVolts=191
BuoyancyPumpOnTime=1899
BuoyancyPumpAmps=216
BuoyancyPumpVolts=172
CurrentPistonPosition=199
DeepProfilePistonPosition=16
GpsFixTime=65
FloatId=5135
ParkDescentPCnt=7
ParkDescentP[0]=5
ParkDescentP[1]=45
ParkDescentP[2]=78
ParkDescentP[3]=95
ParkDescentP[4]=98
ParkDescentP[5]=99
ParkDescentP[6]=99
ParkPistonPosition=71
ParkObs={ 999.8dbar,    5.139C,  34.6385PSU }
ProfileId=009
ObsIndex=21
QuiescentAmps=6
QuiescentVolts=198
RtcSkew=8
Sbe41cpAmps=12
Sbe41cpVolts=190
Sbe41cpStatus=0x0000
status=0x0001
SurfacePistonPosition=177
SurfacePressure=0.01
Vacuum=77

<EOT>
\end{verbatim}}

%%% Local Variables: 
%%% mode: latex
%%% TeX-master: "IridiumApex"
%%% End: 
