MFB Commands
ATV [Analytical Top Valve]
ASV [Analytical Sample Valve]
ARV [Analytical Reagent Valve]
AS
[Syringe Pump]

PSR
[3 Way Valve]

AIV [Analytical Intake Valve]

	Type
	14 Port Valve
	14 Port Valve
	14 Port Valve
	3 Way Valve

	Name
	Analytical Top Valve
	Analytical Waste Valve
	Analytical Reagent Valve
	Analytical Syringe Valve

	Command
	ATV
	ASV
	ARV
	PSR (3 way)

	Center
	:holding coil
	:waste
	:atv9
	:syringePump

	1
	:bleach
	 
	:air
	:carrierSolution

	2
	:waste
	:SPE Inlet
	:MM1
	:holdingCoil

	3
	:TE
	:SPE Outet
	:MM2
	 

	4
	:SPE Outlet
	 
	:P/P1
	 

	5
	:air
	 
	:P/P2
	 

	6
	:wash 1
	:PCR 2
	:P/P3
	 

	7
	:wash 2
	:PCR  1
	:P/P4
	 

	8
	:AIV/sample 
	 
	:P/P5
	 

	9
	:bleach
	 
	:P/P6
	 

	10
	:sample 2
	 
	:P/P7
	 

	11
	:SPE Inlet
	 
	:P/P8
	 

	12
	:ARV 
	 
	:controlDNA
	 

	13
	:air
	 
	:waste
	 

	14
	 :PCR
	 
	:carrierSolution
	 


  
