Dye Tests
	 
	Volume
	Speed
	Dye Color

	PCR Plug
	 
	 
	 

	Prime syringe and holding coil to clear bubbles
	 
	 
	 

	Prime thermal PCR tubing and PCR with PCR water
	 
	 
	 

	Prime Reagent Reservoirs
	 
	 
	 

	Prime Sample line, bringing sample from sample source to the valve
	 
	 
	 

	Air
	10 ul
	 
	 

	P/P
	4 ul
	 
	Blue

	Control DNA
	2 ul
	 
	Yellow

	Master Mix
	18 ul
	 
	Red

	Sample
	10 ul
	 
	Green

	Air
	5 ul
	 
	 

	Dispense Plug to PCR module.
	 
	1 ul/s
	 

	 
	 
	 
	 

	DNA Extraction
	 
	 
	 

	Mix and dispense to pillar chip
	 
	 
	 

	Guanidine
	100 ul
	1ul/s
	Blue

	Sample
	100 ul
	1 ul/s
	Green

	Rinse pillar chip with ethanol
	 
	 
	 

	Ethanol
	3000 ul
	100 ul/s
	Yellow

	Dispense air to pillar chip to displace ethanol
	 
	 
	 

	Air
	200 ul
	10 ul/s
	 

	Dispense Tris/EDTA  elution buffer to pillar chip
	 
	 
	 

	Tris/EDTA
	10 ul
	1 ul/s
	Red

	Heat pillar chip to 80C
	 
	 
	 

	Recover Tris eluent from pillar chip
	10 ul
	1 ul/s
	 

	Despense eluent to flow through PCR module
	 
	 
	 


