ESP Instrument Assembly
Sub-assemblies:

Storage Carousel

Storage Elevator

Processing Clamp

Collection Clamp

Sample Syringe

Processing and Collection Syringes

Flush Puck Garage

Manipulator

Camera

Heaters (2)

Rotary Valves (8)

Series Reagent Valves

Parts:

Assembly Stand

Top Plate

Fasteners:

· Dowel Pins:
· 1/8” x ½” (2) for Flush Garage
· 3/16” x 5/8” (2) for Storage Elevator

· 3/16” x 5/8” (2) for Processing Clamp
· 3/16” x 5/8” (2) for Collection Clamp

· 5/32” x 5/8” (2) for Camera

· 3/32” x 5/8” (1) for Storage Carousel

· 1/8” x 5/8” (1) for Storage Carousel

· 3/16” x 5/8” (2) for Manipulator
Tools needed:

Instructions:

