ESP Weekly Meeting 

23Feb07 (Tank View, 10:00 am)
Attending:

Andrew Chase, Kevin Gomes, John Graybeal, Dianne Greenfield, Doug Pargett, Chris Preston, Chris Scholin, Rich Schramm





Purpose: 
Follow-up meeting to set ESP Data Management and GUI requirements definition.

Pseudo-Minutes:


1. Project data is on Tornado under ESP (not project archive)

2. Best to look at GEN2Deploy3_Reagents spreadsheet.

3. Chris Preston described the process the spread sheetuses to plan reagents, pucks, etc.
4. Waste container is a fixed volume, Roman is setting what the volumes of waste 1 and waste 2 are.

5. Array map (depending upon species) generated manually now, the new printer will make the map automatically.

6. Number of probes on a given array may increase dramatically, like maybe up to 1000.

7. Outside agencies will need the array maps, but we will be generating the arrays (and the reagents to begin with.) 
8. Summary file generated manually from Log file (with keyword searching.)

9. QC data also put into the summary file

10. Image file name, type, date, hour, sample size, and imaging time.

11. Brent question on GG and CTD time stamp sets, and when sync’d?

12. Identifying puck and load position is labor intensive to make sure they (and the arrays they hold) are loaded correctly.
13. Eventually the location of the instrument on the map/overlay/GIS becomes important. The instruments may not always be moored, and a GPS location will be available for all machines. (Either within a watch circle or position as if on a drifter.)

14. There is risk of snowballing, but at this point we don’t want to make decisions that would preclude future capability/options.

