12/14/04

                               ACER RUN PROCEDURE

Red button out

Power on-wait for boot-up

F8-system reset

F1-all axis

Z – Z off-enter-  System homes

F8-Back page

F7-at abs. Zero? (upper line)

Z enter –Move? (if abs. Zero warning, then reboot) jog won’t work

Can now jog –set part, etc. now in manual mode (top left)

Set zero – X enter, Y enter  (resets abs zero’s)

-----To change tools, Z up max. lock - air chuck

