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                                   PRESSURE TEST OF PRESSURE HOUSINGS








FOR:   Norman Maher


When:   1/13/97-1/17/97





What:  2 OSMO housings,  (smaller diam.)  


            3 PISPPI housings, marked with #2,3,4





The above referenced housings were all brought to a pressure of 9000 p.s.i. at a rate of 600 p.s.i./minute.  They were held at 9000 p.s.i. for 3 minutes then returned to ambient for 1 cycle.  There was no evidence of deformation during or after the tests.   They were stamped  9 K  to affirm test level.





Original test sheets available upon request .





A copy of  the Certificate of Conformance is enclosed for the Autoclave Pressure transducer  used. 
