ALVIN GROUP                                                                                                                          1/20/04

RE:    Pressure Test Certification of ANTARES Data Loggers;  


S/N’s, 1854012, 1854017, 1854018, 1854019, 1854022, 1854030.

These items were subjected to 9X  (4300m water depth X  1.5 F.S. X 1.487~9600 psi) with a 10 min hold and a 10th cycle with a 1 hour hold at test pressure in accordance with  the alternative ALVIN procedure.     Please find attached a strip chart of the test sequence. 

Sincerely,          


        Jim Scholfield


        Sr. Mech. Technician


        MBARI


        831-775-1765

                       scji@mbari.org

