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Carl  Brandt


Velcon Filters











	Dear Carl,





Allen at Filtrex has contacted you regarding our problem with a leaky pair of Aquacon AC-409 SP filters.  Here are some additional details.





We changed our system to Tellus 22 oil for the hydraulic system on our new ROV  called Tiburon.  Tellus is more able to emulsify seawater than the Carnation Mineral Oil we were using.  Shortly after we started using the Tellus oil, the filters started leaking.  Our system only runs at 20 psi and the leaks seemed worse when the system was turned off, with only a 1-foot head from the reservoir as residual pressure. We tightened the filters, then  removed and inspected the seals and sealing surfaces, checked for cracks, distortions, checked the hose connections, etc. all to no avail.  There was no apparent cracking or swelling which would indicate a compatibility issue either.  We then replaced the filters with new ones.  Again, no relief.  Finally I noticed that the gaskets were thinner in height (0.200”) than the  older gaskets (0.235”) we had on the filters which had worked fine when we had used the original mineral oil.  Using the older, thicker gaskets has solved the problem so far, no leaks for the past 10 days.  The leak we were chasing was about a liter/day.  I would like to get  a stock of these older, thicker gaskets if no other remedy comes to light.  The thicker gaskets are 2.410” I.D., 0.235” Ht., and 0.170” section width.





Enclosed are 2 of the gaskets which were leaking and an MSDS for Tellus 22.  We appreciate your helping us out with this weird nuisance type problem.





Thanks,





      Jim Scholfield


