FOCE WING BAFFLE SECTION FASTENERS -  EACH ASSEMBLY    9/31/08

All SS 316       ¼ - 20  Hex Head bolts 

L.”
#

1  
6

2.5
4

2.75
58

3
36
most are threaded into tapped holes in Polycarbonate sheets

3.25
68

3.5
4

5
14

5.5
16

Totals- ¼ - 20 fasteners
¼” bolts
206

¼” washers
412
¼” nuts
188

OTHER  FASTENERS

2
5” x ½” – 13  bolts

2
½” – 13 Nylok Nuts

4
½” washers

6ft.
¼”-20 threaded rod for Syntactic foam

28
3/8” Barrel Nuts, threaded 10-32

6
1.5 x 10-32 Flat head screws

22
1.5 x 10-32 Pan head screws

