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PART	DESCRIPTION
V1	Hopkins S.W. Supply Isolation Valve
V2	MBARI S.W. Isolation Valve
V3	Check valve-Prevent back flow
V4	Check Valve
V5	Inlet Inlet Control Valve
V6	Tank Outlet Valve
V7	pH Bypass Inlet V.
V8	pH Bypass outlet V.
V9	Hose Over-Pressure Relief V. 
V10	Red Hose Valve
V11	Recirc Pump Supply
V12	Recirc Pump Outlet
V13	Tank Over-Pressure Relief V.
V14	Tank Vent V.
V15	Tank CO2 inlet V.
V16	Hose Pr. Relief V. isolation (Tank)
V17	Tank Drain V.
V18	Black Hose V.
V19	Back Pressure Relief Valve
V20	On Seaward Manifold
V21	On Seaward Manifold
V22	On Seaward Manifold
PART	DESCRIPTION

P1	S.W. Tank Supply Pump
[bookmark: _GoBack]P2	Peristaltic Hose Supply Pump
P3	S.W. Recirculation Pump
G1	Tank Gas Pressure (0-15 psi-typ.)
							
G2	Hose Pressure (0-40 psi)
G3	Inlet Pump PSI
G4	Recirc Pump PSI
F1	Inlet Water filter
F2 	Recirc Water filter
F3	Hose discharge Filter
RTD	enhanced S.W. Temp Sensor
pH Meter – enh. S.W. pH



