                 LABVIEW BASED CONTROL IN PRESSURE TEST FACILITY                               2/7/05

RECOMMENDED HARDWARE

P/N

COST est.
NOTES:

NI cFP-2010

1,595

2020 not nec. because don’t need 485 comm’s port

NI cFP-BP4

   350

4 slot backplane

      PS-5


   250

24VDC power supply

NI cFP-AIO-600                   600

8 channel Analog IO, provide 4-20 ma and 0-20ma    which         can be converted to 0-10 VDC to drive the strip chart recorder

NI cFP-RLY-421                  250

Drive 120VAC solonoids

NI cFP-I-100                         425

General analog input, ma and 0-30VDC

NI cFP-CB-1                         150  

Gen. Prupose Connector Block, optional use cofig.

SH 37F-P-4                             45  x 2=90       Cable with pigtails, 1 for each       

                SUBTOTAL    $ 3,710

Specific for Pressure Test

SOFTWARE                                                   We already have this in-house (Eric) so we can buy our own later.

BASE LABVIEW                       995

REAL TIME MODULE          1,995

                 SUBTOTAL          $2,990

                  TRAINING             1500
Est. for Real -Time System using Field Point

                          TOTAL        $8200


