                                                                                                                                 8/5/99

GERHARDT GEAR – 818-842-1458 (fax),  818-842-6700

Attn:  Fritz

Ref: telecon with Mitch, 8/5/99

                                          PUMP DRIVE ADAPTOR SHAFT

This adapts a 5/8” keyed shaft hydraulic motor to a an internally splined input shaft on a centrifugal pump.

Mat’l- S.S.,  .625” diam.

Shaft Length – 2.5” if possible,  this is not a hard requirement.

One end will need a key way to receive a 0 .7” long,  std. .155” square key.  The other to be fabricated into a 14 tooth involute spline described on the next page.

Please provide  a quote for 5 pieces, splined and keyed as described.

Thanks,

                   Jim Scholfield          831-775-1765

