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OCEAN ENGINEERING DEPARTMENT
ELECTRICAL FABRICATION WORK REQUEST

	Originator
	Brenton Salmi

	Project
	MARS2

	Job Description
	Rework board to final version

	Submitted Date
	10/17/2024

	Estimated Hours
	2

	Desired Completion Date
	10/23/2024

	Worktag
	AC103988



Drawing file paths and names:

· BOB V2 Altium 365 Page:
· https://applied-physics-lab.365.altium.com/designs/96784F5C-C826-43BF-A453-D7CE2F0ACD9C?activeView=SCH&variant=[No+Variations]&activeDocumentId=Coversheet.SchDoc(1)&location=[1,98.47,15.41,19.94]#design 

Work Description

High Level

· Components will be DNP’d
· Components will be installed

DNP Component(s)

	REF DES
	QTY Total

	TP1
	1






Install Flywire(s)

· Use 30AWG for the flywires
· Stake the wires using hot-glue as appropriate

The final result should look something like this except that TP1 will be removed:
[image: ]



Between TP1 and C1A(PIN2 – TP19A)
Insert the flywire into the TP1 through hole.

[image: ]

Between C1A(PIN2 – TP19A) and C1D(PIN2 – TP19D)

[image: ]

Between C1D(PIN2 – TP19D) and C1C(PIN2 – TP19C)
[image: ]

Between C1C(PIN2 – TP19C) and C1B(PIN2 – TP19B)

[image: ]


Final

Clean the boards accordingly.
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