MARS Fluorinert Safety Equipment
1. FC-77 Wash Apparatus – Used when de-composition of the FC-77 is suspected.  De-composition of FC-77 can result in the production of Hydrogen Fluoride and Perfluoroisobutylene (PFIB).
1. TBD – Chemical protective gear to protect operator when dealing with FC-77 breakdown.

