Jon Uebel

Bayside Motion Group

516.484.5353 Ph.

516.484.5496 Fax

Dear Jon,

We have picked our first motor to design with for the AUV project. It’s an Aveox 1817/3Y.

The optimum gear ratio is 21-22:1. The PS40 lists a 20:1 and a 25:1 ratio. The AUV application requires 200 Rpm at 4.8 N-m to the prop. 

Can we get a quotation for a PS40 20:1 and a PS40 25:1 with adapter for the Aveox 1817/3Y. The Aveox drawings are included with this fax. I hope drawings are readable at your end. If not, let me know and I’ll get Aveox to mail them direct to you.

The distributor we started to work with no longer represents Bayside. Will you recommend another distributor to place the order for the gearbox.

Sincerely,

Gary Thurmond

831.775.1735 Ph

831.775.1646 Fax

thga@mbari.org 

