MARS-router#show conf
Using 22795 out of 524288 bytes
!
! Last configuration change at 21:41:41 UTC Wed Mar 28 2018
! NVRAM config last updated at 21:41:45 UTC Wed Mar 28 2018
!
version 12.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname MARS-router
!
boot-start-marker
boot-end-marker
!
enable secret 5 $1$KV0q$N67FzMrx3xBVCpo.rNiwX.
enable password 7 112E0C441941181F45
!
!
!
no aaa new-model
switch 1 provision ws-c3750g-24ts
system mtu routing 1500
ip routing
ip cef load-sharing algorithm universal 564A8012
ip domain-list marsobs.net
no ip domain-lookup
ip domain-name marsobs.net
ip name-server 10.91.128.61
!
!
ip multicast-routing distributed
!
!
crypto pki trustpoint TP-self-signed-4181914112
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-4181914112
 revocation-check none
 rsakeypair TP-self-signed-4181914112
!
!
crypto pki certificate chain TP-self-signed-4181914112
 certificate self-signed 01 nvram:IOS-Self-Sig#3232.cer
!
!
!
!
spanning-tree mode mst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
ip ftp source-interface Vlan128
ip ftp username mars
ip ftp password 7 130B12021F190A2F7A
!
!
!
interface Loopback1
 no ip address
!
interface GigabitEthernet1/0/1
 switchport trunk encapsulation dot1q
 switchport trunk native vlan 128
 switchport mode trunk
!
interface GigabitEthernet1/0/2
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/3
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/4
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/5
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/6
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/7
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/8
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/9
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/10
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/11
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/12
 switchport access vlan 128
 switchport mode access
!         
interface GigabitEthernet1/0/13
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/14
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/15
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/16
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/17
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/18
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/19
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/20
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/21
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/22
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/23
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/24
 switchport access vlan 128
 switchport mode access
!
interface GigabitEthernet1/0/25
 switchport trunk encapsulation dot1q
 switchport trunk native vlan 128
 switchport mode trunk
!
interface GigabitEthernet1/0/26
 switchport trunk encapsulation dot1q
 switchport trunk native vlan 128
 switchport mode trunk
!
interface GigabitEthernet1/0/27
 switchport trunk encapsulation dot1q
 switchport trunk native vlan 128
 switchport mode trunk
!
interface GigabitEthernet1/0/28
 switchport trunk encapsulation dot1q
 switchport trunk native vlan 128
 switchport mode trunk
!
interface Vlan1
 no ip address
!
interface Vlan3
 description EXTERNAL VLAN (to firewall/INTERNET)
 ip address 10.91.3.1 255.255.255.0
!
interface Vlan4
 description SHORESTATION SCIENCE HOSTING VLAN
 ip address 10.91.4.1 255.255.255.0
 ip helper-address 10.91.128.51
!
interface Vlan11
 description SCIENCE PORT 1 VLAN
 ip address 10.1.11.1 255.255.255.128
 ip access-group 111 in
!
interface Vlan12
 description SCIENCE PORT 2 VLAN
 ip address 10.1.12.1 255.255.255.0
 ip access-group 112 in
!
interface Vlan13
 description SCIENCE PORT 3 VLAN
 ip address 10.1.13.1 255.255.255.0
 ip access-group 113 in
!
interface Vlan14
 description SCIENCE PORT 4 VLAN
 ip address 10.1.14.1 255.255.255.0
 ip access-group 114 in
 ip pim version 1
 ip pim sparse-dense-mode
!
interface Vlan15
 description SCIENCE PORT 5 VLAN
 ip address 10.1.15.1 255.255.255.0
 ip access-group 115 in
!
interface Vlan16
 description SCIENCE PORT 6 VLAN
 ip address 10.1.16.1 255.255.255.0
 ip access-group 116 in
!
interface Vlan17
 description SCIENCE PORT 7 VLAN
 ip address 10.1.17.1 255.255.255.0
 ip access-group 117 in
!
interface Vlan18
 description SCIENCE PORT 8 VLAN
 ip address 10.1.18.1 255.255.255.0
 ip access-group 118 in
!
interface Vlan41
 description SHORESTATION SCIENCE VLAN 1
 ip address 10.91.41.1 255.255.255.0
 ip access-group 123 in
 ip helper-address 10.91.128.51
!
interface Vlan42
 description SHORESTATION SCIENCE VLAN 2
 ip address 10.91.42.1 255.255.255.0
 ip access-group 121 in
 ip helper-address 10.91.128.51
!
interface Vlan43
 description SHORESTATION SCIENCE VLAN 3
 ip address 10.91.43.1 255.255.255.0
 ip access-group 131 in
 ip helper-address 10.91.128.51
!
interface Vlan44
 description SHORESTATION SCIENCE VLAN 4
 ip address 10.91.44.1 255.255.255.0
 ip access-group 141 in
 ip helper-address 10.91.128.51
!
interface Vlan45
 description SHORESTATION SCIENCE VLAN 5
 ip address 10.91.45.1 255.255.255.0
 ip access-group 151 in
 ip helper-address 10.91.128.51
!
interface Vlan46
 description SHORESTATION SCIENCE VLAN 6
 ip address 10.91.46.1 255.255.255.0
 ip access-group 161 in
 ip helper-address 10.91.128.51
!
interface Vlan47
 description SHORESTATION SCIENCE VLAN 7
 ip address 10.91.47.1 255.255.255.0
 ip access-group 171 in
 ip helper-address 10.91.128.51
!
interface Vlan48
 description SHORESTATION SCIENCE VLAN 8
 ip address 10.91.48.1 255.255.255.0
 ip access-group 181 in
 ip helper-address 10.91.128.51
!
interface Vlan127
 description SUBSEA MANAGEMENT LAN
 ip address 10.1.128.1 255.255.255.0
 ip access-group 199 in
!
interface Vlan128
 description MANAGEMENT VLAN
 ip address 10.91.128.1 255.255.255.0
 ip access-group 199 in
 ip pim sparse-dense-mode
!
interface Vlan911
 no ip address
!
router ospf 10
 log-adjacency-changes
 redistribute eigrp 10     
 network 10.0.0.0 0.0.0.255 area 0
!
router rip
 network 10.0.0.0
!
ip classless
ip route 0.0.0.0 0.0.0.0 10.91.128.12
ip http server
ip http secure-server
!
!
ip sla enable reaction-alerts
access-list 111 permit tcp any any established
access-list 111 permit icmp any any echo-reply
access-list 111 permit ip any host 10.91.128.55
access-list 111 permit tcp any host 10.91.128.15 eq 123
access-list 111 permit udp any host 10.91.128.15 eq ntp
access-list 111 permit tcp any host 10.91.128.61 eq domain
access-list 111 permit tcp any host 10.91.128.62 eq domain
access-list 111 permit udp any host 10.91.128.61 eq domain
access-list 111 permit udp any host 10.91.128.62 eq domain
access-list 111 permit ip any 10.91.41.0 0.0.0.255
access-list 111 deny   ip any 10.1.0.0 0.0.255.255
access-list 111 deny   ip any 10.91.0.0 0.0.255.255
access-list 111 deny   ip any 10.91.253.0 0.0.0.255
access-list 111 permit icmp any 10.1.11.0 0.0.0.255
access-list 111 deny   icmp any 10.1.0.0 0.0.255.255
access-list 111 deny   icmp any 10.91.128.0 0.0.0.255
access-list 111 deny   icmp any 10.1.253.0 0.0.0.255
access-list 111 permit ip any any
access-list 111 permit icmp any any
access-list 112 permit tcp any any established
access-list 112 permit icmp any any echo-reply
access-list 112 permit ip any host 10.91.128.55
access-list 112 permit tcp any host 10.91.128.15 eq 123
access-list 112 permit udp any host 10.91.128.15 eq ntp
access-list 112 permit tcp any host 10.91.128.61 eq domain
access-list 112 permit tcp any host 10.91.128.62 eq domain
access-list 112 permit udp any host 10.91.128.61 eq domain
access-list 112 permit udp any host 10.91.128.62 eq domain
access-list 112 permit ip any 10.91.42.0 0.0.0.255
access-list 112 deny   ip any 10.1.0.0 0.0.255.255
access-list 112 deny   ip any 10.91.0.0 0.0.25.255
access-list 112 deny   ip any 10.91.253.0 0.0.0.255
access-list 112 permit icmp any 10.1.12.0 0.0.0.255
access-list 112 deny   icmp any 10.1.0.0 0.0.255.255
access-list 112 deny   icmp any 10.91.128.0 0.0.0.255
access-list 112 deny   icmp any 10.1.253.0 0.0.0.255
access-list 112 permit ip any any
access-list 112 permit icmp any any
access-list 113 permit tcp any any established
access-list 113 permit icmp any any echo-reply
access-list 113 permit ip any host 10.91.128.55
access-list 113 permit tcp any host 10.91.128.15 eq 123
access-list 113 permit udp any host 10.91.128.15 eq ntp
access-list 113 permit tcp any host 10.91.128.61 eq domain
access-list 113 permit tcp any host 10.91.128.62 eq domain
access-list 113 permit udp any host 10.91.128.61 eq domain
access-list 113 permit udp any host 10.91.128.62 eq domain
access-list 113 permit ip any 10.91.43.0 0.0.0.255
access-list 113 deny   ip any 10.1.0.0 0.0.255.255
access-list 113 deny   ip any 10.91.0.0 0.0.255.255
access-list 113 deny   ip any 10.91.253.0 0.0.0.255
access-list 113 permit icmp any 10.1.13.0 0.0.0.255
access-list 113 deny   icmp any 10.1.0.0 0.0.255.255
access-list 113 deny   icmp any 10.91.128.0 0.0.0.255
access-list 113 deny   icmp any 10.1.253.0 0.0.0.255
access-list 113 permit ip any any
access-list 113 permit icmp any any
access-list 114 permit tcp any any established
access-list 114 permit icmp any any echo-reply
access-list 114 permit udp host 10.1.14.4 any
access-list 114 permit ip any host 10.91.128.55
access-list 114 permit tcp any host 10.91.128.15 eq 123
access-list 114 permit udp any host 10.91.128.15 eq ntp
access-list 114 permit tcp any host 10.91.128.61 eq domain
access-list 114 permit tcp any host 10.91.128.62 eq domain
access-list 114 permit udp any host 10.91.128.61 eq domain
access-list 114 permit udp any host 10.91.128.62 eq domain
access-list 114 permit ip any 10.91.44.0 0.0.0.255
access-list 114 deny   ip any 10.1.0.0 0.0.255.255
access-list 114 deny   ip any 10.91.0.0 0.0.255.255
access-list 114 deny   ip any 10.91.253.0 0.0.0.255
access-list 114 permit icmp any 10.1.14.0 0.0.0.255
access-list 114 deny   icmp any 10.1.0.0 0.0.255.255
access-list 114 deny   icmp any 10.91.128.0 0.0.0.255
access-list 114 deny   icmp any 10.1.253.0 0.0.0.255
access-list 114 permit ip any any
access-list 114 permit icmp any any
access-list 115 permit tcp any any established
access-list 115 permit icmp any any echo-reply
access-list 115 permit ip any host 10.91.128.55
access-list 115 permit tcp any host 10.91.128.15 eq 123
access-list 115 permit udp any host 10.91.128.15 eq ntp
access-list 115 permit tcp any host 10.91.128.61 eq domain
access-list 115 permit tcp any host 10.91.128.62 eq domain
access-list 115 permit udp any host 10.91.128.61 eq domain
access-list 115 permit udp any host 10.91.128.62 eq domain
access-list 115 permit ip any 10.91.45.0 0.0.0.255
access-list 115 deny   ip any 10.1.0.0 0.0.255.255
access-list 115 deny   ip any 10.91.0.0 0.0.255.255
access-list 115 deny   ip any 10.91.253.0 0.0.0.255
access-list 115 permit icmp any 10.1.15.0 0.0.0.255
access-list 115 deny   icmp any 10.1.0.0 0.0.255.255
access-list 115 deny   icmp any 10.91.128.0 0.0.0.255
access-list 115 deny   icmp any 10.1.253.0 0.0.0.255
access-list 115 permit ip any any
access-list 115 permit icmp any any
access-list 116 permit tcp any any established
access-list 116 permit icmp any any echo-reply
access-list 116 permit ip any host 10.91.128.55
access-list 116 permit tcp any host 10.91.128.15 eq 123
access-list 116 permit udp any host 10.91.128.15 eq ntp
access-list 116 permit tcp any host 10.91.128.61 eq domain
access-list 116 permit tcp any host 10.91.128.62 eq domain
access-list 116 permit udp any host 10.91.128.61 eq domain
access-list 116 permit udp any host 10.91.128.62 eq domain
access-list 116 permit ip any 10.91.46.0 0.0.0.255
access-list 116 deny   ip any 10.1.0.0 0.0.255.255
access-list 116 deny   ip any 10.91.0.0 0.0.255.255
access-list 116 deny   ip any 10.91.253.0 0.0.0.255
access-list 116 permit icmp any 10.1.16.0 0.0.0.255
access-list 116 deny   icmp any 10.1.0.0 0.0.255.255
access-list 116 deny   icmp any 10.91.128.0 0.0.0.255
access-list 116 deny   icmp any 10.1.253.0 0.0.0.255
access-list 116 permit ip any any
access-list 116 permit icmp any any
access-list 117 permit tcp any any established
access-list 117 permit icmp any any echo-reply
access-list 117 permit ip any host 10.91.128.55
access-list 117 permit tcp any host 10.91.128.15 eq 123
access-list 117 permit udp any host 10.91.128.15 eq ntp
access-list 117 permit tcp any host 10.91.128.61 eq domain
access-list 117 permit tcp any host 10.91.128.62 eq domain
access-list 117 permit udp any host 10.91.128.61 eq domain
access-list 117 permit udp any host 10.91.128.62 eq domain
access-list 117 permit ip any 10.91.47.0 0.0.0.255
access-list 117 deny   ip any 10.1.0.0 0.0.255.255
access-list 117 deny   ip any 10.91.0.0 0.0.255.255
access-list 117 deny   ip any 10.91.253.0 0.0.0.255
access-list 117 permit icmp any 10.1.17.0 0.0.0.255
access-list 117 deny   icmp any 10.1.0.0 0.0.255.255
access-list 117 deny   icmp any 10.91.128.0 0.0.0.255
access-list 117 deny   icmp any 10.1.253.0 0.0.0.255
access-list 117 permit ip any any
access-list 117 permit icmp any any
access-list 118 permit tcp any any established
access-list 118 permit icmp any any echo-reply
access-list 118 permit ip any host 10.91.128.55
access-list 118 permit tcp any host 10.91.128.15 eq 123
access-list 118 permit udp any host 10.91.128.15 eq ntp
access-list 118 permit tcp any host 10.91.128.61 eq domain
access-list 118 permit tcp any host 10.91.128.62 eq domain
access-list 118 permit udp any host 10.91.128.61 eq domain
access-list 118 permit udp any host 10.91.128.62 eq domain
access-list 118 permit ip any 10.91.48.0 0.0.0.255
access-list 118 deny   ip any 10.1.0.0 0.0.255.255
access-list 118 deny   ip any 10.91.0.0 0.0.255.255
access-list 118 deny   ip any 10.91.253.0 0.0.0.255
access-list 118 permit icmp any 10.1.18.0 0.0.0.255
access-list 118 deny   icmp any 10.1.0.0 0.0.255.255
access-list 118 deny   icmp any 10.91.128.0 0.0.0.255
access-list 118 deny   icmp any 10.1.253.0 0.0.0.255
access-list 118 permit ip any any
access-list 118 permit icmp any any
access-list 121 permit tcp any any established
access-list 121 permit icmp any any echo-reply
access-list 121 permit ip any host 10.91.128.55
access-list 121 permit tcp any host 10.91.128.15 eq 123
access-list 121 permit udp any host 10.91.128.15 eq ntp
access-list 121 permit tcp any host 10.91.128.61 eq domain
access-list 121 permit tcp any host 10.91.128.62 eq domain
access-list 121 permit udp any host 10.91.128.61 eq domain
access-list 121 permit udp any host 10.91.128.62 eq domain
access-list 121 permit ip any 10.1.12.0 0.0.0.255
access-list 121 deny   ip any 10.1.0.0 0.0.255.255
access-list 121 deny   ip any 10.91.128.0 0.0.0.255
access-list 121 deny   ip any 10.91.253.0 0.0.0.255
access-list 121 permit icmp any 10.1.12.0 0.0.0.255
access-list 121 deny   icmp any 10.1.0.0 0.0.255.255
access-list 121 deny   icmp any 10.91.128.0 0.0.0.255
access-list 121 deny   icmp any 10.91.253.0 0.0.0.255
access-list 121 permit ip any any
access-list 121 permit icmp any any
access-list 123 permit tcp any any established
access-list 123 permit icmp any any echo-reply
access-list 123 permit ip any host 10.91.128.55
access-list 123 permit tcp any host 10.91.128.15 eq 123
access-list 123 permit udp any host 10.91.128.15 eq ntp
access-list 123 permit tcp any host 10.91.128.61 eq domain
access-list 123 permit tcp any host 10.91.128.62 eq domain
access-list 123 permit udp any host 10.91.128.61 eq domain
access-list 123 permit udp any host 10.91.128.62 eq domain
access-list 123 permit ip any 10.1.11.0 0.0.0.255
access-list 123 deny   ip any 10.1.0.0 0.0.255.255
access-list 123 deny   ip any 10.91.128.0 0.0.0.255
access-list 123 deny   ip any 10.91.253.0 0.0.0.255
access-list 123 permit icmp any 10.1.11.0 0.0.0.255
access-list 123 deny   icmp any 10.1.0.0 0.0.255.255
access-list 123 deny   icmp any 10.91.128.0 0.0.0.255
access-list 123 deny   icmp any 10.91.253.0 0.0.0.255
access-list 123 permit ip any any
access-list 123 permit icmp any any
access-list 131 permit tcp any any established
access-list 131 permit icmp any any echo-reply
access-list 131 permit ip any host 10.91.128.55
access-list 131 permit tcp any host 10.91.128.15 eq 123
access-list 131 permit udp any host 10.91.128.15 eq ntp
access-list 131 permit tcp any host 10.91.128.61 eq domain
access-list 131 permit tcp any host 10.91.128.62 eq domain
access-list 131 permit udp any host 10.91.128.61 eq domain
access-list 131 permit udp any host 10.91.128.62 eq domain
access-list 131 permit ip any 10.1.13.0 0.0.0.255
access-list 131 deny   ip any 10.1.0.0 0.0.255.255
access-list 131 deny   ip any 10.91.128.0 0.0.0.255
access-list 131 deny   ip any 10.91.253.0 0.0.0.255
access-list 131 permit icmp any 10.1.13.0 0.0.0.255
access-list 131 deny   icmp any 10.1.0.0 0.0.255.255
access-list 131 deny   icmp any 10.91.128.0 0.0.0.255
access-list 131 deny   icmp any 10.91.253.0 0.0.0.255
access-list 131 permit ip any any
access-list 131 permit icmp any any
access-list 141 permit tcp any any established
access-list 141 permit icmp any any echo-reply
access-list 141 permit ip any host 10.91.128.55
access-list 141 permit tcp any host 10.91.128.15 eq 123
access-list 141 permit udp any host 10.91.128.15 eq ntp
access-list 141 permit tcp any host 10.91.128.61 eq domain
access-list 141 permit tcp any host 10.91.128.62 eq domain
access-list 141 permit udp any host 10.91.128.61 eq domain
access-list 141 permit udp any host 10.91.128.62 eq domain
access-list 141 permit ip any 10.1.14.0 0.0.0.255
access-list 141 deny   ip any 10.1.0.0 0.0.255.255
access-list 141 deny   ip any 10.91.128.0 0.0.0.255
access-list 141 deny   ip any 10.91.253.0 0.0.0.255
access-list 141 permit icmp any 10.1.14.0 0.0.0.255
access-list 141 deny   icmp any 10.1.0.0 0.0.255.255
access-list 141 deny   icmp any 10.91.128.0 0.0.0.255
access-list 141 deny   icmp any 10.91.253.0 0.0.0.255
access-list 141 permit ip any any
access-list 141 permit icmp any any
access-list 151 permit tcp any any established
access-list 151 permit icmp any any echo-reply
access-list 151 permit ip any host 10.91.128.55
access-list 151 permit tcp any host 10.91.128.15 eq 123
access-list 151 permit udp any host 10.91.128.15 eq ntp
access-list 151 permit tcp any host 10.91.128.61 eq domain
access-list 151 permit tcp any host 10.91.128.62 eq domain
access-list 151 permit udp any host 10.91.128.61 eq domain
access-list 151 permit udp any host 10.91.128.62 eq domain
access-list 151 permit ip any 10.1.15.0 0.0.0.255
access-list 151 deny   ip any 10.1.0.0 0.0.255.255
access-list 151 deny   ip any 10.91.128.0 0.0.0.255
access-list 151 deny   ip any 10.91.253.0 0.0.0.255
access-list 151 permit icmp any 10.1.15.0 0.0.0.255
access-list 151 deny   icmp any 10.1.0.0 0.0.255.255
access-list 151 deny   icmp any 10.91.128.0 0.0.0.255
access-list 151 deny   icmp any 10.91.253.0 0.0.0.255
access-list 151 permit ip any any
access-list 151 permit icmp any any
access-list 161 permit tcp any any established
access-list 161 permit icmp any any echo-reply
access-list 161 permit ip any host 10.91.128.55
access-list 161 permit tcp any host 10.91.128.15 eq 123
access-list 161 permit udp any host 10.91.128.15 eq ntp
access-list 161 permit tcp any host 10.91.128.61 eq domain
access-list 161 permit tcp any host 10.91.128.62 eq domain
access-list 161 permit udp any host 10.91.128.61 eq domain
access-list 161 permit udp any host 10.91.128.62 eq domain
access-list 161 permit ip any 10.1.16.0 0.0.0.255
access-list 161 deny   ip any 10.1.0.0 0.0.255.255
access-list 161 deny   ip any 10.91.128.0 0.0.0.255
access-list 161 deny   ip any 10.91.253.0 0.0.0.255
access-list 161 permit icmp any 10.1.16.0 0.0.0.255
access-list 161 deny   icmp any 10.1.0.0 0.0.255.255
access-list 161 deny   icmp any 10.91.128.0 0.0.0.255
access-list 161 deny   icmp any 10.91.253.0 0.0.0.255
access-list 161 permit ip any any
access-list 161 permit icmp any any
access-list 171 permit tcp any any established
access-list 171 permit icmp any any echo-reply
access-list 171 permit ip any host 10.91.128.55
access-list 171 permit tcp any host 10.91.128.15 eq 123
access-list 171 permit udp any host 10.91.128.15 eq ntp
access-list 171 permit tcp any host 10.91.128.61 eq domain
access-list 171 permit tcp any host 10.91.128.62 eq domain
access-list 171 permit udp any host 10.91.128.61 eq domain
access-list 171 permit udp any host 10.91.128.62 eq domain
access-list 171 permit ip any 10.1.17.0 0.0.0.255
access-list 171 deny   ip any 10.1.0.0 0.0.255.255
access-list 171 deny   ip any 10.91.128.0 0.0.0.255
access-list 171 deny   ip any 10.91.253.0 0.0.0.255
access-list 171 permit icmp any 10.1.17.0 0.0.0.255
access-list 171 deny   icmp any 10.1.0.0 0.0.255.255
access-list 171 deny   icmp any 10.91.128.0 0.0.0.255
access-list 171 deny   icmp any 10.91.253.0 0.0.0.255
access-list 171 permit ip any any
access-list 171 permit icmp any any
access-list 181 permit tcp any any established
access-list 181 permit icmp any any echo-reply
access-list 181 permit ip any host 10.91.128.55
access-list 181 permit tcp any host 10.91.128.15 eq 123
access-list 181 permit udp any host 10.91.128.15 eq ntp
access-list 181 permit tcp any host 10.91.128.61 eq domain
access-list 181 permit tcp any host 10.91.128.62 eq domain
access-list 181 permit udp any host 10.91.128.61 eq domain
access-list 181 permit udp any host 10.91.128.62 eq domain
access-list 181 permit ip any 10.1.18.0 0.0.0.255
access-list 181 deny   ip any 10.1.0.0 0.0.255.255
access-list 181 deny   ip any 10.91.128.0 0.0.0.255
access-list 181 deny   ip any 10.91.253.0 0.0.0.255
access-list 181 permit icmp any 10.1.18.0 0.0.0.255
access-list 181 deny   icmp any 10.1.0.0 0.0.255.255
access-list 181 deny   icmp any 10.91.128.0 0.0.0.255
access-list 181 deny   icmp any 10.91.253.0 0.0.0.255
access-list 181 permit ip any any
access-list 181 permit icmp any any
access-list 199 permit ip any any
access-list 199 permit icmp any any
!
!
!
line con 0
line vty 0 4
 exec-timeout 0 0
 password 7 06211A60421D1A0A44
 login
line vty 5 15
 login
!
ntp clock-period 36028785
ntp server 10.91.128.55 key 99 prefer
ntp server 10.91.128.56 key 99
end