MARS MVC Testing
MBARI is taking delivery of the version 4 MVC from Alcatel.  The MVC will be operated with a 10,000 volt input as part of the acceptance testing.  The testing will take place in the MARS lab in building D.  Due to the nature of some of the system components, dangerous voltage levels can persist for extended periods of time even after the system is powered off.  No one should attempt to enter the MARS lab without approval from Ken Heller, Craig Dawe or Ed Mellinger.  10,000 volt operation will begin as early as today (3/19/2010) and may continue through 3/29/2010.
