MARS External Loads 1-8  SSDS DeviceIDs 1772 thru 1779
 (only one load described here, feilds are the same for each load)

 Sample Record:
 1291017601, -51.399, 1, 0, 0, 135.998, 1, 0, 0, 371566.8, 1940.9, 47753.9, 282.3,  2010-11-29T08:00:01Z

 1 name="Timestamp" longName="Unix epoch seconds" units="seconds"
 2 name="v375_current" longName="v375_current" units="milliAmperes"
 3 name="v375_pwr_fet" longName="v375_pwr_fet" units=""
 4 name="v375_deadface_relay" longName="v375_deadface_relay" units=""
 5 name="v375_hardware_overcurrent" longName="v375_hardware_overcurrent" units=""
 6 name="v48_current" longName="v48_current" units="milliAmperes"
 7 name="v48_pwr_fet" longName="v48_pwr_fet" units=""
 8 name="v48_deadface_relay" longName="v48_deadface_relay" units=""
 9 name="v48_hardware_overcurrent" longName="v48_hardware_overcurrent" units=""
 10 name="external_bus_v375_voltage" longName="external_bus_v375_voltage" units="milliVolts"
 11 name="external_bus_v375_current" longName="external_bus_v375_current" units="milliAmperes"
 12 name="external_bus_v48_voltage" longName="external_bus_v48_voltage" units="milliVolts"
 13 name="external_bus_v48_current" longName="external_bus_v48_current" units="milliAmperes"
 14 name="DateTime" longName="ISO-8601 DateTime of Sample" units="yyyy-MM-ddThh:mm:ssZ"

 -------------------------------------------------------
 MARS Ground Fault  SSDS Device 1780
 Sample Record:
 1291017678, 15.3, 11.2, 4.8, 1.5, 0.0, 2010-11-29T08:01:18Z

 1 name="Timestamp" longName="Unix epoch seconds" units="seconds"
 2 name="v375" longName="v375" units="milliAmperes"
 3 name="v375r" longName="v375r" units="milliAmperes"
 4 name="v48" longName="v48" units="milliAmperes"
 5 name="v48r" longName="v48r" units="milliAmperes"
 6 name="test" longName="test" units="milliAmperes"
 7 name="DateTime" longName="ISO-8601 DateTime of Sample" units="yyyy-MM-ddThh:mm:ssZ"

 -------------------------------------------------------
 MARS Onewire HA7   SSDS DeviceID 1781

 Sample Record:
 1299142800, 18.438, 12.500, 11.625, 20.125, 14.312, 7.000, 5.688, 10.125, 9.875, -99.999, 10.438, 10.625, 2011-03-3T09:00:00Z

 1 name="Timestamp" longName="Unix epoch seconds" units="seconds"
 2 name="NE_East" longName="NE_East" units="deg C"
 3 name="West_Edfa" longName="West_Edfa" units="deg C"
 4 name="East_Edfa" longName="East_Edfa" units="deg C"
 5 name="NE_West" longName="NE_West" units="deg C"
 6 name="East_Edfa_Two" longName="East_Edfa_Two" units="deg C"
 7 name="Below_Dry_Chassis" longName="Below_Dry_Chassis" units="deg C"
 8 name="Below_Ciscos" longName="Below_Ciscos" units="deg C"
 9 name="Above_Ciscos_Outboard" longName="Above_Ciscos_Outboard" units="deg C"
 10 name="Above_XDC" longName="Above_XDC" units="deg C"
 11 name="Above_Ciscos_Inboard" longName="Above_Ciscos_Inboard" units="deg C"
 12 name="Above_XLC" longName="Above_XLC" units="deg C"
 13 name="Above_ILC" longName="Above_ILC" units="deg C"
 14 name="DateTime" longName="ISO-8601 DateTime of Sample" units="yyyy-MM-ddThh:mm:ssZ"

 -------------------------------------------------------
 MARS PSC  SSDS DeviceID 1782

 Sample Record:
 1337590851,-7252,176,1,2012-05-21T09:00:51Z

 1 name="Timestamp" longName="Unix epoch seconds" units="seconds"
 2 name="Voltage" longName="Voltage" units="Volts"
 3 name="Current" longName="Current" units="milliAmperes"
 4 name="State" longName="HV Output State" units=""
 5 name="DateTime" longName="ISO-8601 DateTime of Sample" units="yyyy-MM-ddThh:mm:ssZ"

 -------------------------------------------------------

 MARS LVC  SSDS DeviceID 1783

 Sample Record:
 1338669257, 227.966, 5.798, 5307.007, 5293.274, 252.380, 703.430, 219.727, 219.116, 246.582, 447.998, 78.430, -14.954, 48.914, 54.932, 2.441, 10.071, 0, 1, 0, 0, 0, 0, 0, 0, 0, 0, 0, 1, 0, 0, 1, 1, 371520.996, 1593.018, 47810.669, 140.381, 47100.220, 2721.252, 5169.106, 11819.000, 16.556, 10.483, 55.319, 17.578, 15.045, 2012-06-02 20:34:17

 1 name="Timestamp" longName="Unix epoch seconds" units="seconds"
 2 name="HA7_current" longName="HA7 ILC1 current" units="milliAmperes"
 3 name="Spare2_current" longName="Spare2 ILC2 current" units="milliAmperes"
 4 name="Cisco1_current" longName="Cisco1 ILC3 current" units="milliAmperes"
 5 name="Cisco2_current" longName="Cisco2 ILC4 current" units="milliAmperes"
 6 name="OE_W75_current" longName="OE W75 ILC11 current" units="milliAmperes"
 7 name="Cyclades_current" longName="Cyclades ILC15 current" units="milliAmperes"
 8 name="OE_E75_current" longName="OE E75 ILC7 current" units="milliAmperes"
 9 name="OE_E98_current" longName="OE E98 ILC8 current" units="milliAmperes"
 10 name="OE_W98_current" longName="OE W98 ILC12 current" units="milliAmperes"
 11 name="NE_Switch_West_current" longName="NE Switch West ILC9 current" units="milliAmperes"
 12 name="EDFA_West_current" longName="EDFA West ILC10 current" units="milliAmperes"
 13 name="Spare12_current" longName="Spare ILC16 current" units="milliAmperes"
 14 name="NE_East_current" longName="NE East ILC5 current" units="milliAmperes"
 15 name="EDFA_East_current" longName="EDFA East ILC6 current" units="milliAmperes"
 16 name="OBCA_current" longName="OBCA ILC13 current" units="milliAmperes"
 17 name="OBCB_current" longName="OBCB ILC14 current" units="milliAmperes"
 18 name="HA7_power" longName="HA7 power switch" units=""
 19 name="Spare2_power" longName="Spare2 power switch" units=""
 20 name="Cisco1_power" longName="Cisco1 power switch" units=""
 21 name="Cisco2_power" longName="Cisco2 power switch" units=""
 22 name="OE_W75_power" longName="OE W75 power switch" units=""
 23 name="Cyclades_power" longName="Cyclades power switch" units=""
 24 name="OE_E75_power" longName="OE E75 power switch" units=""
 25 name="OE_E98_power" longName="OE E98 power switch" units=""
 26 name="OE_W98_power" longName="OE W98 power switch" units=""
 27 name="NE_West_power" longName="NE West power switch" units=""
 28 name="EDFA_West_power" longName="EDFA West power switch" units=""
 29 name="Spare12_power" longName="Spare12 power switch" units=""
 30 name="NE_East_power" longName="NE East power switch" units=""
 31 name="EDFA_East_power" longName="EDFA East power switch" units=""
 32 name="OBCA_power" longName="OBCA power switch" units=""
 33 name="OBCB_power" longName="OBCB power switch" units=""
 34 name="external_bus_v375_voltage" longName="external_bus_v375_voltage" units="milliVolts"
 35 name="external_bus_v375_current" longName="external_bus_v375_current" units="milliAmperes"
 36 name="external_bus_v48_voltage" longName="external_bus_v48_voltage" units="milliVolts"
 37 name="external_bus_v48_current" longName="external_bus_v48_current" units="milliAmperes"
 38 name="internal_bus_v48_voltage" longName="internal_bus_v48_voltage" units="milliVolts"
 39 name="internal_v12_voltage" longName="internal_v12_voltage" units="milliVolts"
 40 name="internal_v5_voltage" longName="internal_v5_voltage" units="milliVolts"
 41 name="internal_v-12_voltage" longName="internal_v-12_voltage" units="milliVolts"
 42 name="ilc_temp" longName="ilc_temp" units="deg C"
 43 name="idc_temp" longName="idc_temp" units="deg C"
 44 name="humidity" longName="humidity" units="percent"
 45 name="oe_e75_temp" longName="oe_e75_temp" units="deg C"
 46 name="oe_w75_temp" longName="oe_w75_temp" units="deg C"
 47 name="DateTime" longName="ISO-8601 DateTime of Sample" units="yyyy-MM-ddThh:mm:ssZ"

 ------------------------------------------------------

 MARS MVC SSDS DeviceID 1784
 Sample Record:
 1338846992, 11.769, 8.186, 10.638, 2012-06-04 21:56:32                        
                                         
 1 name="Timestamp" longName="Unix epoch seconds" units="seconds"
 2 name="mv_bellows_temp" longName="mv_bellows_temp" units="deg C"
 3 name="mv_endcap_temp" longName="mv_endcap_temp" units="deg C"
 4 name="mv_pressure" longName="mv_pressure" units="psia"
 5 name="DateTime" longName="ISO-8601 DateTime of Sample" units="yyyy-MM-ddThh:mm:ssZ"