MARS Status September 29, 2009
Current Experiments

1. MOBB on port 1
2. FOCE on port 2

3. Sensor Group on port 4

4. EK60 on port 6
5. EITS on port 8
Issues
ESP and Rover on WNS

Both ESP and Rover tested on WNS.  Tested limited due to failed PIX.
MOBB Cable

MOBB cable appears to have been trawled again.  MOBB functioning and GF looks the same.
WNS PIX failure

The power supply in the WNS PIX failed.  This resulted in no network connection to the outside world from the WNS.  Pete is ordering a new power supply.  Another example of why not to be moving the WNS all the time.
EITS Recovery date

Discussion of EITS remaining deployed until February 2010 time Frame.  Erika raised issue of boat day (has money for this year).

CISCO security changes
Installed on WNS but not the MARS node itself.   Need to address testing issues but otherwise seems to be working well.
WNS Relocation

Power is in.  Conduits through wall being installed today.
Ricketts Ability to Service MARS

Need to look at Ventana tools developed for MARS access.

FOCE

FOCE is still operational.  FOCE is in an “operate and see” mode.   Recover January 2010.
Interface cables/ODI connectors/adapter assembly

ODI has said they will provide ESP cable at tend of September and MARS adapters at end of October.  MARS adapters might slide out further.

MV Converter
Awaiting more information from Keith.  Power data was successfully gotten 8/14/2009.
Schedule MARS Power Down for Service
Looking to do in the October timeframe.
Habitat and Biological Impact survey
To be conducted in the January through April 2010 time frame.  Survey of the MARS cable to evaluate impact.  Jim Barry and Linda Kuhnz.  Will require multiple dive days.

Acoustic Communications Base Station for MARS

It has been discovered this is to include a float 50 meters above the base instrument.  Issue is entanglement with ROV tether.  Lee Freitag announced that the deployment date has slid from 10/28/2009 until sometime in February 2010 due to ODI’s inability to deliver product.

Future deployments

Rover
10/1/2009
Recover 12/18/2009

Connect to port 3
Acoustic Communications Base Station for MARS
Maybe February 2010
6 month deployment
Lee Freitag @WHOI
BPR/Tilt instrument for MARS
Deploy 7/6/2010
Recover 12/4/2010
Bill Chadwick @NOAA

Scott Stalin @NOAA/PMEL

ESP
9/30/2009 thru 10/26/2009
11/25/2009 til early 2010

Chris Scholin
OBS Seismometer

Possibly January time frame
6 month deployment
John Orcutt

Large Aperture Array

2011
NPS

Chinese MARS Node

Dejun Li @Zhejiang University, China

Application is in to NSF.  Plan to be on MARS for 3 months.
No further communications

In-situ calibrator for ph measurement
Kang @Dept of Geology and Geophysics, Univ of Minnesota
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