MARS Status February 02, 2010
Current Experiments - 3
· MOBB on port 1
· EK60 on port 6
· EITS on port 8
Issues
ACOMMS Deployment

Today’s deployment was aborted due to ROV problems.  Deployment rescheduled for tomorrow.
MARS Port 4 Connector Pin 12 Failure

Status of port 4 is unusable.  Port 4 needs to be tested on a future dive.
ODI Penetrator Failure

It was discovered that oil leaked from the ODI oil filled cable into the CTD SIM can.  Cable and a sample of the oil from the SIIM can have been received at ODI.  Swab from face of MINO connector sent to ODI today.
MOBB Move to Port 5

Current plan is to move MOBB to port 5.  Last week was weathered out, maybe March 8th or 9th.
Ricketts Ability to Service MARS

Need to look at Ventana tools developed for MARS access.  
EOI Power
PG&E notified MBARI of planned service interruption:

2/18/2010 from 8:30 am to 9:00 am

2/18/2010 from 2:00 pm to 2:30 pm

The UPS at the end of the island should be able to hold up for the duration of the outages.
Lessons Learned

MARS missed getting all the needed information from WHOI to get all requested network setup completed.  Pete still managed to get it down before the Lobos made it to the MARS site.  However, to try and reduce the possibility of future occurrences, will be adding to the meeting agenda, a review of all deployments/recoveries that will occur in the 4 weeks following the meeting.

MARS Lab UPS
The MARS lab UPS is marginally powered.  Recommend replacement with a 3000 va unit.  Cost approximately $1200.

Future deployments/recoveries
MARS Cable Survey

Started 1/8/2010
ACOMMS
Deploy 2/2/2010 2/3/2010
Recover 8/23/2010
Will attach to port 3
Lee Freitag @WHOI
FOCE

Deploy 3/22/2010 
Recover mid-June (tentative 6/19/2010) August ?
Will attach to port 2

LOOKING (was OBS Seismometer)

Deploy 3/26/2010
Recover 9/30/2010
Will attach to port 1
John Orcutt @UCSD

EITS

Recover 3/24/2010

BPR/Tilt instrument for MARS
Deploy 6/30/2010
Recover 12/14/2010
Will attach to port 7

Bill Chadwick @NOAA

Scott Stalin @NOAA/PMEL

ESP

Deploy 11/30/2010

Recover – Not known yet

Will attach to port ?

Large Aperture Array

2011
NPS

Chinese MARS Node

Dejun Li @Zhejiang University, China

Application is in to NSF.  Plan to be on MARS for 3 months.
Bottom map (Future)
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