MARS Status January 5, 2010 – Updated 1/7/2010
Current Experiments - 3
· MOBB on port 1
· EK60 on port 6
· EITS on port 8
Issues
MARS High Voltage Status
The high voltage is still stable, showing no signs of the earlier problem.  However, no corrective action has yet been taken.  The voltage is being watched closely.  The corrective action planned is to utilize the DB25 on the Voltronics as opposed to the Phoenix connector that is currently being used.  To do this requires a retrofit of the existing spare power supply.  The spare power, while functional, has a broken local/remote control switch.  The plan is to return the spare power supply to Voltronics and have them do the work.  The logistics are still being worked out both to ensure a backup supply is available as well as ensuring a power supply is available to support the V4 MVC testing in late March.
MARS Port 4 Connector Pin 12 Failure

Pin 12 (48 volts) has failed.  Testing showed the pin connected to seawater.  Visually, the connector appreared to have failed to seal when the CTD connector was removed.  375 volts, 1pps and the network all tested good.
Ricketts Ability to Service MARS

Need to look at Ventana tools developed for MARS access.  
EK60

EK60 date still not decided.  
Interface cables/ODI connectors/adapter assembly

The two 10 meter oil filled ODI cable assemblies have arrived.  No testing has been done yet.
CISCO security changes

Installed on WNS but not the MARS node itself.   Based upon testing done on the WNS with the Acternas, testing on the node with the Acternas has been modified.  The shore side Acterna is now attached to the corresponding shore side science vlan.
Future deployments/recoveries
MARS Cable Survey

Starts 1/7/2010 1/8/2010
Acoustic Communications Base Station for MARS
Deploy 2/2/2010
Recover 8/23/2010
Will attach to port 4 unknown.  Need 48 volts.
Lee Freitag @WHOI
FOCE

Deploy 3/9/2010 3/11/2010
Recover mid-June (tentative 6/19/2010)
LOOKING (was OBS Seismometer)

Deploy 3/9/2010. 3/11/2010 3/9/2010
Recover 9/30/2010
Will attach to port 3
John Orcutt @UCSD

EITS

Recover 3/24/2010

BPR/Tilt instrument for MARS
Deploy 6/30/2010
Recover 12/14/2010
Will attach to port 7

Bill Chadwick @NOAA

Scott Stalin @NOAA/PMEL

Large Aperture Array

2011
NPS

Chinese MARS Node

Dejun Li @Zhejiang University, China

Application is in to NSF.  Plan to be on MARS for 3 months.
MARS layout
MARS





EITS





EK60





ACBS





FOCE





Looking





To MOBB





North





BPR/Tilt








