MARS Status January 26, 2010 - Updated
Current Experiments - 3
· MOBB on port 1
· EK60 on port 6
· EITS on port 8
Issues
MARS Port 4 Connector Pin 12 Failure

Status of port 4 is unusable.  Call with ODI this morning.  ODI said the port might be usable.  Port 4 will be tested Tuesday.
ODI Penetrator Failure

It was discovered that oil leaked from the ODI oil filled cable into the CTD SIM can.  Cable and a sample of the oil from the SIIM can have been received at ODI.  Swab from face of MINO connector sent to ODI today.
MOBB Move to Port 5

Current plan is to move MOBB to port 5.  Last week was weathered out, maybe March 8th or 9th.
Ricketts Ability to Service MARS

Need to look at Ventana tools developed for MARS access.  
MARS High Voltage Status

The high voltage is still stable, showing no signs of the earlier problem.  However, no corrective action has yet been taken.  The voltage is being watched closely.  The corrective action planned is to utilize the DB25 on the Voltronics as opposed to the Phoenix connector that is currently being used.  To do this requires a retrofit of the existing spare power supply.  The spare power, while functional, has a broken local/remote control switch.  Will return the spare power supply to Voltronics and have them do the work.  The logistics are still being worked out both to ensure a backup supply is available as well as ensuring a power supply is available to support the V4 MVC testing in late March.

Future deployments/recoveries
MARS Cable Survey

Started 1/8/2010
ACOMMS
Deploy 2/2/2010
Recover 8/23/2010
Will attach to port 3
Lee Freitag @WHOI
FOCE

Deploy 3/22/2010 
Recover mid-June (tentative 6/19/2010) August ?
Will attach to port 2
LOOKING (was OBS Seismometer)

Deploy 3/26/2010
Recover 9/30/2010
Will attach to port 1
John Orcutt @UCSD

EITS

Recover 3/24/2010

BPR/Tilt instrument for MARS
Deploy 6/30/2010
Recover 12/14/2010
Will attach to port 7

Bill Chadwick @NOAA

Scott Stalin @NOAA/PMEL

ESP

Deploy 11/30/2010

Recover – Not known yet

Will attach to port ?
Large Aperture Array

2011
NPS

Chinese MARS Node

Dejun Li @Zhejiang University, China

Application is in to NSF.  Plan to be on MARS for 3 months.
Bottom map (Future)



























To MOBB





ACOMMS 2/2





BPR/Tilt 6/30 666/30





North





Looking 3/9





FOCE 3/22





EK60





EITS off 3/24 and then MARS Camera





MARS





Port 4 unusable








