MARS Status November 15, 2011

Current Experiments – 5
· FOCE on port 2
· PHOBOS on port 4
· MOBB on port 5
· BMFC on port 6
· BPR/Tilt on port 7

Issues
FOCE
Having issues with fan chain.  May need ROV repair.
ODI Connector Failures
A second ODI connector has failed to seal all sockets when connector removed.  Previously port 4 had a single socket fail to seal.  Now port 6 has had 3 sockets fail to seal.
DCS Server failure
The DCS server hardware is repaired, nine days after it failed.  Still some software setup to go.
SES
Deployed today.  Do not know recovery plans.
PHOBUS
Deployed 11/7/2011.  Looking good so far
MARS Data Into SSDS
Actual entry of data into SSDS might take a bit longer (up to several months).  Estimate is October 2011.  (Today must be October 46th)
MARS EOI Maintenance
Several items need to be addressed at the EOI:
1. Sea water ground check
2. Power supply maintenance
3. UPS service
MARS West Gb Link is Down
The link is still down but the East link is running without errors.  Debug efforts will be scheduled again soon.


Future deployments/recoveries
BMFC
Recover 7/17/2012 & 7/18/2012
Port 6
BPR/Tilt instrument for MARS
Recover 11/28/2012
Port 7
Bill Chadwick @NOAA
Scott Stalin @NOAA/PMEL
FOCE
Recover August 2012
Port 2
Ghost Buster
Deploy 10/2/2012
Recover 12/19/2012
Port 8
Kang Ding – University of Minnesota
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