MARS Status October 3, 2012

Current Experiments – 4
· FOCE on port 2
· PHOBOS on port 4
· MOBB on port 5
· BMFC on port 6

Issues
FOCE
To be recovered October 8, 2012
ODI Connector Failures
MARS currently has three ports that require true dummy plugs due to failure of the seals on the connector sockets.  These are ports 4, 6 and 7.  After Monday’s recoveries, two of our three dummies will be in use.  The third will be required when BMFC is recovered.  The concern is what happens if the FOCE port connector fails to seal on Monday.
Ghost Buster
The deployment of Ghost Buster was originally scheduled for October 2, 2012 with recovery scheduled for December 19, 2012.  Obviously the deployment was not possible.  Working on setting up a deployment shortly after the RC becomes operational.
PHOBOS
To be recovered October 8, 2012



Future deployments/recoveries
BMFC
Recover Early November?
Port 6
FOCE
Recover October 8, 2012
Port 2
PHOBOS
Recover October 8, 2012
Port 4
Ghost Buster
Deploy Early November?
Recover 12/19/2012
Port 8
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