Port Test Tool
Account:
Lobos
Password:
ventanarov

Domain:
BELUGA

Once the PTT can has been turned on……

wait 1 minute.

Double click on Port Test Tool icon

Click on 1 PPS Disabled button

Button should turn green

If the pulse width field reads 10000+ usec. (every tenth pulse will be 20000+ usec) then the 1PPS on port 1 is good.

Press 1 PPS Enabled button

Turn off PTT

Disconnect PTT cable.

