MARS Lab 
Re-opening Plan

The MARS facility has remained operational during the COVID shutdown. Periodic visits to do routine maintenance on windows computers and run the generator at the end of the island (EOI) have been conducted. Remote monitoring of the system has also been conducted. 
As MARS is a limited access facility (Dawe, French, Thompson, IS, Facilities) it will be wiped down weekly or more frequently if required by MBARI by either Dawe or Thompson. Cleaning staff do not service the lab.
Access by Facilities and IS should be restricted to a notification system rather than the current unrestricted access. The access badges could be deactivated but it is not a requirement. 
Current safety notifications remain in force when High Voltage testing is being conducted:
· Notification barriers across the entry door
· Notification barriers across the HV “danger” zone, area of the lab beyond the control console and Power supply rack (rack 4 closest to the main door)
· Email to accessible users of the HV testing (dacr@mbari.org, drthom@mbari.org, dfrench@mbari.org, gregv@mbari.org, jreyes-pager@mbari.org, asisfontes@mbari.org, jgomez@mbari.org, truston@mbari.org, will@mbari.org, mneal@mbari.org )
[bookmark: _GoBack]Under this notification, no unescorted access is allowed into the MARS lab.
These same restrictions apply to the EOI anytime. Dangerous voltages are always present!


