MARS Toolsled and Node Testing

Project # 900517

Task List

Node Mock-up

· Send out old Ventana Float pack to Elkhorn Composites for reforming

· Design/build steel frame simulating real node construction dimensions

· Determine ballast requirements of node mock-up.

TRF Mock-up

· Use of actual TRF from MARIPRO is possible

· No need to be built

Node Port Testing Tool

· Identify modules to read voltages (400vdc, 48vdc)

· Identify module to read 1PPS timing signal

· Loop back Ethernet connection or connect to surface IP address

· ODI connector integration into FO can

· Connector purchased by MARS Installation Project

Latch/Stab

· Design latch/stab 

· Finalize release mechanism

· Manufacture (in house or outside service)

Toolsled Design/Manufacture

· Larry?

· Half/full height

· Deck supports 

· Fabrication

· Shipyard requirments

Purchase OTS Equipment

· Schilling Manipulator Camera

· 3 Insite Pegasus cameras

· winch

· sheaves for winch.

· ½ spectra 100 ft(max)

· lights

