MARS Users

We are trying to characterize the type and level of loading on the MARS system. Certain types of loads can cause problems with the MV Converters. 

Please respond with the following information:

Voltage requirements 48, 375, or both

Current requirements

How does the load appear to the MARS LV system, capacitive, resistive?

If you can provide a schematic of the circuit attached to the MARS 375 and/or 48 VDC feeds or the specific equipment attached directly to these feeds, that would be ideal.
If you can provide a measurement or estimate of the inrush current requirements, that would be great.
Does your system provide a soft start function?  This is particularly important for high power (>500 Watts or so) applications.
Can you provide the specs on the cable (length, ohms/km, uF/km, etc.) you are using to connect your system to MARS?

If you are not the primary developer of your equipment and do not know the above all of the above information, please respond with make and model numbers of the equipment you plan to deploy.

Thank you for your assistance.


Craig Dawe

