Teledyne Benthos SM-75 attached to MARS – Timeline
10/27/11 – Deploy, attach, power up, and verify basic acoustic comms

11/4/11 – power outage causes SM-75 to be powered off

11/9/11 – powered on again

11/15/11 – BMFC nodes deployed

11/16/11 – MARS attached SM-75 has some acoustic comms with BMFC nodes

2/?/12 – SM-75 powered down, to save money

5/8/12 10:00 AM EST – SM-75 powered on for testing

5/8/12 10:45 AM EST – SM-75 power shut off due to ground fault (reading maxed out) on the 375V return line.

5/15/12 – SM-75 powered on for a short time, ground fault continues, but operates OK
5/22/12 - SM-75 powered on for a short time, ground fault continues, but operates OK

6/1/12 - SM-75 powered on for a short time, ground fault continues, but operates OK

6/12/12 – SM-75 powered on for a short time, ground fault continues, but operates OK

7/5/12 – SM-75 powered on for a short time, ground fault continues, but operates OK

7/6/12 – SM-75 powered on for a short time, ground fault continues, but operates OK

7/10/12 – SM-75 powered on for a short time, ground fault continues, but operates OK

