M-DUC MEETING NOTES

August 30, 1999

Attendees:
Dave Caress, Duane Edgington, Gernot Friederich, Kim Reisenbichler, Rich Schramm

1. Core Data Streams

Dave has now received responses on the data streams from Chavez, Vrijenhoek, Johnson, and Robison.  

Question:  Chavez asked if the core data streams only applied to MBARI funded cruises.  If data were collected during a cruise on an external ship, how would the data be entered into the database?  This would require extra resources.  This request will need to be added to the data management plan.  

Question:  Reisenbichler asked about data collected during outside researcher's cruises (NURP).  Who owns the data?  We might suggest charging for the service of collecting.  Possible solution is that we require that MBARI share ownership of the core data only.  Policy may need to be written to address this issue.  Caress to check with Marcia on the number of days set aside for outside researchers.  

Question:  Johnson felt that the data collected from the fluorometer need not be included in the CTD core data stream.  After some discussion it was felt trying to remove this data would be more trouble than it was worth.

2. Data Management Plans

Now that Gernot has returned from Eel River, he plans to start work on the shipboard CTD data management plan.  There has been some delay in the navigation data management plan due the fact the Drew has been busy with the AOSN project.  Rich met with Debbie Meyer and Drew Gashler to begin the data management plan for the ROV/CTD data stream.

3. VIMS Meeting

A open forum design review was held so researchers could provide their input on their video needs.  The VIMS project will be reduced to include only those features that were deemed important (framegrabbing and event marking).  The researches did not feel that the electronic notebook was a critical requirement.  The VIMS team will take back all the information they received and put together a VIMS requirement specification.  Video comparison have not yet been done for Charlie Paull and Jim Barry.

4. pH Sensor Addition

Mike McCann can remove the transmissometer data column and null the data.  There is no time in the schedule to allow anything else to be done at this time.

5. HDTV Information Update - Schramm

The HDTV deck doesn't operate properly in the vertical time code.  Only longitude time code is being recorded, but it is not accurate.  It is off on the order of hours.  Chaffey will have a design review after the camera has been installed to provide everyone with the changes. 

The iris values are also not correct.  It does not affect the field width values.  We probably no longer need this data. Reisenbichler indicated that having ballpark figures on the iris opening is important.

There is no way of knowing if the HDTV is recording.  Data Manager only returns the last value written.

