Ken Johnson showed processed mooring data from the MBARI web site which exhibit problems: some bad data are not flagged, some good data are flagged. Leslie and Fred think the data as served does not accurately reflect their processing.

Need to figure out what’s going on. Mike McCann shows that the underlying file has flags correct.

Leslie – issue of thin layers interesting – how do measure thin layers using a sensor that is affected by surface waves.

Francisco – noise at 10 or 20 m depths due to placement within a strong gradient while moving up and down. Leslie says there shouldn’t be spikes in this case.

Leslie: another issue –fouling on surface instruments causes drift in salinity

Ken would like new instrument – replace 200 meter microcat with model 16 with flourometer.

