MBARI LICENSES and Freqs
REV: 9/3/2010

MBARI FRN
0001635101

Password “ventana”
KYZ772 
HF/VHF  Private Coast
Grant Date

08/07/2003

Expiration Date
08/5/2013

156.8000.1 (ch-16)

156.4500 
(ch-9)

4.1460 
(SSB)

WNWN547 
UHF

Grant Date

08/06/2003

Expiration Date
03/26/2013

466.4000

Red
461.4000

Orange
466.7625


461.7625

466.7875

Blue
461.7875

Green
WPXE722
UHF/VHF
Grant Date

03/18/03

Expiration Date
03/18/2013

464.2250

SeaTel pointing (where are ships)
469.2250

159.7200

KD36035

Grant Date

3/07/03

Expiration Date
11/03/2013

2475.5000

WNEX706 (Mt Toro)

Grant Date

08/12/2009

Expiration Date
08/25/2019

6462.5000

25M0D7W
TX to PL

6437.5000

25M0F9W
TX to WF

WPSL379 (LOBOS)

Grant Date

06/08/2001

Expiration Date
06/08/2011

6487.5000

25M0F8W


6512.5000

25M0D7W
TX to Toro

WQHA545 (FLYER)

Grant Date

06/11/2007

Expiration Date
06/11/2017

6487.5000

25M0F8W
TX to Toro

6512.5000

25M0F8W

WNTG789 (Mt TORO)

Grant Date

4/13/2002

Expiration Date
04/11/2012

19315.0
30M0G7W (tx to MBA)



20M0F8W

19440.0
40M0G7W (tx to Moss)

19350.0
20M0F8W (tx to Moss, unused)
WNTP517 (MBARI)

Grant Date

4/13/2002

Expiration Date
04/16/2012

17880.0
40M0G7W

17790.0
20M0F8W

WQKW254 (MBA)

Grant Date

10/2/2009

Expiration Date
10/2/2019

17755.0
30M0G7W

WNTA293 (MBARI)

Grant Date

12/10/2008

Expiration Date
02/15/2019

23025.0 


23375.0 

23375.0 

Expired

WNTA294 (MBA)

WNEX706 (FLYER)
Misc Freq into

TELEX WIRELESS HEADPHONES

PT LOBOS:

BASE RX: 206.000 MHz

                 207.425 MHZ

BASE TX:  177.800 MHz

WESTERN FLYER:

BASE RX:  212.000 MHz

                  212.800 MHz

                  213.425 MHz     

                  213.800 MHz

BASE TX:  183.730 MHz


WF FREQUENCIES 
  
1  
467.7500        
BOAT OPS


2  
467.7750        
BOAT OPS


3  
467.8000        
BOAT OPS


4  
467.8250        
BOAT OPS

The above frequencies are used on board ships for communications during dockings, maintenance and departures
Retired
TORO TX/MBA RX - 19.270 GHz Retired
TORO RX/MBA TX - 17.710 GHz  Retired      
TORO TX/ MBA RX - 18.970 GHz Retired

TORO TX/MBARI RX - 19.430 GHz
TORO RX/MBARI TX - 17.870 GHz 






