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These settings are required for video and mooring downloads.
1. [bookmark: _GoBack]Toro HP Ethernet switch:
a. IGME snooping enable
b. Admin mode enable
c. Filter unknown multicast DISABLE 
2. Toro Netgear Ethernet switch
a. IGME snooping enable
b. Admin mode enable
c. Filter unknown multicast ENABLE 
3. Moss Landing Ethernet switch:
a. IGME snooping enable
b. Admin mode enable
c. Filter unknown multicast DISABLE 
4. Toro Event HD6500 Ethernet payload ports
a. Auto negotiation disable
b. 100mb, Full, Symmetric
5. Harris 18ghz Moss Landing Ethernet payload port
a. Install dumb switch between system and MBARI switch
b. 100m, Full
6. 


