
MT TORO 12VDC POWER SUPPLY
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POS
FUSE
                              EQUIPMENT

  1A
   4A
OASIS UHF XCVR & TNC

  2A
  ½A
PEET BROS WX STATION

  3A
   4A
DGPS XCVR & TNC

  4A
   ½A
6 GHz FILTER SWITCH

  5A
   4A
TELEDESIGN RADIO – OASIS – 466.7875 MHz

  6A



  7A



  8A



  9A



  10A



  1B
   4A
SYS A 6 GHz TX PA (ON TOWER – SEPARATE CABLE FROM CONTROL CABLE)

  2B
   7½A
SYS A 6 GHz XMTR

  3B
   7½A
SYS B 6 GHz XMTR

  4B
   4A
SYS B 6 GHz TX PA (ON TOWER – IN CONTROL CABLE)

  5B



  6B



  7B



  8B



  9B



  10B



