
CUPOLA KNOX

REV: 14SEPT2004


VIDEO 
AUDIO

IN
L
R
1 -
MBARI A - 18 GHz (PL) RCVR VIDEO OUT
RCVR AUDIO CH 2 (UHF RCVR)
RCVR AUDIO CH 1

2 -
MBARI B - 18 GHz (WF) RCVR VIDEO OUT
RCVR AUDIO CH 3
RCVR AUDIO CH 2


3 -
AUX IN (PATCH PANEL)
AUX AUDIO CH 2
AUX AUDIO CH 1

4 -
MAGNI WFM & FRAME GRABBER
N/C
N/C

5 -
N/C
N/C
N/C

6 -
N/C
N/C
N/C

7 -
PACIFIC FORUM (MIXER OUT)
N/C
FEED FROM FORUM

8 -
SAT RCVR
N/C
RCVR FEED

9 -
N/C 
N/C
N/C

10-
FIBER OPTIC FROM BLDG B-TANK CAM
N/C
N/C

11-  BEACH CAM - NORTH
N/C
N/C

12-
BEACH CAM - SOUTH 
N/C
N/C

13-
N/C
N/C
N/C

14-
QUAD SPLITTER (SWITCHED OUTPUT)
N/C
N/C

15-
N/C
N/C
N/C

16- MAGNI WFG (BARS)
+4 dBm TONE
+4 dBm TONE


VIDEO
AUDIO

OUT
L
R
1 -
MBARI A – 18 GHz (PL) XMTR VIDEO IN
XMTR AUDIO CH 2
XMTR AUDIO CH 1

2 -
MBARI B – 18 GHz (PL) XMTR VIDEO IN
XMTR AUDIO CH 3
XMTR AUDIO CH 2

3 -
AUX OUT (PATCH PANEL)
AUX AUDIO CH 2
AUX AUDIO CH 1

4 -
CH 71 MULTI-CHAN MODULATOR
N/C
N/C

5 -
CH 73 MULTI-CHAN MODULATOR
N/C
N/C

6 -
CH 75 MULTI-CHAN MODULATOR
N/C
N/C


7 -
PACIFIC FORUM (AV1)
N/C
FEED TO FORUM



8 -
CH 8 MODULATOR 
N/C
CH 8 MODULATOR

9 -
CH 9 MODULATOR
N/C
CH 9 MODULATOR

10-
CH 10 MODULATOR
N/C
N/C

11-
CH 14 MODULATOR 
N/C
N/C
12-
CH 12 MODULATOR
N/C
CH 12 MODULATOR


13-
FIBER OPTIC XMTR TO BLDG B-SYS A
XMTR CH 2  (UHF RCVR)
XMTR CH1


14-
FIBER OPTIC XMTR TO BLDG B-SYS B
N/C
XMTR CH1

15-
FIBER OPTIC XMTR TO BLDG B-N/C
CH 15 MODULATOR
N/C

16-
FRAME GRABBER & MAGNI WFM IN
N/C
N/C

STORED AS PATTERN 01 (DEFAULT), SEE REVERSE SIDE
TO RECALL PATTERN 01: PRESS “R”, “0”, “1”, “EN”
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*UHF RCVR AUDIO


AUDIO MIXER


CH
CONNECTION
LEVEL



1 IN
FORUM (A/V 2)
~6.2



2 IN
CUPOLA MIC
5


3 IN
N/C
N/A


4 IN
N/C
N/A


OUT
KNOX 7R-IN (FORUM)
5

