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VIDEO 
AUDIO

IN
L
R
1 -
MBARI C - 18 GHz (MBA) RCVR VIDEO OUT
RCVR AUDIO CH 2
RCVR AUDIO CH 1 

2 -
N/C
N/C
N/C


3 -
N/C
N/C
N/C

4 – V3 (FROM AUD?)
AUDIO CH 2
AUDIO CH 1

5 -
V4 (FROM?)
AUDIO CH 2
AUDIO CH 1

6 -
N/C
N/C
N/C

7 -
N/C
N/C
N/C

8 - MAGNI WFG (BARS)
+4 dBm TONE
+4 dBm TONE


VIDEO
AUDIO

OUT
L
R
1 -
MBARI C - 18 GHz (MBA) XMTR VIDEO IN
XMTR AUDIO CH 2
XMTR AUDIO CH 1 

2 - N/C
N/C
N/C

3 -
N/C
N/C
N/C

4 – SIGMA VDA #1 IN (TOO?)
N/C
N/C 

5 - SIGMA VDA #2 IN (TOO?)
N/C
N/C

6 -
N/C
N/C
N/C


7 -
GIL’S OFFICE ?
?
?



8 -
VIDEO MONITOR
N/C
VIDEO MONITOR

STORED AS PATTERN 1 (DEFAULT), SEE REVERSE SIDE
TO RECALL PATTERN 1: PRESS “R”, “1”, “EN”
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